Partially translated to english by niksy... sorry guys, couldnt understand the rest :(


Use any HEX editor for Color_T.cfg setup

             0  1  2   3  4  5   6... F
0x00000000  XX XX XX               组合推出键
0x00000010  XX XX                  时钟的行坐标 时钟的纵坐标
0x00000020  XX XX XX               first number collor
0x00000030  XX XX XX               second number collor
0x00000040  XX XX XX               dots collor
0x00000050  XX XX XX               thirth number collor
0x00000060  XX XX XX               fourth number collor (all collors are in HEX code, you can use some software like photoshop for getting HEX color codes)
0x00000070  XX XX XX XX XX  XX  XX 这行第1个字节为字体种类，第2个字节为边框或阴影
(the 7th byte is for the marquee effect (horisontal collor switchin/scrolling - 00 = off ; 01 = on) Bytes 1-6 here are for text look/effects, I dont know :S

and look at the picture!
http://forum.motofan.ru/index.php?act=Attach&type=post&id=180163

0 1 2 3 4 5 ... F
0x00000000 XX XX XX bond packages
0x00000010 XX XX clock line coordinates of the clock ordinate (This!)
0x00000020 XX XX XX hours of high color
0x00000030 XX XX XX hours of low color
0x00000040 XX XX XX isolation: the color
0x00000050 XX XX XX high-minute color
0x00000060 XX XX XX low-minute color
0x00000070 XX XX XX XX XX XX this line of the first byte as a font type, 2 bytes for the border or shadow (0 without any results,Plus 1 frame, plus 2 after the shadow of the shadow of the former plus 3); the first 3-5 bytes for the effect of color ,No. 6 bytes for the digital space
PS: XX on behalf of a byte

thanks campanula

Thank you so much...and perfect timing too because im almost done with this elf folder! you are a life saver! 1.6 has more options and adds more offsets for more colors! here it is in english:

The original author: Kalvinxp (bimonthly)
Modified: JustinLee (sea Yim)
Source: www.motoedy.cn


Configuration file (Color_T.cfg) description (each line below)
0 1 2 3 4 5 6 ... F
0x00000000 XX XX XX combination eject button (the default setting for the * + # + red button)
0x00000010 XX XX clock position, the horizontal axis and vertical axis
0x00000020 XX XX XX peak hours, the color of RGB
0x00000030 XX XX XX low hours of color
0x00000040 XX XX XX isolation number: color
0x00000050 XX XX XX High-minute color
0x00000060 XX XX XX Low-minute color
0x00000070 XX XX XX isolation number: color
0x00000080 XX XX XX seconds, the color of a high
0x00000090 XX XX XX seconds, the color of low -
0x000000A0 XX XX XX XX XX XX XX XX XX XX XX XX XX XX XX XX
The last line of the first one byte of the font type (ID), an optional different ID to change the font size, the available options are 01 ~ 08,0 A and 0C ~ 0E. ;
The first two bytes of the border, or shadow (0 without any effect, a frame, after two plus the shadow of the shadow of three to Canada);
Clauses 3 to 5 bytes for the effects of color;
No. 6 bytes for the fill color (0 without fill color, a fill all the numbers add color, two color only seconds, plus fill);
Articles 7 to 9 bytes for the fill color of the color;
The first 10 bytes for the outer border (0 without external border, an all digital plus external borders, only two seconds, plus external borders);
The first 11 bytes of digital pitch;
The first 12 bytes for the Marquee effect (1 open, 0 off);
Paragraphs 13 to 16 bytes for the fill color and digital edge of the pitch, corresponding to the left, right, up, down, the configuration file the default is set to 1.

PS: XX represents a byte, without fill color, the second part of the figure will always be overlap displays. 