Instructions
Upgrade AP Bootloader to 1.1.54 Motorola A92x

Method of chose firmware file .shx :

	Hardware Version	PCB revision	Factory Version Code		Recommended file
	-----------------------------------------------------------------------------------------------------------------
	A920 - M02		8487855M02 O	All				REL_30.80.xx_bootldr010154tsh.shx
	A920 - M03		8487855M03 O	All				REL_30.80.xx_bootldr010154tsh.shx
	
	A925 - P1		8488488N01 P1	All				REL_30.80.xx_bootldr010154sny.shx
	A925 - P2a		8488488N01 P2a	All				REL_30.80.xx_bootldr010154sny.shx
	A925 - P2b		8488488N01 P2b	All				REL_30.80.xx_bootldr010154sn2.shx
	A925 - N02		8488488N02 O	L960Q1 – L960Q4			REL_30.80.xx_bootldr010154sn2.shx
	A925 - N02		8488488N02 O	L960Q5 and beyond		REL_30.80.xx_bootldr010154sn3.shx
	-----------------------------------------------------------------------------------------------------------------
	Note 1:  PCB revision can be found under the battery, located just above the SIMCARD holder.
	Note 2:  FVC - Factory Version Code or Bar Code or read phone in force flash mode with USB cable.


Flash must be loaded to phone in PST 6.7 General or higher the same how firmware Generic 30.80.xx

WARNING !!!

Download incorrect .shx file to Your phone may completly damage the possibility to load firmware again and operation phone! 
You download the files to phone at Your own risk! I don't give guaranty to this firmware files.
