This is backup of PDS dumped from demo unit of Motorola E398
The device had firmware version R372_G_0E.20.32R and flex GSKE398T672CY04F on it.
This file not intended for repair or unlocking, but only for research purposes. 
Do not flash it in normaly working phone, unless you 100% sure what you doing.
Always remember making backup of original PDS, before interfere in PDS zone.