This is backup of PDS dumped from engineering sample of Motorola E398 (Test Board) 
The device had firmware version R372_G_0E.20.8AR and flex SE7315AXXB7086 on it.
This file not intended for repair or unlocking, but only for research purposes. 
Do not flash it in normaly working phone, unless you 100% sure what you doing.
Always remember making backup of original PDS, before interfere in PDS zone.