Wing board Rework.
1) Jumper for Mic connection from C51 to C4112. 
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Jumper number 2 from R40 to C16. 
Jumper from R40 



Place other side of jumper to C16 on Bottom side 
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R40 Jumper placement
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C16 jumper placement
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Place jumper from R40


On top side of board
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(view through Board)








