{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Version History","Language  Packs","Template"],"props":{"creator":"CKWu","last_modified_by":"wfr063"},"custom":{"_AuthorEmail":"Edgar.Guerreiro@motorola.com","_AuthorEmailDisplayName":"Guerreiro Edgar-F11399"},"defined_names":["Backlight","DefaultInputMode","MainMenuItem","PowerUpLanguage","T672NV"],"not_rendered":{"macros":1,"external_links":4,"defined_names":6},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Version History","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"flags":["formulas_cached_only"]}
["FFT Version","Version","Date         ","Requestor","Author","Affected Region","Description of Change"]
["0.1","0.1","2008/3/18",null,"Ryan Hsieh","All","Initial draft based on \"V01_ZN200_Slipper_Flex_Matrix.xls\"\n"]
[null,"0.2","2008/4/11",null,"Ryan Hsieh","All","1. Modify incorrect validation list.\n2. Add item for airplane mode enable/disable.\n3. Add Language Packs table.\n4. Remove mixed sorting feature.\n5. Re-adjust Shortcuts list priority."]
[null,"0.3","2008/4/24",null,"Ryan Hsieh","All","1. Add Main Menu selection\n2. Add USB Modem/Disk selection\n3. Add Message Threading selection\n4. Add Out-Of-Box Provision selection\n5. Add Java Flex URL selection\n6. Remove \"nothing\" & \"empty\" wording in Default column to avoid confusion\n7. Add wording - SMS auto registration( for CMCC) & DM Terminal Registration by SMS( for CMCC)"]
[null,"0.4","2008/8/29",null,"Jessica Kuo/CL Yang","All","1. Add Java Profile 1-10 setting under \"Template\" tab"]
[null,"0.5","2008/9/10",null,"Alex Chiu","All","1. Add DRM Exclusive FL selection"]
[null,"0.6","2008/9/11",null,"KevinChang","All","1.Add Disable SMSC edit selection\n2.Add Warning Prompt before browsing selection"]
[null,"0.7","2008-09-12",null,"Jessica Kuo","All","1. Add Java Game Page URL under \"Template\" tab\n2. Remove Java Flex URL selection"]
[null,"0.8","2008-09-24",null,"KevinChang","All","1. Add STK,Moto ID selection in mainmenu"]
[null,"0.9","2008-10-01",null,"KevinChang","All","1.Add FDN limit and FDN limit exception."]
[null,"1.0"]
[null,"1.1"]
[null,"1.2"]
[null,"1.3"]
[null,"1.4"]
[null,"1.5"]
[null,"1.6"]
[null,"1.7"]
[null,"1.8"]
[null,"1.9"]
[null,"2.0"]
[null,"2.1"]
[null,"2.2"]
[null,"2.3"]
[null,"2.4"]
[null,"2.5"]
[null,"2.6"]
[null,"2.7"]
[null,"2.8"]
[null,"2.9"]
[null,"3.0"]
[null,"3.1"]
[null,"3.2"]
[null,"3.3"]

{"sheet":"Language  Packs","index":1,"n_rows":38,"n_cols":5,"rows_kept":38,"flags":["formulas_cached_only"]}
["Region","Id","Name","Supported Language","Comments"]
[null,"00","Generic","ENGLISH (US)\nCHINESE (TRADITIONAL)"]
[null,"01","Taiwan","ENGLISH (US)\nCHINESE (TRADITIONAL)"]
[null,"02","PRC","ENGLISH (US)\nCHINESE (SIMPLE)"]
[null,"03","HK","ENGLISH (UK)\nCHINESE (TRADITIONAL)"]
[null,"04","Indonesia, Thailand, Philippines, Vitenam","ENGLISH (UK)\nBAHASA_INDONESIAN\nTHAI\nVIETNAMESE\nTAGALOG"]
[null,"05","Malaysia, Singapore","ENGLISH (UK)\nCHINESE (SIMPLE)\nBAHASA_MALAY"]
[null,"06","Australia, NewZealand","ENGLISH (UK)\nCHINESE (SIMPLE)\nGREEK\nITALIAN\nVIETNAMESE"]
[null,"07","India,SWA","ENGLISH (UK)\nHINDI\nHINGLISH (text input only; can not be under \"Initial Setup > Language >\"","maybe have a separate pack for Bangali, Tamil, and Telegu (prompts only)"]
[null,"07.2","India","English (UK)\nBangal\nTamil\nTelegu\nHindi\nHinglish (text input only)"]
[null,"08","MiddleEast","ENGLISH (UK)\nFRENCH\nARABIC\nFARSI\nURDU"]
[null,"09","Turkey","ENGLISH (UK)\nFRENCH\nTURKISH\nRUKSIAN\nGERMAN"]
[null,"10","Isreal","ENGLISH (UK)\nARABIC\nHEBREW\nRUKSIAN"]
[null,"11","Sahara,South.Africa","ENGLISH (UK)\nFRENCH\nPORTUGUESE\nDUTCH"]
[null,"12","Russian,Ukraine","ENGLISH (UK)\nRUKSIAN\nGERMAN\nUKRAINE"]
[null,"13","LATAM","ENGLISH (UK)\nCANADIAN_FRENCH\nBRAZILIAN_PORTUGUESE\nCOLUMBIA_SPANISH"]
[null,"14","Cambodia,Bangladesh","ENGLISH (UK)\nCHINESE (SIMPLE)\nTHAI\nVIETNAMESE"]
[null,"15","SriLanka","ENGLISH (UK)\nCHINESE (SIMPLE)\nFRENCH\nPORTUGUESE"]
[null,"16","Poland","ENGLISH (UK)\nPOLISH"]
[null,"17","RestofAfrica","ENGLISH (UK)\nFRENCH\nPORTUGUESE\nSWAHILI\nZULU\nYOROBA\nAFRIKAANS\nIBO\nSESOTHO\nHAUKA"]
[null,"18","Philippines","ENGLISH (UK)\nBAHASA_INDONESIAN\nTHAI\nVIETNAMESE"]
[]
[null,"19","EMEAL01","ENGLISH (UK)\nFRENCH\nGERMAN\nITALIAN"]
[null,"20","EMEAL02","ENGLISH (UK)\nFRENCH\nGERMAN\nDUTCH"]
[null,"21","EMEAL03","ENGLISH (UK)\nSPANISH\nPORTUGUESE\nGREEK"]
[null,"22","EMEAL04","ENGLISH (UK)\nNORWEGIAN\nDANISH\nSWEDISH"]
[null,"23","EMEAL05","ENGLISH (UK)\nSWEDISH\nFINNISH\nESTONIAN"]
[null,"24","EMEAL06","ENGLISH (UK)\nLITHUANIAN\nLATVIAN\nRUKSIAN"]
[null,"25","EMEAL07","ENGLISH (UK)\nSERBIAN\nSLOVENIAN\nCROATIAN"]
[null,"26","EMEAL08","ENGLISH (UK)\nHUNGARIAN\nPOLISH\nCZECH\nSLOVAK"]
[null,"27","EMEAL09","ENGLISH (UK)\nARABIC\nHEBREW\nRUKSIAN"]
[null,"28","EMEAL10","ENGLISH (UK)\nGREEK\nBULGARIAN\nROMANIAN\nRUKSIAN"]
[null,"29","EMEAL11","ENGLISH (UK)\nARABIC\nURDU\nFARSI\nFRENCH"]
[null,"30","EMEAL12","ENGLISH (UK)\nRUKSIAN\nUKRAINE\nGERMAN"]
[null,"31","EMEAL13","ENGLISH (UK)\nFRENCH\nPORTUGUESE\nGERMAN\nDUTCH"]
[null,"32","EMEAL14","ENGLISH (UK)\nTURKISH\nRUKSIAN\nGERMAN\nITALIAN"]
[null,"33","EMEAL15","ENGLISH (UK)\nALBANIAN\nMACEDONIAN\nRUKSIAN\nSERBIAN"]
[null,"34","EMEAL16","ENGLISH (UK)\nRUKSIAN"]

{"sheet":"Template","index":2,"n_rows":866,"n_cols":14,"rows_kept":866,"merged":[[0,0,0,11],[1,0,1,3],[1,9,1,10],[2,0,2,10],[3,1,3,10],[18,1,18,10],[19,0,19,10],[65,1,65,10],[137,1,137,10],[144,1,144,10],[152,1,152,10],[213,1,213,10],[390,1,390,10],[567,1,567,10],[594,10,599,10]],"flags":["formulas_cached_only"]}
["Duo V1.0"]
["Requester Name: Eder Rabelo\nTelephone Number: + 55 11 3847 0529\nLocation:  São Paulo\nVRF Version:  \nDate Requested: 22-Nov-2008\nProduct: EM25\nCountry: Brazil\nCustomer: Claro",{"$nulls":4},"SW Version: 0.34L\nFlex: 0.009.441-M0V00\nLanguage Pack: 0.007.413\n\nPress *#**372#send on idle screen and select \"S/W ver. & model\" to get this information",{"$nulls":3},"Validation Notices:\n- Fields to be validated: Yellow background\n- Fields not to be validated: White background\n- The validation needs to be done manually (no validation tool supported)"]
[]
[null,"Main Menu"]
[null,"Main Menu",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Phonebook",null,1,null,2,{"$nulls":3},"Assign the order for Main menu.","[Main Menu]"]
[null,"Recent Calls",null,2,null,1]
[null,"Messages",null,3,null,5]
[null,"Tools",null,4,null,3]
[null,"Games",null,5,null,7]
[null,"Browser",null,6,null,4]
[null,"Multimedia",null,7,null,8]
[null,"Invisible Net Link (Google Pointer)",null,8]
[null,"Alarm"]
[null,"Settings",null,9,null,9]
[null,"STK"]
[null,"Moto ID",{"$nulls":3},6]
[]
[null,"Settings"]
[]
[null,"Personalize",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path",null,"Result","comment"]
[null,"Homekeys - Up",null,"RingStyles",null,"Camera",null,{"$error":"#REF!"},null,"Homekey accessing in idle state. \nAvailable Values:\nPhonebook, Recent Calls, Messages, Tools, Games, WebAccess, Multimedia, Alarm Clock, Settings, Ring Styles, QICQ, Chat, Shortcuts, STK, Calendar, Calculator, FM Radio, Browser, Web Shortcuts, GoTo URL, W","[Settings]-> [Personalize]-> [Home Screen]-> [Home Keys]",null,"P"]
[null,"Homekeys - Down",null,"Phonebook",null,"Phonebook",{"$nulls":3},"as Homekeys-Up","[Settings]-> [Personalize]-> [Home Screen]-> [Home Keys]",null,"P"]
[null,"Homekeys - Left",null,"RecentCalls",null,"WebAccess",{"$nulls":3},"as Homekeys-Up","[Settings]-> [Personalize]-> [Home Screen]-> [Home Keys]",null,"P"]
[null,"Homekeys - Right",null,"Browser",null,"Messages",{"$nulls":3},"as Homekeys-Up","[Settings]-> [Personalize]-> [Home Screen]-> [Home Keys]",null,"P"]
[null,"Homekeys - Show/Hide Icons",null,"Hide Icon",null,"Show Icon",{"$nulls":3},"Show/Hide homekey icons in idle screen","[Settings]-> [Personalize]-> [Home Screen]-> [Home Keys]",null,"P"]
[null,"Home Screen Layout",null,"Left-Justified",null,"Left-Justified",{"$nulls":3},"Hide/Left-justify/Center the operator information in idle screen","[Settings]-> [Personalize]-> [Home Screen]-> [Layout]",null,"P"]
[null,"Home Screen Clock",null,"On",null,"On",{"$nulls":3},"Display clock in idle screen\n","[Settings]-> [Personalize]-> [Home Screen]-> [Clock]",null,"P"]
[null,"Color Style",null,"Alkali",null,"Alkali",{"$nulls":3},"Default color style selection","[Settings]-> [Personalize]-> [Color Style]",null,"P"]
[null,"Default Wallpapers",null,"Wallpaper1",null,"Wallpaper1",{"$nulls":3},"Allows each region to set the default wallpaper.\nValue: Wallpaper 1~5\n---\nWallpaper 1 (Cricket)","[Settings]-> [Personalize]-> [Wallpaper]->[Picture]",null,"P"]
[null,"Wallpaper Layout",null,"Fit-to-screen",null,"Fit-to-screen",{"$nulls":3},"The layout of wallpapers.\nValue: Center, Tile, or Fit-to-screen, ","[Settings]-> [Personalize]-> [Wallpaper]->[Layout]",null,"P"]
[null,"Screen Saver - Picture",null,"Off",null,"ScreenSaver1",{"$nulls":3},"Allows each region to set the default screen saver.\nValue: Off, Screen Saver 1~3","[Settings]-> [Personalize]-> [Screen Saver]->[Picture]",null,"P"]
[null,"Screen Saver - Delay",null,"1Minute",null,"Off",{"$nulls":3},"The screen saver delay time.\nValue: Off, 1 Minute, 2 Minutes","[Settings]-> [Personalize]-> [Screen Saver]->[Delay]",null,"P"]
[null,"Slide Tone",null,"Basic",null,"Basic",{"$nulls":3},"Default slide tone","[Settings]-> [Personalize]-> [Slide Tone]",null,"P"]
[null,"Lock Application - Phonebook",null,"Off",null,"Off",{"$nulls":3},"Lock Application:\nWhen enabled, the phone will ask for \"Phone code\" (the password) before accessing the specific application.","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - Recent Calls",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - Messages",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - Tools",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application -  -Calculator",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application -  -Calendar",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application -  -Shortcuts",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Chat",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -SIM Toolkit",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application -WebAccess",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Browser",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Web Sessions",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application -Multimedia",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Camera",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Pictures",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -FM Radio",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Voice Notes",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application -Alarm Clock",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application -Settings",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Ring Styles",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Lock Application - -Network",null,"Off",null,"Off",{"$nulls":3},"Same as \"Lock Application - Phonebook\"","[Settings]-> [Security]-> [Lock Application]",null,"P"]
[null,"Quick Dial",null,"Default",null,"Customer Requirement",{"$nulls":3},"Comments","Validation Path"]
[null,"Quick Dial  1 Number",null,"Voice Mailbox",null,"Cannot be modified",null,{"$error":"#REF!"},null,"In [Idle] state, longpress keys 1~9 to dial preset phonebook numbers.\nDefault Key1: Voice Mailbox number (cannot be modified)","No Validation Path in Settings.\n[Idle]->Longpress Key1",null,"P"]
[null,"Quick Dial  2 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key2","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[null,"Quick Dial  3 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key3","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[null,"Quick Dial  4 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key4","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[null,"Quick Dial  5 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key5","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[null,"Quick Dial  6 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key6","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[null,"Quick Dial  7 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key7","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[null,"Quick Dial  8 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key8","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[null,"Quick Dial  9 Number",null,"No number preset",{"$nulls":3},{"$error":"#REF!"},null,"Customized p.book number for Key9","[Settings]-> [Personalize]-> [Quick Dial]",null,"P"]
[]
[null,"USB",null,"Default",null,"Customer Requirement",{"$nulls":3},"Comments","Validation Path"]
[null,"USB",null,"USB Modem",null,"USB Disk",{"$nulls":3},"USB device type","[Settings]->[USB]"]
[]
[null,"Ringing Styles",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Default Ring Style",null,"Loud",null,"Loud",{"$nulls":3},"Select Active Ring-Style.\nValue: \"Loud\", \"Soft\", \"Vibrate\", \"Vibe & Ring\", \"Silent\"","[Settings]-> [Ring Styles]-> [Style]",null,"P"]
[null,"Ring Style Detail - Loud",{"$nulls":8},"[Settings]-> [Ring Styles]-> [Style]-> [Loud]"]
[null,"Ring Volume",null,"Volume5",null,"Volume5",{"$nulls":3},"Default volume of ring-tone","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Ringing Volume]",null,"P"]
[null,"Ring Tone",null,"Hello Moto",null,"Tone 1",null,{"$error":"#REF!"},null,"Default ring-tone\n---\nTone 1 (HelloMoto)","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Ringing Tone]",null,"P"]
[null,"Ring Type",null,"Continuous Ring",null,"Continuous Ring",{"$nulls":3},"Repeating Style of ringtones:\nValue: Off, Continous, Ring Once, Ascending","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Incoming Call Alert]",null,"P"]
[null,"Messages Alert Tone",null,"Tone5",null,"Tone5",{"$nulls":3},"Default alert tone for Messages\nValue: Off, Tone1 ~ Tone5","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Message Alert Tone]",null,"P"]
[null,"Key Tone Volume",null,"Level 5",null,"Level5",null,{"$error":"#REF!"},null,"Volume of the keypad tone. \nValue: Level-1 ~ Level-5.","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Key Tone Volume]",null,"P"]
[null,"Key Tone Type",null,"Key Tone1",null,"Key Tone1",{"$nulls":3},"Keypad Tone selection.\nValue: Off, Tone1 to Tone5.","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Key Tone Type]",null,"P"]
[null,"Reminders",null,"On",null,"On",{"$nulls":3},"Notification tones. For example: Charger tone (plug-in/out), heaset tone (plug-in/out), Battery Low alert, …etc.","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Remiders]",null,"P"]
[null,"Startup Music",null,"On",null,"On",{"$nulls":3},"Enable/disable Startup Music","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Startup Music]",null,"P"]
[null,"Poweroff Music",null,"Off",null,"Off",{"$nulls":3},"Enable/disable Poweroff Music","[Settings]-> [Ring Styles]-> [Loud Detail]-> [Power Off Music]",null,"P"]
[null,"Ring Style Detail - Soft",{"$nulls":8},"[Settings]-> [Ring Styles]-> [Style]-> [Soft]"]
[null,"Ring Volume",null,"Volume3",null,"Volume3",{"$nulls":3},"same as \"Ring Style - Loud\"","[Settings]-> [Ring Styles]-> [Soft Detail]-> [Ringing Volume]",null,"P"]
[null,"Ring Tone",null,"Hello Moto",null,"Tone 1",null,{"$error":"#REF!"},null,"Tone 1 (HelloMoto)","[Settings]-> [Ring Styles]-> [Soft Detail]-> [Ringing Tone]",null,"P"]
[null,"Ring Type",null,"Ring Once",null,"Continuous Ring",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Soft Detail]-> [Incoming Call Alert]",null,"P"]
[null,"Messages Alert Tone",null,"Tone 1",null,"Tone1",null,{"$error":"#REF!"},null,null,"[Settings]-> [Ring Styles]-> [Soft Detail]-> [Message Alert Tone]",null,"P"]
[null,"Key Tone Volume",null,"Level5",null,"Level3",null,{"$error":"#REF!"},null,null,"[Settings]-> [Ring Styles]-> [Soft Detail]-> [Key Tone Volume]",null,"P"]
[null,"Key Tone Type",null,"Key Tone1",null,"Key Tone1",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Soft Detail]-> [Key Tone Type]",null,"P"]
[null,"Reminders",null,"On",null,"On",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Soft Detail]-> [Remiders]",null,"P"]
[null,"Startup Music",null,"Off",null,"On",null,{"$error":"#REF!"},null,null,"[Settings]-> [Ring Styles]-> [Soft Detail]-> [Startup Music]",null,"P"]
[null,"Poweroff Music",null,"Off",null,"Off",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Soft Detail]-> [Power Off Music]",null,"P"]
[null,"Ring Style Detail - Vibrate",{"$nulls":8},"[Settings]-> [Ring Styles]-> [Style]-> [Vibrate]"]
[null,"No settings for Vibrate mode",null,"No settings for Vibrate mode",null,"No settings for Vibrate mode",{"$nulls":3},"No settings for Vibrate mode",null,null,"P"]
[null,"Ring Style Detail - Vibe & Ring",{"$nulls":8},"[Settings]-> [Ring Styles]-> [Style]-> [Vibe & Ring]"]
[null,"Ring Volume",null,"Volume5",null,"Volume5",{"$nulls":3},"same as \"Ring Style - Loud\"","[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Ringing Volume]",null,"P"]
[null,"Ring Tone",null,"Hello Moto",null,"Tone 1",null,{"$error":"#REF!"},null,null,"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Ringing Tone]",null,"P"]
[null,"Ring Type",null,"Continuous Ring",null,"Continuous Ring",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Incoming Call Alert]",null,"P"]
[null,"Messages Alert Tone",null,"Tone5",null,"Tone5",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Message Alert Tone]",null,"P"]
[null,"Key Tone Volume",null,"Level 5",null,"Level5",null,{"$error":"#REF!"},null,null,"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Key Tone Volume]",null,"P"]
[null,"Key Tone Type",null,"Key Tone1",null,"Key Tone1",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Key Tone Type]",null,"P"]
[null,"Reminders",null,"On",null,"On",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Remiders]",null,"P"]
[null,"Startup Music",null,"On",null,"On",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Startup Music]",null,"P"]
[null,"Poweroff Music",null,"Off",null,"Off",{"$nulls":4},"[Settings]-> [Ring Styles]-> [Vibe & Ring Detail]-> [Power Off Music]",null,"P"]
[null,"Ring Style Detail - Silent",{"$nulls":8},"[Settings]-> [Ring Styles]-> [Style] -> [Silent]"]
[null,"No settings for Silent mode",null,"No settings for Silent mode",null,"No settings for Silent mode",{"$nulls":3},"No settings for Silent mode",null,null,"P"]
[]
[null,"Initial Settings",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Time format",null,"24 hrs",null,"24 hrs",{"$nulls":3},"Time Format\nValue: 24hrs, am-pm format","[Settings]-> [Initial Setup]-> [Time and Date]-> [24-hour Time]",null,"P"]
[null,"Date format",null,"yyyy/mm/dd",null,"dd/mm/yyyy",null,{"$error":"#REF!"},null,"Year-Month-Day format.\nvalue: yyyy/mm/dd, mm/dd/yyyy, dd/mm/yyyy.","[Settings]-> [Initial Setup]-> [Time and Date]-> [Date Format]",null,"P"]
[null,"Auto Adjust Time",null,"Off",null,"Off",{"$nulls":3},"Automatically adjust the date/time from operator when handset power-on. (NITZ)\n*Availability of this service depends on the operator.","[Settings]-> [Initial Setup]-> [Time and Date]-> [Auto Adjustment]",null,"P"]
[null,"Time Zone",null,"Taipei",null,"Rio De Janeiro",{"$nulls":3},"Select default \"timezone\" (by \"city\") from following list.\nValues:\nVancouver, LosAngel, Mexico, Chicago, Havana, Toronto, NewYork, Buenos Aries, Rio de Janeiro, Madrid, London, Paris,\nAmsterdam, Berlin, Rome, Helsinki, Moscow, Johannesburg, Cairo, NewDelh","[Settings]-> [Initial Setup]-> [Time and Date]-> [Time Zone]",null,"P"]
[null,"Slide Closed",null,"ContinueTask",null,"EndTask",{"$nulls":3},"Application shall continue or end when slide is closed.\nValues: Continue Task, End Task","[Settings]-> [Initial Setup]-> [Slide Closed]",null,"P"]
[null,"Language",null,"English",null,"Portuguese",{"$nulls":3},"Default language.\nValue: Automatic + available languages for region (See Language Packs)","[Settings]-> [Initial Setup]-> [Language]",null,"P"]
[null,"Automatic language -- Source",null,"From SIM language",null,"From SIM language",{"$nulls":3},"When the default language is set as \"Automatic\", refer to the appropriate source.","Not viewable from UI."]
[null,"Automatic language -- Default language",null,"English",null,"Portuguese",{"$nulls":3},"When the defulat language is set as \"Automatic\" and there is no language information got from SIM, take this language as default language.\nValue:  Available languages for region ((See Language Packs)","Not viewable from UI."]
[null,"Brightness",null,"Level3",null,"Level3",{"$nulls":3},"Default brightness level for LCD","[Settings]-> [Initial Setup]-> [Brightness]",null,"P"]
[null,"Connection Indication - Vibration",null,"Off",null,"Off",{"$nulls":3},"When a MO call is connected, playing vibrator indication.","[Settings]-> [Initial Setup]-> [Connection Indication]-> [Vibration]",null,"P"]
[null,"Connection Indication - Beep",null,"Off",null,"Off",{"$nulls":3},"When a MO call is connected, playing Beep indication.","[Settings]-> [Initial Setup]-> [Connection Indication]-> [Beep]",null,"P"]
[null,"Headset & Car Setting- Auto Answer",null,"Off",null,"Off",{"$nulls":3},"Auto answer timer when headset/Car kit is plugged in.","[Settings]-> [Headset & CarSetting]-> [Auto Answer]",null,"P"]
[null,"Keypad Lock",null,"4Seconds",null,"8Seconds",null,{"$error":"#REF!"},null,"Keypad lock settings, possible value: Off, 2 Seconds, 4 Seconds, 8 Seconds","[Settings]-> [Security]-> [Keypad Lock]->[Timer]",null,"P"]
[]
[null,"Call-Related Features",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Flexed Emergency Number",null,"911, 112",null,"190, 911, 112",null,{"$error":"#REF!"},null,"Maximum upto 15 emergency numbers can be defined.\n112 is necessay for dual-band 900/1800 system. 911 and 112 are necessary to tri-band system. \n","[Idle]-> dial emergency #'s.",null,"P"]
[null,"Show/Hide [Active Line]",null,"Show Item",null,"Hide Item",{"$nulls":3},"Show/Hide the menu item. This item only can be hidden when ALS isn't supported by SIM.","[Settings]-> [Phone Status]-> [Active Line] ",null,"P"]
[null,"Phone lines",null,"Line 1",null,"Line 1",{"$nulls":3},"Alternative Line Selection.\nvalue: Line 1, Line 2.\nWhen ALS isn't supported by SIM. Line 2 will be hidden automatically.","[Settings]-> [Phone Status]-> [Active Line]",null,"P"]
[null,"Show/Hide Alternative Line Selection Icon",null,"Show Icon",null,"Hide Icon",{"$nulls":3},"Show/Hide ALS Icon on the Idle screen.","ALS Icon is displayed on the top of the Idle screen.",null,"P"]
[null,"Anykey Answer",null,"Off",null,"Off",{"$nulls":3},"Use anykey to answer an incoming call.","[Settings]-> [In-Call Setup]-> [Anykey Answer]",null,"P"]
[null,"Auto Redial",null,"Off",null,"Off",{"$nulls":3},"Automatically redial when a MO call is failed and the reason is specified as in GSM 02.07.","[Settings]-> [In-Call Setup]-> [Auto Redial]",null,"P"]
[null,"In-call Timer",null,"Call Time",null,"Off",{"$nulls":3},"Displaying timer statistic when in-call","[Settings]-> [In-Call Setup]-> [In-Call Timer]->[In-Call Count]",null,"P"]
[null,"Minute Reminder",null,"Off",null,"Off",{"$nulls":3},"Beep notification while in-call","[Settings]-> [In-Call Setup]-> [In-Call Timer]->[Minute Reminder]",null,"P"]
[]
[null,"Network Setup",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Band",null,"900/1800MHz",null,"900/1800MHz",{"$nulls":3},"Network band.","[Settings]-> [Network]-> [Network Setup]-> [Band]",null,"P"]
[null,"Search Type",null,"Automatic",null,"Automatic",{"$nulls":3},"Automatic / Manual network search mode.","[Settings]-> [Network]-> [Network Setup]-> [Type]",null,"P"]
[null,"Service Tone",null,"Off",null,"Off",{"$nulls":3},"When the phone registered to some network, play the beep tone.","[Settings]-> [Network]-> [Setvice Tone]",null,"P"]
[null,"CPHS",null,"Off",null,"On",{"$nulls":3},"Enable/disable CPHS","Not viewable from UI."]
[]
[null,"Phonebook"]
[]
[null,"Quick Dial",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Default Storing Memory",null,"SIM first",null,"SIM first",{"$nulls":3},"Preferred memory for new phonebook record:\nvalue: SIM first / Phone first","[Phonebook]->[Option]->[Setting]->[Memory]",null,"P"]
[null,"Phonebook Sorting",null,"Alphanumeric",null,"Alphanumeric",{"$nulls":3},"Sorting method of the phonebook list.\nValue: Alphanumeric, BPMF/PinYin, Stroke, Location, Thai, Greek, Russian, Hebrew, Arabic, Farsi, Urdu","[Phonebook]->[Option]->[Setting]->[Sort By]",null,"P"]
[null,"CLI Lookup Digits",null,8,null,7,{"$nulls":3},"#(digits) compared for CLI when incoming call/SMS, depends on regions.","Not viewable from UI."]
[]
[null,"Multimedia"]
[]
[null,"Camera settings",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Camera Shutter Sound",null,"On",null,"On",{"$nulls":3},"Allow user to turn on/off shutter sound in camera.","[Multimedia]-> [Camera]-> [Options]-> [Camera Setup]-> [Shutter sound]",null,"P"]
[]
[null,"Multimedia",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Sort Files",null,"By Date",null,"By Name",null,{"$error":"#REF!"},null,"Sort multimedia files by:\nDate, Size, Name","[Multimedia]-> [Pictures]-> [Option]-> [Sort Files]",null,"P"]
[]
[null,"Tools"]
[]
[null,"Alarm clock",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments","Validation Path"]
[null,"Default Alarms Tone",null,"Hello Moto",null,"Tone 32",null,{"$error":"#REF!"},null,"Default ringtone used for Alarm-Clock.\nvalue: Tone 1 to Tone 35.","[Alarm Clock]-> [New Alarm]-> [Alarm tone]",null,"P"]
[]
[null,"Shortcuts",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments","Validation Path"]
[null,"MotoID",null,1,null,2,{"$nulls":3},"Setup 9 items and assign the order for Shortcuts menu. ","[Tools]-> [Shortcuts]",null,"P"]
[null,"FM Radio",null,2,null,3,{"$nulls":6},"P"]
[null,"Music Library",null,3,null,4,{"$nulls":6},"P"]
[null,"Sounds",null,4,{"$nulls":8},"P"]
[null,"Pictures",null,5,null,6,{"$nulls":6},"P"]
[null,"Wallpaper",null,6,null,7,{"$nulls":6},"P"]
[null,"Bluetooth",null,7,null,8,{"$nulls":6},"P"]
[null,"Alarm Clock",null,8,null,9,{"$nulls":6},"P"]
[null,"GoTo URL",null,9,{"$nulls":8},"P"]
[null,"Call Time",{"$nulls":10},"P"]
[null,"Call Cost",{"$nulls":10},"P"]
[null,"New Multimedia Msg",{"$nulls":10},"P"]
[null,"Message Inbox",{"$nulls":10},"P"]
[null,"Outbox",{"$nulls":10},"P"]
[null,"Draft",{"$nulls":10},"P"]
[null,"Voicemail",{"$nulls":10},"P"]
[null,"Tools",{"$nulls":10},"P"]
[null,"Calculator",{"$nulls":3},5,{"$nulls":6},"P"]
[null,"Calendar",{"$nulls":10},"P"]
[null,"Chat",{"$nulls":10},"P"]
[null,"SIM toolkit",{"$nulls":3},1,{"$nulls":6},"P"]
[null,"Lantern",{"$nulls":10},"P"]
[null,"Game",{"$nulls":10},"P"]
[null,"Web Access",{"$nulls":10},"P"]
[null,"Browser",{"$nulls":10},"P"]
[null,"Web Shortcuts",{"$nulls":10},"P"]
[null,"GoTo URL",{"$nulls":10},"P"]
[null,"Web Sessions",{"$nulls":10},"P"]
[null,"Web Settings",{"$nulls":10},"P"]
[null,"Multimedia",{"$nulls":10},"P"]
[null,"Pictures",{"$nulls":10},"P"]
[null,"Sounds",{"$nulls":10},"P"]
[null,"FM Radio",{"$nulls":10},"P"]
[null,"Settings",{"$nulls":10},"P"]
[null,"Personalize",{"$nulls":10},"P"]
[null,"Color Style",{"$nulls":10},"P"]
[null,"Wallpaper",{"$nulls":10},"P"]
[null,"Quick Dial",{"$nulls":10},"P"]
[null,"Ring Styles",{"$nulls":10},"P"]
[null,"Call Forward",{"$nulls":10},"P"]
[null,"In-Call Setup",{"$nulls":10},"P"]
[null,"Initial Setup",{"$nulls":10},"P"]
[null,"Time and Date",{"$nulls":10},"P"]
[null,"Timezone",{"$nulls":10},"P"]
[null,"World Clock",{"$nulls":10},"P"]
[null,"Backlight",{"$nulls":10},"P"]
[null,"Language",{"$nulls":10},"P"]
[null,"Brightness",{"$nulls":10},"P"]
[null,"My Tel Number",{"$nulls":10},"P"]
[null,"Active Line",{"$nulls":10},"P"]
[null,"Battery Meter",{"$nulls":10},"P"]
[null,"Security",{"$nulls":10},"P"]
[null,"Bluetooth",{"$nulls":10},"P"]
[null,"Network",{"$nulls":10},"P"]
[]
[null,"Web Access"]
[]
[null,"User agaent profile settings",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments","Validation Path"]
[null,"UA Profile URL ",{"$nulls":7},"URL for the operator server to store User Agent Profile   ","Not viewable from UI."]
[]
[null,"Bookmark settings",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments","Validation Path"]
[null,"Bookmark 1",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",null,"click4wap",null,"Hellomoto",{"$nulls":3},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",null,"http://www.click4wap.co.uk/welcome.wml",null,"http://www.hellomoto.com.mx/wml/inv/br/claro",null,{"$error":"#REF!"},null,"Web Shortcut URL (Error response)","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 2",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",null,"Moto Download",null,"Portal Claro",{"$nulls":3},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",null,"http://wap.t720.mymobilesoft.com",null,"http://wap.claro.com.br",null,{"$error":"#REF!"},null,"Web Shortcut URL","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 3",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",null,"Nancy Download",null,"Busca Download ",{"$nulls":3},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",null,"08/wapbj/welcomepage.jsp?nanflag=1",null,"http://wap.claro.com.br/busca",null,{"$error":"#REF!"},null,"Web Shortcut URL (Error response)","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 4",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",null,"autotest",null,"Idéias Music Store",{"$nulls":3},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",null,"http://testing.opengroup.org/tswap1.1.7/",null,"http://claro.imusica..com.br/m",null,{"$error":"#REF!"},null,"Web Shortcut URL (Error response)","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 5",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",null,"google",{"$nulls":5},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",null,"http://www.google.com/wml?hl=zh-TW",{"$nulls":3},{"$error":"#REF!"},null,"Web Shortcut URL","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 6",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",{"$nulls":7},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",{"$nulls":5},{"$error":"#REF!"},null,"Web Shortcut URL","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 7",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",{"$nulls":7},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",{"$nulls":5},{"$error":"#REF!"},null,"Web Shortcut URL","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 8",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",{"$nulls":7},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",{"$nulls":5},{"$error":"#REF!"},null,"Web Shortcut URL","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"Bookmark 9",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments"]
[null,"Title",{"$nulls":7},"Web Shortcut title","[WebAccess]-> [Web Shortcuts]",null,"P"]
[null,"URL",{"$nulls":5},{"$error":"#REF!"},null,"Web Shortcut URL","[WebAccess]-> [Web Shortcuts]",null,"P"]
[]
[null,"Web Sessions",null,"Default ",null,"Customer Requirement",{"$nulls":3},"Comments","Validation Path"]
[null,"Default profile",null,"中華電信",null,"Profile 1","yes",{"$error":"#REF!"},null,"Default active WAP profile.\nvalue: profile 1 to profile 10","[WebAccess]-> [Web Sessions]",null,"P"]
[null,"Auto Switch",null,"Off",null,"Off",{"$nulls":3},"auto switch active profile by SIM if profile is in flex.\nOn: the SIM mcc:mnc will be checked, the matching WAP profile will be set as default one.\nOff: no SIM mcc:mnc will be checked.","Not viewable from UI."]
[null,"Profile 1",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"中華電信",null,"Portal Claro","OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",null,"WAP 1.2",null,"WAP 2.0",{"$nulls":3},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"10.1.1.1",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)\n",null,9201,null,9201,"9201",null,null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":3},"200.169.126.11","10.30.3.151",{"$error":"#REF!"},null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":3},8799,"9201",{"$error":"#REF!"},null,"Proxy Port Number","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"Homepage URL",null,"http://wap.emome.net",null,"http://wap.claro.com.br","http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",null,"emome",null,"wap.claro.com.br","web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":3},"claro",null,{"$error":"#REF!"},null,"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":3},"claro",null,{"$error":"#REF!"},null,"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",null,"Read & write",{"$nulls":3},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 2",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"台灣大哥大",null,"Claro Dados","OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",null,"WAP 1.2",null,"WAP 2.0",{"$nulls":3},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"10.1.1.1",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,9203,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":3},0,"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",9201]
[null,"Homepage URL",null,"http://catch",null,"http://","http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",null,"mms",null,"claro.com.br","web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",null,"wap",null,"claro",null,{"$error":"#REF!"},null,"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",null,"wap",null,"claro",null,{"$error":"#REF!"},null,"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",null,"Read & write",{"$nulls":3},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 3",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"遠傳電信易通卡",null,null,"OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"210.241.199.199",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","210.241.199.199"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",9201]
[null,"Homepage URL",null,"http://www.istyle.com.tw",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",null,"fetnet01",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 4",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"東信電訊",null,null,"OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Adress",null,"192.168.77.5",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"Homepage URL",null,"http://www.mobeelift.net",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",null,"gprs1",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",null,"gprs",{"$nulls":3},{"$error":"#REF!"},null,"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",null,"gprs",{"$nulls":3},{"$error":"#REF!"},null,"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 5",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"泛亞電信",null,null,"OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"211.78.224.100",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","nothing"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"Homepage URL",null,"http://www.hank.net.tw",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",null,"hank",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 6",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"和信電訊",null,null,"OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"210.241.199.199",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","nothing"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"Homepage URL",null,"http://mobile 1.fetnet.net",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",null,"fetnet01",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 7",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"Homepage URL",null,"http://",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 8",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"Homepage URL",null,"http://",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 9",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"Homepage URL",null,"http://",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Profile 10",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[WebAccess]-> [Web Sessions]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]->[ IP Address]",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"Homepage URL",null,"http://",null,null,"http://plus.orangehk.com",{"$error":"#REF!"},null,"Default internet WAP site.","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Homepage]",null,"P"]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[WebAccess]-> [Web Sessions]-> [Profile]",null,"P"]
[]
[null,"Messages"]
[]
[null,"General",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Message Sorting",null,"By Time",null,"By Time",{"$nulls":3},"Sorting method of Inbox messages","[Messages]-> [Option]-> [Message Setup]-> [Message Sorting]",null,"P"]
[null,"Info Service(Cell Broadcast) - Reception",null,"Off",null,"On",{"$nulls":3},"Enable/Disable the reception of Info. Service (Cell Braodcase messages)","[Messages]-> [Option]-> [Message Setup]-> [Info Srvc Setup]-> [Service]",null,"P"]
[null,"Voice Mailbox number",{"$nulls":3},"*100",{"$nulls":3},"Using the number as voice mailbox number when there is no default number set in SIM card.  ","Not viewable from UI."]
[null,"VoiceMail icon",null,"Off",null,"On",{"$nulls":3},"Clear VoiceMail icon by Network.\nOn: Don't clear VoiceMail icon until accepting network's message.\nOff: Clear VoiceMail icon automatically.","Not viewable from UI."]
[null,"Simplified unified composer",null,"Off",null,"On",{"$nulls":3},"On: unified composer on                             Off: unified composer off","[messages]->[create message]                   [messages]->[option]->[create message]    [phonebook]->[option]->[send message]     "]
[null,"Message Threading",null,"Off",null,"Off",{"$nulls":3},"Enable/disable message threading","[Message]->[Conversations]"]
[]
[null,"SMS settings",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Bearer Services",null,"GSM first",null,"GSM only",{"$nulls":3},"Bearer service used for sending MO SMS messages.","[Messages]-> [Option]-> [Message Setup]-> [Text Messages]-> [Send by]",null,"P"]
[null,"Delivery Report",null,"Off",null,"Off",{"$nulls":3},"Request the Delivery Report when sending a SMS.\nUser will be notified of successful message delivery to the terminating party","[Messages]-> [Option]-> [Message Setup]-> [Text Messages]-> [Status Report]",null,"P"]
[null,"Default SMS storage",null,"SIM first",null,"Phone first",null,{"$error":"#REF!"},null,"Preferred SMS storage:\nSIM first, Phone first","[Messages]-> [Option]-> [Memory Meter]-> [Select SMS Memory]",null,"P"]
[null,"Force 7-bit SMS encoding",null,"Off",null,"On",{"$nulls":3},"Force convert accented characters to 7-bit MO-SMS","Not viewable from the UI."]
[null,"Disable SMSC edit\n\n",null,"Off",null,"Off",{"$nulls":3},"Make the SMSC non-editable","Messages]-> [Option]-> [Message Setup]-> [Text Messages]-> [Profile]->[SIM Profile]->[Customize]"]
[null,"FDN limit",null,"Off",null,"Off",{"$nulls":3},"If this option is On, user send SMS only when SMSC in FDN list.","Not viewable from UI."]
[null,"FDN limit exception.",null,"Off",null,"Off",{"$nulls":3},"If this option is On, user only need to add  the internation code in FDN List then he could send SMS to any phone number which starting from this internation code when FDN is On.\nThis option only avaliable when \"FDN limit\" is On.","Not viewable from UI."]
[]
[null,"MMS settings",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Auto Signature",{"$nulls":7},"Automatically attach the preloaded user signature (text file) while editing a MMS message.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Auto signature]",null,"P"]
[null,"Auto fetch",null,"On",null,"On",{"$nulls":3},"Incoming messages are downloaded automatically without prompting user. \nvalues: On, Off, ask me","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Auto Fetch]",null,"P"]
[null,"Fetch while Roaming",null,"Delayed Retrieval",null,"Immediate Retrieval",{"$nulls":3},"While roaming, incoming messages are downloaded automatically without prompting user. \nvalues:  Immediate, Delayed, Ask Me","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [While Roaming]",null,"P"]
[null,"Backup Sent message",null,"On",null,"On",{"$nulls":3},"Backup a copy of sending message in outbox.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Save Sent Msgs.]",null,"P"]
[null,"Deny Read Reply",null,"Off",null,"Off",{"$nulls":3},"Reject the sending of a Read-Reply message, when the incoming MMS is read and \"read-reply\" is requested by originator.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Deny Read Reply]",null,"P"]
[null,"Request Delivery Report",null,"On",null,"Off",{"$nulls":3},"Request the Status-Report on the sending MMS.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Sending Options]-> [Status Report]",null,"P"]
[null,"Request Read-Reply",null,"Off",null,"Off",{"$nulls":3},"Request the Read-Reply on the sending MMS.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Sending Options]-> [Request Read Reply]",null,"P"]
[null,"Validity period",null,"Maximum",null,"Maximum",{"$nulls":3},"Expiration period from time of delivery that messages are kept on the MMS server before being automatically deleted. \nvalues: Maximum, 1 hour, 6 hours, 24 hours, 3 days, 1 week","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Sending Options]-> [Validity Period]",null,"P"]
[null,"Priority",null,"Medium",null,"Medium",{"$nulls":3},"Preset Message Priority(Importance):\nHigh, Medium, Low","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Sending Options]-> [Priority]",null,"P"]
[null,"Send as Anonymous",null,"Off",null,"Off",{"$nulls":3},"Hide the sender's number in MMS.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Sending Options]-> [Send as Anonymous]",null,"P"]
[null,"Allow Advertisment",null,"On",null,"On",{"$nulls":3},"Allow the receiving of Advertisment MMS","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Incoming Filters]-> [Allow Ads.]",null,"P"]
[null,"Block Anonymous Message",null,"Off",null,"Off",{"$nulls":3},"Block the receiving of Anonymous MMS","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Incoming Filters]-> [Block Anonymous]",null,"P"]
[null,"Message size limit",null,"300k",null,"300Kb",null,{"$error":"#REF!"},null,"Maximum size allowable for incoming & outgoing message.  Phone support up to 300kb","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Incoming Filters]-> [Maximum Size]",null,"P"]
[]
[null,"MMS connection settings",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Default profile",null,"Profile 1",null,"Profile 1","yes",null,null,"Active profile of the followings. Possible value: \nProfile 1 ~ 10","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]",null,"P"]
[null,"Auto Switch",null,"ON",null,"OFF",{"$nulls":3},"auto switch active profile by SIM if profile is in flex.\nOn: the SIM mcc:mnc will be checked, the matching MMS profile will be set as default one.\nOff: no SIM mcc:mnc will be checked.","Not viewable from the UI."]
[null,"MMS Server Setting 1",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"中華電信",null,"Claro Foto",null,{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://mms.emome.net:8002",null,"http://mms.claro.com.br",null,{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",null,"WAP 1.2",null,"WAP 2.0",{"$nulls":3},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"10..1.1.1",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,9201,"9201",null,null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":3},"200.169.126.10","10.30.3.151",{"$error":"#REF!"},null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":3},8799,"9201",{"$error":"#REF!"},null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",null,"emome",null,"mms.claro.com.br","web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":3},"claro",null,{"$error":"#REF!"},null,"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":3},"claro",null,{"$error":"#REF!"},null,"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",null,"Read & write",{"$nulls":3},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 2",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"台灣大哥大",{"$nulls":3},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://mms",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"10.1.1.1",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",null,"mms",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",null,"wap",{"$nulls":3},{"$error":"#REF!"},null,"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",null,"wap",{"$nulls":3},{"$error":"#REF!"},null,"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"p"]
[]
[null,"MMS Server Setting 3",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"遠傳電信易通卡",{"$nulls":3},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"Http://MMS",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P","http://mms"]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"210.241.199.199",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",null,"fetnet01",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 4",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"東信電訊",{"$nulls":3},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://mms.mobeelife.net/mms/wapenc",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"192.168.77.5",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",null,"gprs1",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",null,"gprs",{"$nulls":3},{"$error":"#REF!"},null,"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",null,"****",{"$nulls":3},{"$error":"#REF!"},null,"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 5",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"泛亞電訊",{"$nulls":3},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://mms",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"211.78.224.100",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",null,"hank",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 6",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"和信電訊",{"$nulls":3},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://mms.kgtmms.net.tw/mms/wapenc",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",null,"WAP 1.2",{"$nulls":5},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"172.28.33.5",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",null,"kgtmms",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 7",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":5},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 8",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":5},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 9",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":5},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"MMS Server Setting 10",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":5},{"$error":"#REF!"},null,"MMS profile name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"MMS Server URL",null,"http://",{"$nulls":3},{"$error":"#REF!"},null,"MMS Server Center location","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Hompage]",null,"P"]
[null,"Default WAP Stack",{"$nulls":7},"Default Active Stack:\nvalue: WAP 1.2, WAP 2.0\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]\nWAP -- WAP 1.2\nHTTP -- WAP 2.0",null,"P"]
[null,"Primary IP Address (WAP1.2)\n---\nIP Address",null,"0.0.0.0",null,null,"10.30.3.151",{"$error":"#REF!"},null,"Primary IP Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [IP Address]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Ed",null,"P","0.0.0.0"]
[null,"Primary Port Number (WAP1.2)",null,9201,null,null,"9201",{"$error":"#REF!"},null,"Primary Port Number\nvalue: 9200~9203","[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Protocol type]-> [WAP]-> [Session Mode] & [Connection Security]\nport=9200: Temporary+Off\nport=9201: Permanent+Off\nport=9202: Temporary+On\nport=9203: Permanent+On\n---\n[WebAccess]-> [Web Sessions]-> [Prof",null,"P"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","proxy.hinet.net"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number\n","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",80]
[null,"GPRS Access Point Name",{"$nulls":4},"web.orangehk.com",null,null,"GPRS Access Point Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]-> [Edit]-> [",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Messages]-> [Options]-> [Message Setup]-> [Multimedia Msgs.]-> [Connection Settings]-> [Profile]",null,"P"]
[]
[null,"Software customizations"]
[]
[null,"Chat",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"OICQ",null,"Off",null,"Off",{"$nulls":3},"Whether the OICQ (QQ) service is enabled in this FLEX.","[Tools]-> no item OICQ",null,"P"]
[]
[null,"Operator Customised Key",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"CMCC UI",null,"Off",null,"Off",{"$nulls":3},"Whether the CMCC customized UI is enabled in this FLEX","Whether CMCC UI is applied.",null,"P"]
[]
[null,"Miscellaneous Features",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Default security Code",null,1234,null,"Cannot be modified",null,{"$error":"#REF!"},null,"Security code (phone code) used to access some phone functions such as Master Reset, Lock Application","[Settings]-> [Security]-> [New Passwords]-> [Phone Lock Code]",null,"P"]
[]
[null,"Other Options",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Browser Custom Name Option",{"$nulls":3},"This itme only can be modified by CMCC.",null,{"$error":"#REF!"},null,"CMCC requirement.\nAllows you to have a customized name for WAP browser.","[\"WebAccess name\"] in main menu."]
[null,"Allow forward downloaded media object",null,"On",null,"On",{"$nulls":3},"If On, user is allowed to forward downloaded media (ring tone, picture, etc) through MMS/EMS","Not viewable from UI"]
[]
[null,"Input Setup",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Primary Input Mode",null,"iTAP English",null,"Multi Portuguese",{"$nulls":3},"possible value depends on language pack (see Language Config table):\nTAP/iTAP -English\nStroke/BPMF/PinYin -Traditional Chinese\nStroke/PinYin -Simplified Chinese\nTAP/iTAP -Bahasa Indonesia\nTAP/iTAP -Bahasa Malayu\nTAP/iTAP -Thai\nTAP/iTAP -Russian\nTAP/iTAP -","[Messages]-> [Create Message]-> [New Short Msg]-> [Options]-> [Input Setup]-> [Primary]",null,"P"]
[null,"Secondary Input Mode",null,"iTAP English",null,"iTap Portuguese",{"$nulls":3},"possible value : same as primary input mode and with additional vaule: \"Off\"","[Messages]-> [Create Message]-> [New Short Msg]-> [Options]-> [Input Setup]-> [Secondary]",null,"P"]
[]
[null,"GPRS General Settings",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Mode B",null,"Off",null,"On",{"$nulls":3},"Attach to GPRS network when needed to establish PDP context for GPRS applications WAP, WEB, MMS etc. It will detach from GPRS network after quitting from GPRS applications. \nOff : auto attach when power on. \nOn: attach when needed ","[Idle]-> check GPRS icon",null,"P","Modle 402"]
[null,"Encryption",null,"On",null,"On",{"$nulls":3},"Data is sent encrypted.","Not viewable from UI"]
[null,"GPRS Linger Timeout in Seconds",null,300,null,120,null,{"$error":"#REF!"},null,"The time the phone will try to connect to the Web before it stops. Range : 0 ~ 65535 (seconds)","Not viewable from UI"]
[]
[null,"Subsidy Lock ",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Subsidy Lock Enabled:",null,"Off",null,"On",null,{"$error":"#REF!"},null,"Turn on the Subsidy Lock.","Power on with test SIM.\nOn: Ask for password\nOff: Don’t ask for password",null,"P"]
[null,"Subsidy Lock Detail",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Subsidy Lock Type",null,"Type-0",null,"Type-8",{"$nulls":3},"Determines the type of subsidy lock configured on the device.","Subsidy Lock Detail only should be set when Subsidy Lock is Enabled. \nIts inoformation will be set in EDF file.\nPlease use MST to download the corresponding EDP file. "]
[null,"Factory Subsidy Lock Type",null,"Type-0",null,"Type-8"]
[null,"Subsidy Code numbers (if relevant)",{"$nulls":3},72405,{"$nulls":3},"Any relvant code numbers ie GID1 codes"]
[null,"Service Provider Name (if relevant)",{"$nulls":7},"Use if relevant"]
[null,"Number of Allowed Password Retries",null,3,null,5,{"$nulls":3},"Determines how many unsuccessful attempts to unlock the phone before it becomes subsidy locked. Range: 1~255"]
[null,"Length of Penalty Time (in minutes)",null,"30",null,5,{"$nulls":3},"Determines the amount of time between unsuccessful attempts for when the user can retry the code again. Range: 1~255"]
[]
[null,"Network diagnostics features\n",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Enhanced Field Engineering Mode (EFEM)",null,"Off",null,"Off",{"$nulls":3},"Engineering Mode Strings.\nUsed for testing the network.","[Idle]-> *#**364#[Send]\nOn: can access the network info\nOff: cannot access the network info",null,"P"]
[]
[null,"Auto. Dial Number Parser & Correction",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Feature Enabled",null,"On",null,"On",{"$nulls":3},"LATAM feature requirement.\nTurn on  the Auto Dial-Num Parser & Correction (MRS9685/9686)","Setting=On: [Settings]-> [In-Call Setup]-> [Dialing Prefix] should exist\nSetting=Off: [Settings]-> [In-Call Setup]-> [Dialing Prefix] should NOT exist",null,"P"]
[null,"Auto Change",null,"Off",null,"Off",{"$nulls":3},"Auto Change Values: \nOff: Dial-num will not be changed\nAdd: operator-code will be added if it is not present.\nReplace or Add: operator-code will be added if it is not present; and will be replaced if it is present.","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Auto Change]",null,"P"]
[null,"Selected Operator",null,1,null,1,{"$nulls":3},"Which operator is selected as active one. \nValue range: 1~16\nIf [Auto Change] is not set as OFF, there must be at lease one opertors in list.","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Max. Operator Prefix Length",null,6,null,6,{"$nulls":3},"Max. length of operator prefix (long distance operator code).\nValue must be <= 6.","Not viewable from UI"]
[null,"Min. Operator Prefix Length",null,2,null,2,{"$nulls":3},"Min. length of operator prefix (long distance operator code).\n1 <= value <= max.length","Not viewable from UI"]
[null,"Preferred Operator 1",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",null,"Embratel",null,"Embratel",{"$nulls":3},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",null,21,null,21,{"$nulls":3},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 2",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",null,"TIM",{"$nulls":5},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",null,41,{"$nulls":5},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 3",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",null,"SuperTel",{"$nulls":5},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",null,61,{"$nulls":5},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 4",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 5",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 6",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 7",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 8",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 9",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 10",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 11",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 12",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 13",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 14",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 15",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Preferred Operator 16",null,"Default",null,"Customer Requirement"]
[null,"Operator Name",{"$nulls":7},"Name of long distance operator.\n1<=length<=16","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[null,"Operator Prefix",{"$nulls":7},"Long distance operator code","[Settings]-> [In-Call Setup]-> [Dialing Prefix]-> [Pref. Operator]",null,"P"]
[]
[null,"STK",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"SETUP CALL confirmation",null,"Off",null,"Off",{"$nulls":3},"LATAM requirement.\nOn: When STK command SETUP_CALL is requested, the phone will ask for confirmation from user to dial the call.\nOff: No confirmation needed for SETUP_CALL.","Not viewable from UI"]
[]
[null,"Network",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Show/Hide SPN",null,"Hide Item",null,"Hide Item",{"$nulls":3},"Show/Hide SPN on the Idle screen.","SPN is displayed on the 2nd Operator Line of the idle screen (HPLMN). Only for the SIM card which provided this feature."]
[null,"Short string digit == 1",null,"Off",null,"On",{"$nulls":3},"if short string digits is set to \"n\", then only \"n+1\" number of digits/characters can be treated as valid number.\nOn: any combination of two characters/numbers, could be *7, 77, etc.\nOff: any combination of three characters/numbers, could be *77, 777, etc","Dial \"*7\" in dile mode. When set as On, \"*7\" will be treated as a valid number. Otherwise, it will be treated as USSD"]
[]
[null,"FM Radio",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Default frequency ",null,87.5,{"$nulls":5},"The default frequency user can hear when turnning on the FM radio.","Please plug in headset first. [Multimeida]->[FM Radio]",null,"P"]
[null,"Preset frequency 1",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 2",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 3",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 4",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 5",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 6",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 7",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 8",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Preset frequency 9",null,87.5,{"$nulls":5},"The preset frequency.","Please plug in headset first. [Multimeida]->[FM Radio]->[Option]->[Manage Presets]",null,"P"]
[null,"Channel 1",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 2",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 3",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 4",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 5",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 6",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 7",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 8",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"Channel 9",null,"Default",null,"Customer Requirement"]
[null,"Channel Name",{"$nulls":7},"Name of Channel.\nlength<=10","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets->Options->Rename"]
[null,"Frequency",null,87.5,{"$nulls":5},"Frequency of Channel.","[Multimeida]->[FM Radio]->Options->Manage Presets",null,"P","[Multimeida]->[FM Radio]->Options->Manage Presets"]
[null,"SMS auto registration( for CMCC)",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Feature Enabled",null,"Off",{"$nulls":5},"Enable/Disable Motorola UE automatic registration via SMS","Not viewable from UI."]
[null,"Total call time",null,30,{"$nulls":5},"Threshould of total call time to invlke SMS registration. Default is 30 minutes","Not viewable from UI."]
[null,"Total SMS number",null,30,{"$nulls":5},"Threshold of total SMS number to invoke SSM registration. Default is 30 times.","Not viewable from UI."]
[null,"One-to-one list of MCC-MNC, SP number, Port number ",{"$nulls":7},"MCC_MNC: Mobile Country Code:Mobile Network Code, for this profile.\nSP number: SMS SP numbers associated with MCC-MNC codes.\nPort number: Port numbers associated  with MCC_MNC codes and SP numbers.\nPlease list all service info in following format\nMCC-MNC,","Not viewable from UI."]
[null,"Network comparison",null,"On",{"$nulls":5},"Comparing current network MCC-MNC code to that of IMSI.","Not viewable from UI."]
[null,"Maximun attempt times",null,3,{"$nulls":5},"The number fo maximum attempt times.","Not viewable from UI."]
[null,"DM Terminal Registration by SMS( for CMCC)",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Feature Enabled",null,"Off",{"$nulls":5},"Enable/Disable DM Terminal Registration by SMS","Not viewable from UI."]
[null,"Carrier server 1",null,"Default",null,"Customer Requirement"]
[null,"MNC",{"$nulls":7},"Mobile network code","Not viewable from UI."]
[null,"Carrier server ID ",{"$nulls":7},"The carrier server ID shall contain the SMS number and the destination port of the DM server","Not viewable from UI."]
[null,"Carrier server 2",null,"Default",null,"Customer Requirement"]
[null,"MNC",{"$nulls":7},"Mobile network code","Not viewable from UI."]
[null,"Carrier server ID ",{"$nulls":7},"The carrier server ID shall contain the SMS number and the destination port of the DM serve","Not viewable from UI."]
[null,"Carrier server 3",null,"Default",null,"Customer Requirement"]
[null,"MNC",{"$nulls":7},"Mobile network code","Not viewable from UI."]
[null,"Carrier server ID ",{"$nulls":7},"The carrier server ID shall contain the SMS number and the destination port of the DM serve","Not viewable from UI."]
[null,"Carrier server 4",null,"Default",null,"Customer Requirement"]
[null,"MNC",{"$nulls":7},"Mobile network code","Not viewable from UI."]
[null,"Carrier server ID ",{"$nulls":7},"The carrier server ID shall contain the SMS number and the destination port of the DM serve","Not viewable from UI."]
[null,"Carrier server 5",null,"Default",null,"Customer Requirement"]
[null,"MNC",{"$nulls":7},"Mobile network code","Not viewable from UI."]
[null,"Carrier server ID ",{"$nulls":7},"The carrier server ID shall contain the SMS number and the destination port of the DM serve","Not viewable from UI."]
[null,"Airplane Mode",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Feature Enabled",null,"Off",null,"On",{"$nulls":3},"Enable/Disable airplane mode.","Not viewable from UI."]
[null,"Display name in setting menu",null,"Airplane Mode",{"$nulls":5},"Set display name in setting menu","[Settings]",null,"P"]
[null,"Display name in menu title",null,"Airplane Mode",{"$nulls":5},"Set display name in menu tile","[Settings]->[Airplane Mode]",null,"P"]
[null,"Display name in sub-menu title",null,"Airplane Mode",{"$nulls":5},"Set display name in sub-menu tile","[Settings]->[Airplane Mode]->[Airplane Mode]",null,"P"]
[null,"Display name in dialog content",null,"Airplane Mode",{"$nulls":5},"Set display name in dialog content.","[Settings]->[Airplane Mode]->[Airplane Mode]->[On/Off]",null,"P"]
[null,"Display name in Home Screen",null,"Airplane Mode",{"$nulls":5},"Set display name in home screen.","The service name on Home Screen",null,"F"]
[null,"Cipher A5.1/5.2/5.3",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"A5.1",null,"On",null,"On",{"$nulls":3},"Enable/Disable A5.1","Not viewable from UI."]
[null,"A5.2",null,"Off",null,"Off",{"$nulls":3},"Enable/Disable A5.2","Not viewable from UI."]
[null,"A5.3",null,"On",null,"On",{"$nulls":3},"Enable/Disable A5.3","Not viewable from UI."]
[null,"Out-Of-Box Provision"]
[null,"Feature Enabled",null,"Off",null,"Off",{"$nulls":3},"Enable/Disable out of box provision","Not viewable from UI."]
[null,"Java",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Java Profile 1",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"中華電信",null,"Java Session","OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":3},"200.169.126.11","10.30.3.151",{"$error":"#REF!"},null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":3},0,"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,"claro.com.br","web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":3},"claro",null,{"$error":"#REF!"},null,"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":3},"claro",null,{"$error":"#REF!"},null,"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",null,"Read & write",{"$nulls":3},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",null,"http://wap.claro.com.br/jogos",{"$nulls":3},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile 2",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"台灣大哥大",null,null,"OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile 3",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",null,"遠傳電信",null,null,"OrangePlus",{"$error":"#REF!"},null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile4",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile5",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile6",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile7",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile8",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P","10.1.1.1"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P",8080]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile9",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P"]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"Java Profile10",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments"]
[null,"Profile Name",{"$nulls":4},"OrangePlus",null,null,"The name of the profile.","[Game&Apps]-> [Java settings]-> [Profile] -> Profile Name",null,"P"]
[null,"MCC:MNC",null,"000:00",{"$nulls":5},"Mobile Country Code:Mobile Network Code, for this profile","Not viewable from UI."]
[null,"Proxy Enable",null,false,{"$nulls":5},"Enable proxy server","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Enable]"]
[null,"Proxy Server Address (WAP 2.0)",{"$nulls":4},"10.30.3.151",null,null,"Proxy Server Address","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy IP]",null,"P"]
[null,"Proxy Port Number (WAP 2.0)",{"$nulls":4},"9201",null,null,"Proxy Port Number","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Protocol type]-> [HTTP]-> [Proxy Port]",null,"P"]
[null,"GPRS Access Point Name",null,"internet",null,null,"web.orangehk.com",{"$error":"#REF!"},null,"GPRS Access Point Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS Access Point]",null,"P"]
[null,"GPRS User Name\n---\nUser Name",{"$nulls":7},"GPRS User Name","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS username]\n---\n[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [User Name]",null,"P"]
[null,"GPRS Password\n---\nPassword",{"$nulls":7},"GPRS Password","[Game&Apps]-> [Java settings]-> [Profile]-> [Edit]-> [Data Bearer]-> [GPRS password]\n---\n[WebAccess]-> [Web Sessions]-> [Profile]-> [Edit]-> [Password]",null,"P"]
[null,"Access Type",null,"Read & write",{"$nulls":5},"Decide if the profile is editable. When it is set as read only, it means this profile can't be edited. The option \"Edit\" will be hidden.","[Game&Apps]-> [Java settings]-> [Profile]",null,"P"]
[null,"Game Page URL",null,"http://",{"$nulls":5},"Get Java application URL","[Game&Apps]-> [Java settings]-> [Profile]-> [Select the Profile]-> [View]-> Homepage"]
[]
[null,"DRM Setup",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"DRM Exclusive Forward Lock",null,"Off",null,"Off",{"$nulls":3},"Exclusive FL will only support DRM forward lock type. Current setting supports all DRM forward lock, combined delivery and separated delivery types.","Not viewable from UI."]
[null,"Warning Prompt before browsing",null,"Default",null,"Customer Requirement",null,"Change from Default",null,"Comments","Validation Path"]
[null,"Enable the warning prompt of Browser",null,"Disable warning prompt",null,"Disable warning prompt",{"$nulls":3},"When browsing from [Main Menu]->[WebAccess]->[Browser] or [Main Menu]->[Browser], if DUT should show a prompt about \"Additional charges may apply\"","[Main Menu]->[WebAccess]->[Browser] or [Main Menu]->[Browser]"]