{"text_format":"5","workbook":"xls","n_sheets":10,"sheets":["01_Misc Setup","02_NAM","03_SMS-MMS","04_Subsidy Lock","05_Data connectivity","06_aGPS","Engineering (Hide)","Template Revision History ","History list","CPV Input"],"props":{"title":"E380 PRI","creator":"Rafael Canabal","last_modified_by":"wfr063","manager":"Osvaldo Meneghel","company":"Motorola"},"custom":{"_EmailSubject":"[V3c] Verizon Dominican Republic PRI Validation","_AuthorEmail":"pablo.gomez@omegaqa.com","_AuthorEmailDisplayName":"Pablo Gomez"},"defined_names":["_120E_Ringtones","_60X_Ringtones","_720_MENU_ORDER","_720_RING_TONES","_C33x_Ring","C343_MENU_ORDER","C343_RING_TONES","V60E_P_MENU_ORDER"],"not_rendered":{"external_links":1,"defined_names":19,"comments":44},"notes":{"written":44,"chars":6728},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"01_Misc Setup","index":0,"n_rows":75,"n_cols":59,"rows_kept":75,"merged":[[0,0,0,13],[2,0,3,1],[2,2,2,5],[2,7,2,8],[2,9,2,12],[3,2,3,5],[3,7,3,8],[3,9,3,12],[4,7,4,8],[4,9,4,12],[5,0,5,1],[5,2,5,5],[6,0,6,1],[6,2,6,5],[6,7,6,8],[6,9,6,12],[7,0,7,1],[7,2,7,5],[7,7,7,8],[7,9,7,12],[8,1,8,2],[8,4,8,5],[9,1,9,2],[9,4,9,5],[11,0,12,0],[11,1,11,13],[12,1,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,13],[13,1,13,13],[14,1,14,3],[14,4,14,5],[14,6,14,7],[14,8,14,13],[15,1,15,3],[15,4,15,5],[15,6,15,7],[15,8,15,13],[16,1,16,3],[16,4,16,5],[16,6,16,7],[16,8,16,13],[17,1,17,3],[17,4,17,5],[17,6,17,7],[17,8,17,13],[18,1,18,3],[18,4,18,5],[18,6,18,7],[18,8,18,13],[19,1,19,3],[19,4,19,5],[19,6,19,7],[19,8,19,13],[20,1,20,3],[20,4,20,5],[20,6,20,7],[20,8,20,13],[21,1,21,3],[21,4,21,5],[21,6,21,7],[21,8,21,13],[22,1,22,3],[22,4,22,5],[22,6,22,7],[22,8,22,13],[23,1,23,13],[24,1,24,3],[24,4,24,5],[24,6,24,7],[24,8,24,13],[25,1,25,3],[25,4,25,5],[25,6,25,7],[25,8,25,13],[26,1,26,3],[26,4,26,5],[26,6,26,7],[26,8,26,13],[27,1,27,3],[27,4,27,5],[27,6,27,7],[27,8,27,13],[28,1,28,3],[28,4,28,5],[28,6,28,7],[28,8,28,13],[29,1,29,3],[29,4,29,5],[29,6,29,7],[29,8,29,13],[30,1,30,3],[30,4,30,5],[30,6,30,7],[30,8,30,13],[31,1,31,3],[31,4,31,5],[31,6,31,7],[31,8,31,13],[32,1,32,3],[32,4,32,5],[32,6,32,7],[32,8,32,13],[33,1,33,3],[33,4,33,5],[33,6,33,7],[33,8,33,13],[34,1,34,3],[34,4,34,5],[34,6,34,7],[34,8,34,13],[35,1,35,3],[35,4,35,5],[35,6,35,7],[35,8,35,13],[36,1,36,3],[36,4,36,5],[36,6,36,7],[36,8,36,13],[37,1,37,3],[37,4,37,5],[37,6,37,7],[37,8,37,13],[38,1,38,3],[38,4,38,5],[38,6,38,7],[38,8,38,13],[39,1,39,3],[39,4,39,5],[39,6,39,7],[39,8,39,13],[40,0,40,13],[41,1,41,3],[41,4,41,5],[41,6,41,7],[41,8,41,13],[42,1,42,3],[42,4,42,5],[42,6,42,7],[42,8,42,13],[43,1,43,3],[43,4,43,5],[43,6,43,7],[43,8,43,13],[44,1,44,3],[44,4,44,5],[44,6,44,7],[44,8,44,13],[45,1,45,3],[45,4,45,5],[45,6,45,7],[45,8,45,13],[46,1,46,3],[46,4,46,5],[46,6,46,7],[46,8,46,13],[47,1,47,3],[47,4,47,5],[47,6,47,7],[47,8,47,13],[48,1,48,3],[48,4,48,5],[48,6,48,7],[48,8,48,13],[49,1,49,3],[49,4,49,5],[49,6,49,7],[49,8,49,13],[50,1,50,3],[50,4,50,5],[50,6,50,7],[50,8,50,13],[51,1,51,3],[51,4,51,5],[51,6,51,7],[51,8,51,13],[52,1,52,3],[52,4,52,5],[52,6,52,7],[52,8,52,13],[53,1,53,3],[53,4,53,5],[53,6,53,7],[53,8,53,13],[54,1,54,3],[54,4,54,5],[54,6,54,7],[54,8,54,13],[55,1,55,3],[55,4,55,5],[55,6,55,7],[55,8,55,13],[56,1,56,3],[56,4,56,5],[56,6,56,7],[56,8,56,13],[57,1,57,3],[57,4,57,5],[57,6,57,7],[57,8,57,13],[58,1,58,3],[58,4,58,5],[58,6,58,7],[58,8,58,13],[59,1,59,3],[59,4,59,5],[59,6,59,7],[59,8,59,13],[60,1,60,3],[60,4,60,5],[60,6,60,7],[60,8,60,13],[61,0,61,13],[62,1,62,3],[62,4,62,5],[62,6,62,7],[62,8,62,13],[63,1,63,3],[63,4,63,5],[63,6,63,7],[63,8,63,13],[64,1,64,3],[64,4,64,5],[64,6,64,7],[64,8,64,13],[65,0,65,13],[66,1,66,3],[66,4,66,5],[66,6,66,7],[66,8,66,13],[67,1,67,3],[67,4,67,5],[67,6,67,7],[67,8,67,13],[68,1,68,3],[68,4,68,5],[68,6,68,7],[68,8,68,13],[69,1,69,3],[69,4,69,5],[69,6,69,7],[69,8,69,13],[70,0,70,13],[71,1,71,3],[71,4,71,5],[71,6,71,7],[71,8,71,13],[72,1,72,3],[72,4,72,5],[72,6,72,7],[72,8,72,13],[73,0,73,13],[74,1,74,3],[74,4,74,5],[74,6,74,7],[74,8,74,13]],"headers":{"footer":["Motorola Confidential","","Page"]},"flags":["formulas_cached_only"]}
["V3c_República Dominicana_Verizon_WOMinlock"]
[]
["T-Option/ \nSpec No:",{"$nulls":6},"PRI Version",null,2.8]
[{"$nulls":7},"PRI Date",null,"2006-07-13"]
[{"$nulls":7},"PRI Expiration Date",null,"2007-07-13"]
["Software Version",null,"GATW_05.04.00R"]
[{"v":"Monster file name","$note":[{"by":"Alexandre Araujo","t":"The file name, cannot be read through UI."}]},null,"V3CLA_05.04.00R_Verizon_Dominican_Republic_Monster_2006-07-05_JAGla11511.shx.gz",{"$nulls":4},"Carrier",null,"Verizon"]
[{"v":"Flex file version ","$note":[{"by":"Alexandre Araujo","t":"To check flex number, go to test mode --> Version View --> Flex Version"}]},null,"XS4VZDR01GATWLA1D.00R - 0.1",{"$nulls":4},"Country",null,"República Dominicana"]
["PRL - NAM1","1901-683C_EVDO.rla",null,"Version",{"v":1901,"d":"01901"}]
["PRL - NAM2","1901-683C_EVDO.rla",null,"Version",{"v":1901,"d":"01901"}]
[]
["Item 1","Initial Setup,Personalize,and other features"]
[null,"Name",null,null,"Default Value",null,"Customer Selection",null,"Description",{"$nulls":6},"How to Check Manually ?"]
[null,"Ringstyles"]
["1.01","Style",null,null,"Loud",null,"Loud",null,"Loud,Soft,Vibrate,Vibe&Ring,Silent",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Style <Change>","Loud","Soft","Vibrate","Vibe&Ring","Silent"]
["1.02","Calls",null,null,"Classic",null,"Classic",null,"Select the default ringer tone from the list of tones available on the phone. ",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Calls","Silent","Classic","Vibe Dot","Vibe Dash","Vibe Dot Dot","Vibe Dot Dash","Vibe Pulse","Alert","Triads","Nightlife","Wind Chime","Random","Bit & Bytes","Door Bell","Chimes High","Chimes Low","Ding","TaDa","Notify","Drum","Claps","Fanfare","Chord High","Chord low","Ambient","Dynamic","Energize","Espresso","Helix","Hello Moto","Hyperactive","Jitters","Latin loops","Motion","Passion","Power surge","Rings","Sonic","Tempo","This is techno","Urban style","Velvet","Waves"]
["1.03","Inbox",null,null,"Alert",null,"Alert",null,"Select the default ringer tone from the list of tones available on the phone. ",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Inbox","Silent","Classic","Vibe Dot","Vibe Dash","Vibe Dot Dot","Vibe Dot Dash","Vibe Pulse","Alert","Triads","Nightlife","Wind Chime","Random","Bit & Bytes","Door Bell","Chimes High","Chimes Low","Ding","TaDa","Notify","Drum","Claps","Fanfare","Chord High","Chord low","Ambient","Dynamic","Energize","Espresso","Helix","Hello Moto","Hyperactive","Jitters","Latin loops","Motion","Passion","Power surge","Rings","Sonic","Tempo","This is techno","Urban style","Velvet","Waves"]
["1.04","Voicemail",null,null,"Alert",null,"Alert",null,"Select the default ringer tone from the list of tones available on the phone. ",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Voicemail ","Silent","Classic","Vibe Dot","Vibe Dash","Vibe Dot Dot","Vibe Dot Dash","Vibe Pulse","Alert","Triads","Nightlife","Wind Chime","Random","Bit & Bytes","Door Bell","Chimes High","Chimes Low","Ding","TaDa","Notify","Drum","Claps","Fanfare","Chord High","Chord low","Ambient","Dynamic","Energize","Espresso","Helix","Hello Moto","Hyperactive","Jitters","Latin loops","Motion","Passion","Power surge","Rings","Sonic","Tempo","This is techno","Urban style","Velvet","Waves"]
["1.05","Alarms",null,null,"Alert",null,"Alert",null,"Select the default ringer tone from the list of tones available on the phone. ",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Alarms","Silent","Classic","Vibe Dot","Vibe Dash","Vibe Dot Dot","Vibe Dot Dash","Vibe Pulse","Alert","Triads","Nightlife","Wind Chime","Random","Bit & Bytes","Door Bell","Chimes High","Chimes Low","Ding","TaDa","Notify","Drum","Claps","Fanfare","Chord High","Chord low","Ambient","Dynamic","Energize","Espresso","Helix","Hello Moto","Hyperactive","Jitters","Latin loops","Motion","Passion","Power surge","Rings","Sonic","Tempo","This is techno","Urban style","Velvet","Waves"]
["1.06","Data Calls",null,null,"Alert",null,"Alert",null,"Select the default ringer tone from the list of tones available on the phone. ",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Data Calls","Silent","Classic","Vibe Dot","Vibe Dash","Vibe Dot Dot","Vibe Dot Dash","Vibe Pulse","Alert","Triads","Nightlife","Wind Chime","Random","Bit & Bytes","Door Bell","Chimes High","Chimes Low","Ding","TaDa","Notify","Drum","Claps","Fanfare","Chord High","Chord low","Ambient","Dynamic","Energize","Espresso","Helix","Hello Moto","Hyperactive","Jitters","Latin loops","Motion","Passion","Power surge","Rings","Sonic","Tempo","This is techno","Urban style","Velvet","Waves"]
["1.07","Fax Calls",null,null,"Alert",null,"Alert",null,"Select the default ringer tone from the list of tones available on the phone. ",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Fax Calls","Silent","Classic","Vibe Dot","Vibe Dash","Vibe Dot Dot","Vibe Dot Dash","Vibe Pulse","Alert","Triads","Nightlife","Wind Chime","Random","Bit & Bytes","Door Bell","Chimes High","Chimes Low","Ding","TaDa","Notify","Drum","Claps","Fanfare","Chord High","Chord low","Ambient","Dynamic","Energize","Espresso","Helix","Hello Moto","Hyperactive","Jitters","Latin loops","Motion","Passion","Power surge","Rings","Sonic","Tempo","This is techno","Urban style","Velvet","Waves"]
["1.08","Ringer ID",null,null,"On",null,"On",null,"On,Off",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Ringer ID","On","Off"]
["1.09","Reminders",null,null,"Beep",null,"Beep",null,"Beep,Vibrate,OFF",{"$nulls":6},"Menu, Tones & Images, Ring Styles, Loud Detail <Change> ↓ Reminders","Beep","Vibrate","OFF"]
[null,"Personalize"]
["1.10","Home Screen/Home Keys/Icons",null,null,"Show",null,"Show",null,"Show,Hide",{"$nulls":6},"Menu, Personalize, Home Screen , Home Keys","Show","Hide"]
["1.11","Home Screen/Home Keys/Up",null,null,"Media Center",null,"Media Center",null,"Media Center,Alert Styles,Settings,Shortcuts,Voice Memos,Office tools,Contacts,recent calls,message center,Brew,Browser, Video Camera",{"$nulls":6},"Menu, Personalize, Home Screen , Home Keys, UP","Media Center","Alert Styles","Settings","Shortcuts","Voice Memos","Office tools","Contacts","Recent calls","Message Center","Brew","Browser","Video Camera"]
["1.12","Home Screen/Home Keys/Down",null,null,"Neo Mensajería",null,"Message Center",null,"Media Center,Alert Styles,Settings,Shortcuts,Voice Memos,Office tools,Contacts,recent calls,message center,Brew,Browser, Video Camera",{"$nulls":6},"Menu, Personalize,  Home Screen , Home Keys, Down","Neo Mensajería","Alert Styles","Settings","Shortcuts","Voice Memos","Office tools","Contacts","Recent calls","Message Center","Brew","Browser","Video Camera"]
["1.13","Home Screen/Home Keys/Left",null,null,"Neo Aplicaciones",null,"Brew",null,"Media Center,Alert Styles,Settings,Shortcuts,Voice Memos,Office tools,Contacts,recent calls,message center,Brew,Browser, Video Camera",{"$nulls":6},"Menu, Personalize, Home Screen , Home Keys, Left","Neo Aplicaciones","Alert Styles","Settings","Shortcuts","Voice Memos","Office tools","Contacts","Recent calls","Message Center","Brew","Browser","Video Camera"]
["1.14","Home Screen/Home Keys/Right",null,null,"Neo Nevagacion",null,"Browser",null,"Media Center,Alert Styles,Settings,Shortcuts,Voice Memos,Office tools,Contacts,recent calls,message center,Brew,Browser, Video Camera",{"$nulls":6},"Menu, Personalize, Home Screen , Home Keys, Right","Neo Navegación","Alert Styles","Settings","Shortcuts","Voice Memos","Office tools","Contacts","Recent calls","Message Center","Brew","Browser","Video Camera"]
["1.15","Home Screen/Home Keys/Left Soft Key",null,null,"Recent calls",null,"Recent calls",null,"Media Center,Alert Styles,Settings,Shortcuts,Voice Memos,Office tools,Contacts,recent calls,message center,Brew,Browser, Video Camera",{"$nulls":6},"Menu, Personalize, Home Screen , Home Keys, Left Soft Key","Media Center","Alert Styles","Settings","Shortcuts","Voice Memos","Office tools","Contacts","Recent calls","Message Center","Brew","Browser","Video Camera"]
["1.16","Home Screen/Home Keys/Right Soft Key",null,null,"Contacts",null,"Contacts",null,"Media Center,Alert Styles,Settings,Shortcuts,Voice Memos,Office tools,Contacts,recent calls,message center,Brew,Browser, Video Camera",{"$nulls":6},"Menu, Personalize, Home Screen , Home Keys, Right Soft Key","Media Center","Alert Styles","Settings","Shortcuts","Voice Memos","Office tools","Contacts","Recent calls","Message Center","Brew","Browser","Video Camera"]
["1.17","Home Screen/Layout",null,null,"Centered",null,"Centered",null,"Left Justified,Centered",{"$nulls":6},"Menu, Personalize, Home Screen , Layout","Left Justified","Centered"]
["1.18","Home ScreenBanner",{"$nulls":4},"Motorola",null,"Banner in Home Screen (12 Characters max)  This the message/banner that appears above time and date stamp on idle mode.",{"$nulls":6},"Menu, Settings, Personalize, Home Screen , Banner"]
["1.19","Home Screen/Clock",null,null,"Digital",null,"Digital",null,"Digital,Analog",{"$nulls":6},"Menu, Personalize, Home Screen , Clock","Digital","Analog"]
["1.20","Main Menu/View",null,null,"Icons",null,"Icons",null,"Icons,List",{"$nulls":6},"Menu, Personalize, Main Menu , View","Icons","List"]
["1.21","Wallpaper/Picture",{"$nulls":13},"Menu, Personalize, Wallpaper , Picture"]
["1.22","Wallpaper",null,null,"Fit-to-screen",null,"Fit-to-screen",null,"Center\nTile\nFit-to-screen",{"$nulls":6},"Menu, Personalize, Wallpaper , Layout","Center","Tile","Fit-to-screen"]
["1.23","Screensaver/Picture",{"$nulls":13},"Menu, Personalize, Screen Saver, Picture"]
["1.24","Screensaver/Delay",null,null,"Off",null,"1 minute",null,"OFF\n1 minute\n2 minutes",{"$nulls":6},"Menu, Personalize, Screen Saver, Delay","OFF","1 minute","2 minutes"]
["1.25","Skinning",null,null,"Moto",null,"Moto",null,"This will customize the interface used by the terminal.",{"$nulls":6},"Menu, Personalize, Skin","Moto","Scarlet","Techno","Vivo"]
["In-Call-Setup"]
["1.26","Time Format",null,null,"12H",null,"12 hour",null,"The phone will display the time in any of these formats:\n12H: For example 12:00am\n24H: For example 00:00",{"$nulls":6},"Menu, Other Functions, Settings, Initial Setup, Time and  Date, <Change>","12 hour","24 hour"]
["1.27","Date format",null,null,"dd-mmm-yy",null,"12/31/99",null,"dd-mm-yy: 30-Aug-03\ndd-mm-yy: 30-08-03\nmm-dd-yy: 08-30-03",{"$nulls":6},"Menu, Other Functions, Settings, Initial Setup, Time and  Date,  ↓ <Change>, Format <Change>","12/31/99","31/12/99","31-DEC-1999"]
["1.28","Auto Redial",null,null,"Off",null,"Off",null,"On: To enable auto redialing when call origination fails.\nOff: To disable auto redialing.",{"$nulls":6},"Menu, Other Functions, Settings, Initial Setup, Auto Redial","On","Off"]
["1.29","Display Timeout",null,null,"2 Minutes",null,"2 minutes",null,"Off, 1 min, 2min, 5 min, 10 min",{"$nulls":6},"Menu, Other Functions, Settings, Initial Setup, Display Timeout","Off","1 minute","2 minutes","5 minutes","10 minutes"]
["1.30","Backlight",null,null,"20 Seconds",null,"5 seconds",null,"5 sec, 10 sec, 20 sec, 30 sec, 50 sec",{"$nulls":6},"Menu, Other Functions, Settings, Initial Setup, Backlight","5 seconds","10 seconds","20 seconds","30 seconds","50 seconds"]
["1.31","Menu Scroll",null,null,"Wrap arround",null,"Wrap Around",null,"UP/DOWN: \nWrap arround:",{"$nulls":6},"Menu, Other Functions, Settings, Initial Setup, Scroll","UP/DOWN","Wrap Around"]
["1.32","Current Language",null,null,"Spanish",null,"Spanish",null,"Options: Spanish,Portuguese,English \n",{"$nulls":6},"Menu , Other Functions, Settings, Language, <Change>","Spanish","Portuguese","English"]
["1.33","DTMF",null,null,"Long",null,"Short",null,"Off: No DTMF tones transmited                                                                                                                                                                                                                        Long: Long DTMF tones transmited\nShort: Short DTMF tones transmited",{"$nulls":6},"Menu, Settings, Initial Setup, DTMF","Off","Long","Short"]
["1.34","Open to answer",null,null,"Off",null,"On",null,"On: The phone will connect the incoming call when flip is opened. \nOff: The phone will not connect the incoming call when flip is opened. ",{"$nulls":6},"Menu, Other Functions, Settings, In-Call Setup, Answer Options, Open to answer","On","Off"]
["1.35","Multiple Key answer",null,null,"Off",null,"On",null,"\nOn: The user can answer an incoming call by pressing any key\nOff: The user can only answer an incoming call by pressing SEND.",{"$nulls":6},"Menu, Other Functions, Settings, In-Call Setup, Answer Options, Multi-Key","On","Off"]
["1.36","Auto answer (Headset and Car settings)",null,null,"2 seconds",null,"Off",null,"Off\n2 seconds\n5 seconds\n10 seconds",{"$nulls":6},"Menu, Other Functions, Settings, Car Settings or Headset, Auto answer , <Change>","Off","2 seconds","5 seconds","10 seconds"]
["1.37","Auto Handsfree",null,null,"On",null,"Off",null,"On: \nOff: ",{"$nulls":6},"Menu, Other Functions, Settings, Car Settings or Headset, Auto Handsfree","On","Off"]
["1.38","Auto Display Hyphens",null,null,"Off",null,"On",null,"If ON,autho hyphenation will be enabled. For example: 1234-567-890",{"$nulls":6},"Press 12345678890 and check, if OFF will display without hyphens","On","Off"]
["1.39","Wake Up Greeting Enabled",null,null,"Enabled",null,"Enabled",null,"Enabled: The user will be able to personalize the wake up greeting.\nDisabled: The item \"Wake up Greeting\" won't appear inside the \"Personalize\" Menu, not allowing the user to set a wake up greeting.",{"$nulls":6},"if ON - Menu, Personalize, Greeting","Enabled","Disabled"]
["1.40","Carrier wakeup banner",{"$nulls":6},"Animated GIF file format.  Max size is 15K,7-8 frames per second.  This information is contained in the flex file.",{"$nulls":6},"Turn on the Phone, Wake UP Banner"]
["1.41","Carrier wakeup greeting",{"$nulls":6},"Insert a text string with 32 letters max sixe. Appears when the phone is waking up.",{"$nulls":6},"if ON - Menu, Personalize, Greeting"]
["1.42","Carrier wakeup greeting Editable",null,null,"On",{"$nulls":3},"On: The user will be able to personalize the wake up greeting.\nOff: The item \"Wake up Greeting\" won't appear inside the \"Personalize\" Menu,not allowing the user to set a wake up greeting.",{"$nulls":5},"Invalid Entry","if ON - Menu, Personalize, Greeting","On","Off"]
["1.42","External Display",null,null,"Movilnet",null,"Motorola",null,"Text or Graphic file to be shown on the external display when the flip is open",{"$nulls":6},"Text to be shown on the external display when the flip is open"]
["1.43","Browser Splash Screen Picture",null,null,"default Image",null,"OPENWAVE",null,"GIF/BMP file format. Max size is 12K. This information is contained in the flex file.",{"$nulls":6},"If ON - lauching the Browser and check the image."]
["1.44","Browser Splash Screen",null,null,"ON",null,"ON",null,"ON - Openwave GIF file appears when launching the Browser;\nOFF - No Wake-up Banner pictures appears when launching the Browser.",{"$nulls":6},"If ON - lauching the Browser and check the image.","ON","OFF"]
["Bluetooth Setup"]
["1.45","Power",null,null,"Off",null,"Off",null,"On\nOff",{"$nulls":6},"Menu, Other Functions, Connection, Bluetooth Link <Select>, Setup <Select>, Power  <Change>","On","Off"]
["1.46","Voice Dial",null,null,"Off",null,"On",null,"On\nOff",{"$nulls":6},"CPV","On","Off"]
["1.47","Transfer files",null,null,"Enabled",null,"Disabled",null,"Enabled\nDisabled",{"$nulls":6},"if On you can transfer files by bluetooth. ","Enabled","Disabled"]
["Other Settings"]
["1.48","Location Setting",null,null,"On",null,"On",null,"On: Phone allows the user to be found.\nOff: Phone does not allows the user to be found.",{"$nulls":6},"Menu, Other Functions, Settings, Location Setting","On","Off"]
["1.49","Calling Voice Mail \nwhen pressing \"1\"",null,null,"On",null,"On",null,"On: The key number 1 will be used as a quick dial for the voice mail.\nOff: The key number 1 will be used as a quick dial for the phone stored on the first memory position.",{"$nulls":6},"press number 1 for few seconds, if apperar \"Calling VoiceMail\" feature is ON ","On","Off"]
["1.50","Digital TTY",null,null,"Off",null,"On",null,"This feature allows the phone to be used as a modem for devices designed for hearing empaired people.",{"$nulls":6},"Menu, Settings, Initial Setup, if appear on Menu feature  is ON","On","Off"]
["1.51","EFS File System",null,null,"Disabled",null,"Enabled",null,"Enabled/Disabled",{"$nulls":6},"FLEX - CPV","Enabled","Disabled"]
["Multimedia Settings"]
["1.52","Video Length (Phone & MMC Memory)",null,null,"Maximum",null,"Maximum",null,"MMS: Shortest duration\nLong: Medium duration\nMaximum: Maximum duration",{"$nulls":6},"Video , Videos Setup, Video Length","MMS","Long","Maximum"]
["1.53","Camera Resolution",null,null,"High",null,"Medium",null,"Thumbnail (160x120)\n Low (320x240)\n Medium (640x480)\n High (1280x960)",{"$nulls":6},"Camera , Menu, Picutre Setup, Resolution <Change>","Thumbnail","Low","Medium","High"]
["EVDO Settings"]
["1.54","Phone Operation",null,null,"Hybrid",null,"Hybrid",null,"Hybrid\nCDMA 1x only mode\nEVDO only mode",{"$nulls":6},"Menu 0setup","Hybrid","CDMA 1x only mode","EVDO only mode"]

{"sheet":"02_NAM","index":1,"n_rows":34,"n_cols":20,"rows_kept":34,"merged":[[0,0,1,0],[0,1,1,14],[4,1,4,3],[4,9,4,12],[4,13,4,14],[5,1,5,3],[5,9,5,12],[5,13,5,14],[6,1,6,3],[6,9,6,12],[6,13,6,14],[7,1,7,3],[7,9,7,12],[7,13,7,14],[8,1,8,3],[8,9,8,12],[8,13,8,14],[9,13,9,14],[10,1,10,3],[11,1,11,3],[11,9,11,12],[11,13,11,14],[12,1,12,3],[12,9,12,12],[12,13,12,14],[13,9,13,12],[13,13,13,14],[14,1,14,3],[14,9,14,12],[14,13,14,14],[15,1,15,3],[15,9,15,12],[16,1,16,3],[16,9,16,12],[17,1,17,3],[17,9,17,12],[17,13,17,14],[18,9,18,12],[18,13,18,14]],"headers":{"footer":["Motorola Confidential","","Page"]},"flags":["formulas_cached_only"]}
["Item 2","NAM Settings"]
[]
[]
[null,"NAM Fields",null,null,"NAM1","NAM2","How to Check Manually ?"]
["2.01",{"v":"Option Byte 1","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\nOption Byte 1:\nBit 2 => Dissallow non-Home side foreign SID in PSCAN.  True = 1; False = 0\nBit 7 => Local Use Mark.  This bit must ALWAYS be set to 1"}]},null,null,"10000000","10000000",{"$nulls":3},"Carrier Defined Phone Numbers",{"$nulls":6},"How to Check Manually ?"]
["2.02",{"v":"Mobile Identification Number","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nMIN:\nIf the MIN is not an ESN based number this value must be set to either 1111110111 OR a specific number that is desired.\nIf ESN based it must be 000000****, where **** will be based on the ESN.\n\nNOTE: Make sure you specify if it's ESN based or not in Section 8.0 \"Security Information\" under \"Mobile ID Number\"."}]},null,null,"000000****","000000****",null,null,"2.27","Emergency Number 1",{"$nulls":3},911,null,null,"Menu 0setup , 00000  Extended NAM "]
["2.03",{"v":"Mobile Directory Number (Phone Number)","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nMDN:\nMake sure the value of the MDN is the same as the MIN value."}]},null,null,"000000****","000000****",null,null,"2.28","Emergency Number 2",{"$nulls":6},"Menu 0setup , 00000  Extended NAM "]
["2.04",{"v":"Station Class Mark (SCM)","$note":[{"by":"batwings","t":"Motorola PC:\nNon-FLEX\n\nSCM: \nThis will have a value between 0-255 decimal. The choices are:\n  106 = CDMA 800/AMPS 800\n  160 = CDMA 1900\n  234 = CDMA Dual Band"}]},null,null,234,234,null,null,"2.29","Emergency Number 3",{"$nulls":6},"Menu 0setup , 00000  Extended NAM "]
["2.05",{"v":"Option Byte 3","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nOption Byte 3:\nbits 7 and  6 => Active NAMS \n   00 = single NAM\n   01 = dual NAM\n\nHence, the 2 options for this field are:\n\"00000000\"=> Single NAM\n\"01000000\"=> Dual NAM"}]},null,null,"01000000",{"$nulls":3},"2.30","Voice Mail Number",{"$nulls":3},"*9",null,null,"Menu, Message Center,   Message settings , voice mail"]
["2.06","Option Byte 4",null,null,"00100000",{"$nulls":3},"2.31","Voice Portal number (VIVO feature only)"]
["2.07",{"v":"Option Byte 5","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nOption Byte 5:\nBit 0=> Mob Term for NID Roamer\n   \"0\"=OFF ; \"1\" =ON;  (must be ON)\nBit 1=> Mob Term for SID Roamer\n   \"0\"=OFF ; \"1\"=ON; (must be ON)\nBit 2=> Mob Term  for Home Roamer\n   \"0\"=OFF ; \"1\"=ON (must be ON)\nBit 3=> Voice Privacy Feature\n   \"0\"= OFF ; \"1\"= ON\nBit 6 and 5=> Preferred mode.\n   If 6 = 0 and 5 = 0, => CDMA Only\n   If 6 = 0 and 5 = 1, => CDMA Preferred\n   If 6 = 1 and 5 = 0. => Analog Only\n   If 6 = 1 and 5 = 1, => CDMA Selected (Voice Privacy)\nBit 7=> Force Preferred VOCODER on Terminations\n   \"0\" = OFF; \"1\" = ON;"}]},null,null,"00001111","00001111"]
["2.08",{"v":"CDMA Slot Cycle Index","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nValid choices for Slot Cycle Index are 0-7."}]},null,null,2,2,{"$nulls":3},"Security Information"]
["2.09",{"v":"CDMA Home System ID (SID  1)","$note":[{"by":"batwings","t":"Motorola PC:\nNon-FLEX\n\nIf SID is only 4 digits, add a 0 before the SID.\n(For eg:  05205)"}]},null,null,"08832","08832","Menu 0setup , 00000  - SID/NID Pair",null,"2.32",{"v":"A Key  NAM1","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe options are:\n  Random\n  Zero"}]},{"$nulls":3},"Random"]
["2.10","CDMA Network ID (NID 1)",null,null,65535,65535,"Menu 0setup , 00000  - SID/NID Pair",null,"2.33",{"v":"A Key  NAM2","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe options are:\n  Random\n  Zero"}]},{"$nulls":3},"Random"]
["2.11","Mobile Country Code (MCC)",null,null,"370","370",null,null,"2.34",{"v":"Phone Lock Code","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\n4 digit lock code for locking the phone. Defaulted to \"1234\".\n"}]},{"$nulls":3},1234,null,null,"Menu 0setup , 00000  Extended NAM "]
["2.12","IMSI 12 and IMSI 11",null,null,"02","02",null,null,"2.35",{"v":"Master Subsidy lock","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe choices are:\n  -Random => Type \"Random\"\n  -Fixed => Type in the value of the fixed password that will be used.\n  -Zero (None) => Type \"Zero\"\n"}]},{"$nulls":3},"Zero",{"$note":[{"by":"wed014","t":"If fixed the Password should be field here"}]}]
["2.13",{"v":"System Mode","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nSystem Mode:\n0 - Home Only\n1 - Standard Scan\n2 - ScanA\n3 - ScanB\n4 - Automatic A (Verizon only feature)\n5 - Automatic B (Verizon only feature)"}]},null,null,1,1,null,null,"2.36",{"v":"One-time Subsidy lock","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe choices are:\n  -Random => Type \"Random\"\n  -Fixed => Type in the value of the fixed password that will be used.\n  -Zero (None) => NOT SUPPORTED !!!\n"}]},{"$nulls":3},"Zero",{"$note":[{"by":"wed014","t":"If fixed the Password should be field here"}]}]
["2.14",{"v":"Vocoder Type","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nThe regular 8K option is not available for 1X phones. Hence the only options for this field are \"Yes\" or \"No\".\n"}]},null,null,"EVRC","EVRC",null,null,"2.37","Number of Retries",{"$nulls":3},15]
["2.15","CDMA Primary Ch. System A",null,null,283,283,"Menu 0setup , 00000  Extended NAM ",null,"2.38",{"v":"Mobile ID Number","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nESN Based\nNone\n"}]},{"$nulls":3},"ESN BASED"]
["2.16","CDMA Primary Ch. System B",null,null,384,384,"Menu 0setup , 00000  Extended NAM "]
["2.17","CDMA Secondary Ch. System A",null,null,691,691,"Menu 0setup , 00000  Extended NAM ",null,null,"MIN Matching Check",null,"NAM1","NAM2"]
["2.18","CDMA Secondary Ch. System B",null,null,777,777,"Menu 0setup , 00000  Extended NAM ",null,"2.39","NAM",null,true,true]
[{"$nulls":8},"2.40","MDN",null,true,true]
[null,"Option Byte 3"]
["2.19","Number of NAMs",null,null,2]
[null,"Option Byte 4"]
["2.20","Long DTMF Enabled",null,null,"Y"]
[null,"Option Byte 5",null,null,"NAM1","NAM2",{"$nulls":11},"CDMA Preferred","CDMA Only","CDMA Selected (Voice Privacy)"]
["2.21","Mob Term for NID Roamer",null,null,"Y","Y"]
["2.22","Mob Term for SID Roamer",null,null,"Y","Y"]
["2.23","Mob Term for Home Roamer",null,null,"Y","Y"]
["2.24","Voice Privacy",null,null,"Y","Y"]
["2.25","Prefferred Mode",null,null,"CDMA Only","CDMA Only"]
["2.26","Force Prefferred Vocoder",null,null,"N","N"]

{"sheet":"03_SMS-MMS","index":2,"n_rows":19,"n_cols":23,"rows_kept":19,"merged":[[0,0,1,0],[0,1,0,11],[1,1,1,3],[1,4,1,5],[1,6,1,11],[3,1,3,3],[3,4,3,5],[3,6,3,11],[4,1,4,3],[4,4,4,5],[4,6,4,11],[5,1,5,3],[5,4,5,5],[5,6,5,11],[6,1,6,3],[6,4,6,5],[6,6,6,11],[7,1,7,3],[7,4,7,5],[7,6,7,11],[8,1,8,3],[8,4,8,5],[8,6,8,11],[9,1,9,3],[9,4,9,5],[9,6,9,11],[11,1,11,3],[11,4,11,5],[11,6,11,11],[12,1,12,3],[12,4,12,5],[12,6,12,11],[13,1,13,3],[13,4,13,5],[13,6,13,11],[14,1,14,3],[14,4,14,5],[14,6,14,11],[15,1,15,3],[15,4,15,5],[15,6,15,11],[16,1,16,3],[16,4,16,5],[16,6,16,11],[17,1,17,3],[17,4,17,5],[17,6,17,11],[18,1,18,3],[18,4,18,5],[18,6,18,11]],"headers":{"footer":["","Page of"]},"flags":["formulas_cached_only"]}
["Item 3","MMS/SMS Settings"]
[null,"Name",null,null,"Value",null,"Description"]
["MMS only settings "]
["3.01","MMSC server URL",null,null,"http://mms.verizon.net.do/servlets/mms",null,"Server URL it self (same as SERVER NAME/IP inside phone MMS settings)."]
["3.02","MMSC IP Address",{"$nulls":4},"Server IP adress equivalent to server URL (Not available inside phone MMS settings)."]
["3.03","MMSC IP port",null,null,8080,null,"(Not available inside phone MMS settings)"]
["3.04","Profile URL.",null,null,"http://uaprof.vtext.com/mot/v3/v3v1.xml",null,"URL where RDF file is stored (same as UAPROF URL inside phone MMS settings)."]
["3.05","Proxy HTTP URL.",{"$nulls":4},"Proxy URL address itself (Not available inside phone MMS settings)."]
["3.06","Proxy HTTP IP",{"$nulls":4},"Proxy IP address itself (same as PROXY IP inside phone MMS settings)"]
["3.07","Proxy HTTP Port",{"$nulls":4},"Proxy Port Number"]
["SMS only settings"]
["3.09","MO SMS to email",null,null,"On",null,"This option allows the user to send an MO SMS to an email address. MO SMS MUST be enabled before this can be enabled. The options are: \nOn; Off; Automatically filled based on email gateway info.",{"$nulls":6},"On","Off"]
["3.10","MO SMS default entry mode",null,null,"TAP Method",null,"If the MO SMS to email is off, then the \"To:\" field will accept only Numeric Entry. Inside the message body the options are: Numeric, Tap Methof, iTAP, Symbol",{"$nulls":6},"iTAP","TAP Method","Numeric","Symbol"]
["3.11","SMS to email gateway",null,null,6245,null,"Phone number assigned to the SMS to email gateway"]
["3.12","Max # of chars in a MO SMS",null,null,160]
["3.13","Primary Input Method for SMS",null,null,"TAP (Language)",null,"This is the default selected input method for composing text messages",{"$nulls":6},"iTAP English","iTAP Español","iTAP Português","TAP (Language)","TAP Extendido"]
["3.14","Secondray Input Method of SMS",null,null,"iTAP Español",null,"This is the secondary input method for composing text messages",{"$nulls":6},"None","iTAP English","iTAP Español","iTAP Português","TAP (Language)","TAP Extendido"]
["3.15","SMS Character Support",null,null,"7-Bits",null,"7 Bits: Normal ASCII  table.\n8 Bits: Extended ASCII table (supports LatAm characters)",{"$nulls":6},"7-Bits","8-Bits",{"$nulls":7},"Default: 7-Bits"]
["3.16","Delivery Report for SMS",null,null,"Off",null,"On\nOff",{"$nulls":6},"On","Off"]

{"sheet":"04_Subsidy Lock","index":3,"n_rows":30,"n_cols":21,"rows_kept":30,"merged":[[0,0,1,0],[0,1,0,5],[1,1,1,5],[1,6,1,7],[1,8,1,13],[2,3,2,5]],"headers":{"footer":["","Page of"]},"flags":["formulas_cached_only"]}
["Item 4","Subsidy lock"]
[null,"MIN Matching Table"]
[null,null,"MIN 2","MIN 1"]
[null,"Lines","Digit 1","Digit 2","Digit 3","Digit 1",{"$nulls":11},"MIN NAM1","MIN NAM2","MDN NAM1","MDN NAM2"]
[null,1,{"$nulls":14},0,0,0,0,0]
[null,2,{"$nulls":14},0,0,0,0,0]
[null,3,{"$nulls":14},0,0,0,0,0]
[null,4,{"$nulls":14},0,0,0,0,0]
[null,5,{"$nulls":14},0,0,0,0,0]
[null,6,{"$nulls":14},0,0,0,0,0]
[null,7,{"$nulls":14},0,0,0,0,0]
[null,8,{"$nulls":14},0,0,0,0,0]
[null,9,{"$nulls":14},0,0,0,0,0]
[null,10,{"$nulls":14},0,0,0,0,0]
[null,11,{"$nulls":14},0,0,0,0,0]
[null,12,{"$nulls":14},0,0,0,0,0]
[null,13,{"$nulls":14},0,0,0,0,0]
[null,14,{"$nulls":14},0,0,0,0,0]
[null,15,{"$nulls":14},0,0,0,0,0]
[null,16,{"$nulls":14},0,0,0,0,0]
[null,17,{"$nulls":14},0,0,0,0,0]
[null,18,{"$nulls":14},0,0,0,0,0]
[null,19,{"$nulls":14},0,0,0,0,0]
[null,20,{"$nulls":14},0,0,0,0,0]
[null,21,{"$nulls":14},0,0,0,0,0]
[null,22,{"$nulls":14},0,0,0,0,0]
[null,23,{"$nulls":14},0,0,0,0,0]
[null,24,{"$nulls":14},0,0,0,0,0]
[null,25,{"$nulls":14},0,0,0,0,0]
[{"$nulls":16},0,0,0,0,0]

{"sheet":"05_Data connectivity","index":4,"n_rows":54,"n_cols":17,"rows_kept":54,"merged":[[0,0,1,0],[0,1,1,7],[2,1,2,3],[3,1,3,3],[4,1,4,3],[5,1,5,3],[6,1,6,3],[7,1,7,3],[8,1,8,3],[9,1,9,3],[10,1,10,3],[12,1,12,5],[13,1,13,3],[13,4,13,5],[14,1,14,3],[14,4,14,5],[15,1,15,3],[15,4,15,5],[16,4,16,5],[17,4,17,5],[18,4,18,5],[20,1,20,5],[21,1,21,3],[21,4,21,5],[22,1,22,3],[22,4,22,5],[23,1,23,3],[23,4,23,5],[24,1,24,3],[24,4,24,5],[25,1,25,3],[25,4,25,5],[26,1,26,3],[26,4,26,5],[27,1,27,3],[27,4,27,5],[28,1,28,3],[28,4,28,5],[29,1,29,3],[29,4,29,5],[30,1,30,3],[30,4,30,5],[31,1,31,3],[31,4,31,5],[32,1,32,3],[32,4,32,5],[34,1,34,5],[35,1,35,3],[35,4,35,5],[36,1,36,3],[36,4,36,5],[37,1,37,3],[37,4,37,5],[38,1,38,3],[38,4,38,5],[39,1,39,3],[39,4,39,5],[40,1,40,3],[40,4,40,5],[41,1,41,3],[41,4,41,5],[42,1,42,3],[42,4,42,5],[44,1,44,3],[46,1,46,5],[47,1,47,3],[49,1,49,3],[51,1,51,5],[53,1,53,3]],"flags":["formulas_cached_only"]}
["Item 5","Data connectivity"]
[]
["# 1","CDMA Browser Settings",null,null,"Profile 1","Profile 2","Profile 3","Profile 4"]
[5.01,"Profile name",null,null,"VZW"]
[5.02,"Edit rights",null,null,"Yes"]
[{"v":5.029999999999999,"d":"5.03"},"WAP IP 1",null,null,"200.88.125.27"]
[{"v":5.039999999999999,"d":"5.04"},"WAP Port 1",null,null,8080]
[{"v":5.049999999999999,"d":"5.05"},"WAP IP 2",null,null,"200.88.125.27"]
[{"v":5.059999999999999,"d":"5.06"},"WAP Port 2",null,null,8080]
[{"v":5.0699999999999985,"d":"5.07"},"Timeout (Linger time)",null,null,30]
[{"v":5.079999999999998,"d":"5.08"},"Default Home Page URL",null,null,"http://homepage"]
[]
["# 2","Browser Options"]
[{"v":5.089999999999998,"d":"5.09"},{"v":"Browser Enable","$note":[{"by":"batwings","t":"Motorola MDB:\nThe options are:\n - YES\n - NO\n\n"}]},"Browser Enable","Browser Enable","Yes",{"$nulls":3},"Yes","No"]
[{"v":5.099999999999998,"d":"5.10"},{"v":"Cache Start Up","$note":[{"by":"batwings","t":"Motorola MDB:\nWhen this is turned ON, the phone will always go to the last site visited during the previous session. The options available are:\n - ON\n - OFF\n"}]},"Cache Start Up","Cache Start Up","Off",{"$nulls":3},"On","Off"]
[{"v":5.109999999999998,"d":"5.11"},{"v":"Confirmation at start","$note":[{"by":"batwings","t":"Motorola MDB:\nIf set to ON,  phone will prompt user that additional charges my apply when browser is launched. The options are:\n - ON\n - OFF"}]},"Confirmation at start","Confirmation at start","Off",{"$nulls":3},"On","Off"]
[{"v":5.119999999999997,"d":"5.12"},"Invisible Net - Instant Messaging URL (Vivo Only)"]
[{"v":5.129999999999997,"d":"5.13"},"Invisible Net - Chat WAP URL (Vivo Only)"]
[{"v":5.139999999999997,"d":"5.14"},"Invisible Net - Email WAP URL (Vivo Only)"]
[]
["# 3","Brew Settings"]
[{"v":5.149999999999997,"d":"5.15"},{"v":"Primary DNS","$note":[{"by":"batwings","t":"Motorola MDB:\nPrimary IP address of the Brew Server. This needs to be decided by the Carrier in consulation with Qualcomm."}]},null,null,"196.003.081.005"]
[{"v":5.159999999999997,"d":"5.16"},{"v":"Secondary DNS","$note":[{"by":"batwings","t":"Motorola MDB:\nSecondary IP address of the Brew Server. This also needs to be decided by the Carrier in consulation with Qualcomm."}]},"Secondary DNS","Secondary DNS","196.003.081.132"]
[{"v":5.169999999999996,"d":"5.17"},{"v":"Authentication Policy","$note":[{"by":"batwings","t":"Motorola MDB:\nThis is determined by the carrier depending on the kind of authentication they want to employ. The choices are:\n- None (No separate authentication)\n- SID\n- Text\n- Number"}]},"Authentication Policy","Authentication Policy","SID",{"$nulls":3},"None","SID","Text","Number"]
[{"v":5.179999999999996,"d":"5.18"},{"v":"Privacy Policy","$note":[{"by":"batwings","t":"Motorola MDB:\nThis is determined by the carrier, depending on what kind of approved applications can be run on the phone. The choices are:\n- BREW: Qualcomm signed apps\n- Carrier: Carrier only needs to authorize apps.\n- BREW or Carrier: Either Qualcomm, OR the carrier can authorize the apps.\n- BREW and Carrier: Either Qualcomm AND the carrier can authorize the apps."}]},"Privacy Policy","Privacy Policy","BREW or Carrier ",{"$nulls":3},"Brew","Carrier","BREW or Carrier ","BREW and Carrier"]
[{"v":5.189999999999996,"d":"5.19"},{"v":"Key Use","$note":[{"by":"batwings","t":"Motorola MDB:\nThis field is used to determine which key is used for authentication. This field has 2 possible values. \n- B-Key;\n- A-Key;"}]},"Key Use","Key Use","B-Key",{"$nulls":3},"B-Key","A-Key"]
[{"v":5.199999999999996,"d":"5.20"},{"v":"Check Prepay option (On = Yes Off = No)","$note":[{"by":"batwings","t":"Motorola MDB:\nThis flags indicates that this maybe a prepay phone and BREW needs to check with ADS before allowing an application to download. The possibe values are:\n- NO = Phone cannot be switched between prepay and postpay.\n- YES = Phone can be switched between prepay and postpay.\n"}]},"Check Prepay option","Check Prepay option","Off",{"$nulls":3},"On","Off"]
[{"v":5.2099999999999955,"d":"5.21"},{"v":"Prepaid phone option","$note":[{"by":"batwings","t":"Motorola MDB:\nThis flag indicates that this is a BREW prepay phone. Any purchases that are made from this phone requires the user's account to be checked out for sufficient funds before allowing an application to download. \nThe possible values are:\n- Postpay phone\n- Prepay phone\n\nNote: This field can only be chosen if the \"Check Prepay\" option is also chosen. That is,only if \"Check Prepay\"=\"YES\""}]},"Prepaid phone option","Prepaid phone option","Postpay",{"$nulls":3},"Postpay","Prepay"]
[{"v":5.219999999999995,"d":"5.22"},{"v":"ADS Commercial Server URL","$note":[{"by":"batwings","t":"Motorola MDB:\nURL entry of the commercial web server.\n\n"}]},"ADS Commercial Server URL","ADS Commercial Server URL","brew.verizon.net.do "]
[{"v":5.229999999999995,"d":"5.23"},{"v":"ADS Test Server URL","$note":[{"by":"batwings","t":"Motorola MDB:\nURL entry of the test web server.\n\n"}]},"ADS Test Server URL","ADS Test Server URL"]
[{"v":5.239999999999995,"d":"5.24"},"Carrier Id","ADS Test Server URL","ADS Test Server URL",63]
[{"v":5.249999999999995,"d":"5.25"},"Platform Id","ADS Test Server URL","ADS Test Server URL",8092]
[{"v":5.2599999999999945,"d":"5.26"},"Advice of Charge in Brew",null,null,"OFF",{"$nulls":3},"ON","OFF"]
[]
["# 4","1X Data Connection"]
[{"v":5.269999999999994,"d":"5.27"},{"v":"MDR Mode","$note":[{"by":"batwings","t":"Motorola MDB:\nMDR Mode Options (MDR=Medium Data Rate, also known as HSPD)\nThe options are:\n- MDR Only: MS will originate w/ SO22 or SO25 only. If these are not available, MS will not negotiate to other Service Options.\n- MDR if available: MS will originate w/ SO22 or SO25. If these are not available, MS will negotiate LSPD Service Options.  MS will NOT negotiate 1X (SO33).\n- No MDR: MS will originate LSPD only. MS will NOT negotiate SO 22, 25 or 33.\n- Svc Opt 33 Prfd: MS will originate 1X (SO33). If these are not available, it will negotiate to MDR or LSPD."}]},null,null,"SO 33 Preferred",{"$nulls":3},"MDR Only","MDR If Available","No MDR","SO 33 Preferred"]
[{"v":5.279999999999994,"d":"5.28"},{"v":"Service Option","$note":[{"by":"batwings","t":"Motorola MDB:\nThis is used to set the Data Service Option number set. This is saved in the NVM of the phone.\n- Pre-707 SO numbers\n- Qualcomm proprietary SO numbers\n- IS-707 SO numbers"}]},"Service Option","Service Option","IS-707",{"$nulls":3},"Pre 707","QC Proprietary","IS-707"]
[{"v":5.289999999999994,"d":"5.29"},{"v":"Data QNC","$note":[{"by":"batwings","t":"Motorola MDB:\nThis is to enable or disable Quick Net Connect.\n- Disable: This means that Packet Originations will use the Packet Data Service Option number.\n- Enable: This means that Packet Originations will use the Async Data Service Option number.\n"}]},"Data QNC","Data QNC","Yes",{"$nulls":3},"Yes","No"]
[{"v":5.299999999999994,"d":"5.30"},{"v":"Data SCRM","$note":[{"by":"batwings","t":"Motorola MDB:\nThis is to enable or disable Data SCRM.\n- Disable:\n- Enable:"}]},"Data QNC","Data QNC","Yes",{"$nulls":3},"Yes","No"]
[{"v":5.309999999999993,"d":"5.31"},{"v":"Primary DNS","$note":[{"by":"batwings","t":"Motorola MDB:\nThis is to enable or disable Data SCRM.\n- Disable:\n- Enable:"}]},"Data QNC","Data QNC","196.3.81.5"]
[{"v":5.319999999999993,"d":"5.32"},"Secondary DNS","Data QNC","Data QNC","196.3.81.132"]
[{"v":5.329999999999993,"d":"5.33"},"Dial Up Number",null,null,"#777"]
[{"v":5.339999999999993,"d":"5.34"},"PAP or CHAP","Data QNC","Data QNC","CHAP",{"$nulls":3},"PAP","CHAP"]
[{"v":5.3499999999999925,"d":"5.35"},"Username",null,null,"MDN","@vzdr3g.com",null,null,"ESN-Hex","ESN-Dec","MIN","MDN","Fixed"]
[{"v":5.359999999999992,"d":"5.36"},{"v":"Password","$note":[{"t":"q15483:\nThis field needs to be null for random password"}]},null,null,"Fixed","vzw",null,null,"ESN-Hex","ESN-Dec","MIN","MDN","Fixed","Random","Fixed",null,"Random1 (Movistar): 16 dígits alphanumeric with lower and upper caps alternanted randomic.\n\nRandom2 (Vivo): 16 dígits alphanumeric with lower caps only alternanted randomic."]
[]
["# 5","EVDO Data Connection"]
[{"v":5.369999999999992,"d":"5.37"},"PAP or CHAP","Data QNC","Data QNC","PAP",{"$nulls":3},"PAP","CHAP"]
[{"v":5.379999999999992,"d":"5.38"},"Username",null,null,"MDN","@vzdr3g.com",null,null,"ESN-Hex","ESN-Dec","MIN","MDN","Fixed"]
[{"v":5.389999999999992,"d":"5.39"},{"v":"Password","$note":[{"t":"q15483:\nThis field needs to be null for random password"}]},null,null,"Fixed","vzw",null,null,"ESN-Hex","ESN-Dec","MIN","MDN","Fixed","Random",null,null,"Random1 (Movistar): 16 dígits alphanumeric with lower and upper caps alternanted randomic.\n\nRandom2 (Vivo): 16 dígits alphanumeric with lower caps only alternanted randomic."]
[]
["# 6","CSD Connection"]
[{"v":5.3999999999999915,"d":"5.40"},"Username",null,null,"Fixed","qnc",null,null,"ESN-Hex","ESN-Dec","MIN","MDN","Fixed"]
[{"v":5.409999999999991,"d":"5.41"},{"v":"Password","$note":[{"t":"q15483:\nThis field needs to be null for random password"}]},null,null,"Fixed","qnc",null,null,"ESN-Hex","ESN-Dec","MIN","MDN","Fixed","Random1","Random2"]

{"sheet":"06_aGPS","index":5,"n_rows":6,"n_cols":15,"rows_kept":6,"merged":[[0,0,1,0],[0,1,0,11],[1,1,1,3],[1,4,1,5],[1,6,1,11],[3,1,3,3],[3,4,3,5],[3,6,3,11],[4,1,4,3],[4,4,4,5],[4,6,4,11],[5,1,5,3],[5,4,5,5],[5,6,5,11]],"flags":["formulas_cached_only"]}
["Item 6","aGPS Settings"]
[null,"Name",null,null,"Value",null,"Description"]
["aGPS settings"]
["6.01","PTLM type",null,null,"TCP/IP",null,"Choose between data burst or TCP/IP",{"$nulls":6},"TCP/IP","Data Burst"]
["6.02","PTLM IP",null,null,"0.0.0.0",null,"GPS one server"]
["6.03","PTLM Port",null,null,0,null,"GPS one port"]

{"sheet":"Engineering (Hide)","index":6,"n_rows":15,"n_cols":16,"rows_kept":15,"merged":[[0,0,2,0],[0,1,1,11],[2,1,2,3],[2,4,2,5],[2,6,2,11],[3,1,3,3],[3,4,3,5],[3,6,3,11],[4,1,4,3],[4,4,4,5],[4,6,4,11],[5,1,5,3],[5,4,5,5],[5,6,5,11],[6,1,6,3],[6,4,6,5],[6,6,6,11],[7,1,7,3],[7,4,7,5],[7,6,7,11],[8,1,8,3],[8,4,8,5],[8,6,8,11],[9,1,9,3],[9,4,9,5],[9,6,9,11],[10,1,10,3],[10,4,10,5],[10,6,10,11],[11,1,11,3],[11,4,11,5],[11,6,11,11],[12,1,12,3],[12,4,12,5],[12,6,12,11],[13,1,13,3],[13,4,13,5],[13,6,13,11],[14,1,14,3],[14,4,14,5],[14,6,14,11]],"flags":["formulas_cached_only"]}
["Item 7","Engineering"]
[]
[null,"Name",null,null,"Value",null,"Description"]
[7.01,"All SMS on Traffic Channel",null,null,"Enabled",null,"Enable: All SMS messages will use the Traffic Channels.\nDisable: SMS messages will be sent depending on network configuration.",{"$nulls":6},"Enabled","Disabled"]
[7.02,"Allow New System Redial",null,null,"No",null,"When a call Fails, whether you can Redial = (Yes, No)",{"$nulls":6},"Yes","No"]
[7.03,"BREW Test Enable",null,null,"Off",null,"On, Off",{"$nulls":6},"On","Off"]
[7.04,"Background Scan Timer",null,null,2700,null,"Time that the terminal will scan while idle. (Enter value in seconds)"]
[7.05,"Re-Scan on Release",null,null,"Off",null,"On, Off",{"$nulls":6},"On","Off"]
[7.06,"Video Format",null,null,"H263",null,"Encoding Format (H263, MP4)",{"$nulls":6},"H263","MP4"]
[7.07,"Audio Format",null,null,"AMR",null,"Encoding Format (QCELP,AAC,AMR)",{"$nulls":6},"QCELP","AAC","AMR"]
[7.08,"Send Key Format",null,null,"Dialed/Received Calls",null,"Dialed Calls\nDialed/Received Calls",{"$nulls":6},"Dialed Calls","Dialed/Received Calls"]
[7.09,"Service Level",null,null,"Restrict Access = 0",null,"Restrict Access = 0\nFull Access = 4",{"$nulls":6},"Restrict Access = 0","Full Access = 4"]
[{"v":7.1,"d":"7.10"},"WAP Connection Type",null,null,"WAP2.0",null,"WAP 1.0 = (WSP, WTLS, WTP)\nWAP 2.0 = (HTTP, TCP/UDP, IP)",{"$nulls":6},"WAP1.0","WAP2.0"]
[7.11,"User Agent Header (MMS)",null,null,"motov3",null,"User Agent String to be sent to the MMS Server."]
[7.12,"User Agent Header (Browser)",null,null,"MOT-GATW_/00.62 UP.Browser/6.2.3.4.c.1.109 (GUI) MMP/2.0",null,"User Agent String to be sent to the Browser Server."]

{"sheet":"Template Revision History ","index":7,"n_rows":35,"n_cols":7,"rows_kept":35,"hidden":true,"merged":[[0,0,1,0],[0,1,0,6],[1,1,1,3],[1,4,1,5],[1,7,1,10],[5,5,5,6],[6,5,6,6],[7,5,7,6],[8,5,8,6],[9,5,9,6],[10,5,10,6]],"flags":["formulas_cached_only"]}
["Item 9","History List"]
[]
["Version","Date",{"v":"Owner Name","$note":[{"t":"Administrator:\nWho is executing the change."}]},"Description of Change",{"v":"Item #","$note":[{"t":"Administrator:\nSee number in the PRI Spreadsheet, i.e.:\n4.0.17 (NAM File loc17); 5.0 (Need the field Name);...\n\n"}]},"Field Name"]
["1.0","2005-09-13","Evandro Dalben","Initial Release based on E815 v2.1 CPV"]
["1.1","2005-09-26","Evandro Dalben","CPV Mapping corrected by Eldorado"]
["2.0","2005-10-31","Evandro Dalben","Added new feature","1.43","Browser Splash Screen Picture"]
["2.0","2005-10-31","Evandro Dalben","Moved to Misc_Setup","1.44","Browser Splash Screen"]
["2.0","2005-10-31","Evandro Dalben","Added new feature","1.47","Transfer files"]
["2.0","2005-10-31","Evandro Dalben","Added new feature","3.16","Delivery Report for SMS"]
["2.0","2005-10-31","Evandro Dalben","Added new feature",5.26,"Advice of Charge in Brew"]
["2.1","2005-11-03","Evandro Dalben","Added new feature","2.37","Number of Retries"]
["2.2","2005-12-20","Evandro Dalben","Options and Description","1.42","Wake Up Greeting Editable"," Enabled/Disabled"]
["2.2","2005-12-20","Evandro Dalben","Options and Description","1.47","Location Setting"," On/Off"]
["2.2","2005-12-20","Evandro Dalben","Description","1.46","External Display"," Description"]
["2.2","2005-12-20","Evandro Dalben","Description","1.42","Wake Up Greeting Overwrite"," Description"]
["2.2","2005-12-20","Evandro Dalben","Description","1.54","Phone Operation"]
["2.2","2005-12-20","Evandro Dalben","Options","1.39","Wake Up Greeting Enabled","Enabled;Disabled"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","1.4x","Location Setting Authorization"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","3.01","MMSC server URL"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","2.14","Vocoder Type"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","5.34 / 5.37","PAP or CHAP"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","5.40 / 5.41","CSD Connection"]
["2.4","2006-03-08","Rodrigo Pescio","Updated description","3.10","MO SMS default entry mode"]
["2.5","2006-03-20","Evandro Dalben","CPV Sheet (Removed option)",null,"Dysplay File System Files"]
["2.6","2006-04-26","Thiago Couto","New options added","1.36","Auto answer (Headset and Car settings)"]
["2.6","2006-04-26","Thiago Couto","\"Invalid Entry\" form correction","5.39","Password"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","7.12","User Agent Header (MMS)"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.01","MMSC server URL"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.05","Proxy HTTP URL"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.08","Polling URL"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.11","SMS to email gateway (NAM 1)"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.11","SMS to email gateway (NAM 2)"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","7.04","Background Scan Timer"]
["2.7","2006-05-11","Thiago Santos","New values added (Random1 and Random2)","5.36 and 5.39","Password"]
["2.8","2006-07-03","Rodrigo Pescio","Hexin values changed","CPV Input"]

{"sheet":"History list","index":8,"n_rows":18,"n_cols":7,"rows_kept":18,"merged":[[0,0,1,0],[0,1,0,6],[1,1,1,3],[1,4,1,5],[1,6,1,7],[1,8,1,13]],"flags":["formulas_cached_only"]}
["Item 8","History List"]
[]
["Date",{"v":"Owner Name","$note":[{"t":"Administrator:\nWho is executing the change."}]},{"v":"Item #","$note":[{"t":"Administrator:\nSee number in the PRI Spreadsheet, i.e.:\n4.0.17 (NAM File loc17); 5.0 (Need the field Name);...\n\n"}]},"Field Name","Old Field Value","New Field Value","Version"]
["2006-05-24","Ana Guerrero",1.18,"HomeScreen Banner","PCS Verizon","Motorola",{"v":2.5,"d":"2.50"}]
["2006-05-24","Ana Guerrero",1.42,"External Display","Verizon","Motorola",{"v":2.5,"d":"2.50"}]
["2006-05-24","Ana Guerrero",null,"SW Version","GATW_05.02.00","GATW_05.04.00",{"v":2.5,"d":"2.50"}]
["2006-05-24","Ana Guerrero",3.12,"Max # of chars in MO SMS",132,160,{"v":2.5,"d":"2.50"}]
["2006-05-25","Carlos Ore",3.08,"Polling URL ","Empty","http://mms.verizon.net.do/servlets/mms"]
["2006-05-25","Carlos Ore",1.52,"Video Length","MMS","Maximun"]
["2006-05-25","Carlos Ore",1.11,"Home Screen/Home Keys/ Up","Shortcuts","Multimedia"]
["2006-05-25","Carlos Ore",1.13,"Home Screen/Home Keys/Left","Browser","Brew"]
["2006-05-25","Carlos Ore",1.14,"Home Screen/Home Keys/Right ","Brew","Browser"]
["2006-05-25","Carlos Ore",1.43,"Browser Splash Screen Picture","Empty","OPENWAVE"]
["2006-05-25","Carlos Ore",5.34,"PAP or CHAP","PAP","CHAP"]
["2006-05-25","Carlos Ore",6.03,"PTLM Port","Empty",0]
["2006-05-25","Carlos Ore",7.04,"Background Scan Timer",45,2700]
["2006-05-25","Carlos Ore",7.09,"Service Level","Full Access = 4",0]
["2006-07-10","Ana Guerrero",null,"Cambio de forma CPV"]

{"sheet":"CPV Input","index":9,"n_rows":496,"n_cols":6,"rows_kept":496,"flags":["formulas_cached_only"]}
["CUSTOMER ITEM","VALUE","COMMAND","HEXIN","FUNCTION","TOKEN STRING"]
["DEFINE_MA","CDMA1X6500"]
["DEFINE_MODEL","V3CB"]
["Header","######01_MISC SETUP#######################"]
["Header","PHONE STATUS"]
["Software Version","GATW_05.04.00R","VERSION","FFFF","Hex2ASCII","StartByte=5"]
["Flex File","XS4VZDR01GATWLA1D.00R - 0.1","RDELEM","288F00010000001B","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["PRL - NAM1 (Version)",1901,"RDELEM","0101000100010002","Hex2Dec","ByteSwap=True|BytesPerData=2"]
["PRL - NAM2 (Version)",1901,"RDELEM","0101000200010002","Hex2Dec","ByteSwap=True|BytesPerData=2"]
["Header","RINGSTYLES",null,null,"CDMA1XRingStyles"]
["Style","Loud","RDELEM","275A0001000A0001","SelectCase","00=Loud|01=Soft|02=Vibrate|03=Vibe&Ring|04=Silent"]
[" DEFINE_RINGTONES ","00=Continental|01=Classic|03=Acoustica|3B=Alert|14=Jitters|06=Bells|26=Bits & Bytes|2E=Cosmic|28=Ding|27=Door Bell|15=Upbeat|18=Expose|16=Expresso|17=Flare|08=Glacier|09=Guitar Strings|2B=Harmonics|0A=High Impact|0B=High Tide|0C=Higher Plane|2C=Interlude|12=Jubilation|11=Kaleidoscope|0D=Luna|0E=Mania|10=Moonlit Haze|0F=Nightlife|29=One Moment|2A=Provincial|25=Random|1A=Silent|2D=Snaggle|05=Standard|2F=Gyroscope|54=Triads|13=Up and Down|1C=Vibe Dash|1E=Vibe Dot Dash|1D=Vibe Dot Dot|1B=Vibe Dot|1F=Vibe Pulse|58=Wind Chime|30=Sweet|31=Chimes high|32=Chimes low|33=Ding|34=TaDa|35=Notify|36=Drum|37=Claps|38=Fanfare|39=Chord high|3A=Chord low|04=Ambient|3C=Dynamic|3D=Energize|3E=High Impact|3F=Moonlit Haze|48=Hello Moto|41=Passion|42=Power Surge|43=This Is Techno|44=Motion|4C=Velvet"]
["Calls","<MANUAL>",null,null,"GetAnswer","ANS=Calls"]
["Inbox","<MANUAL>",null,null,"GetAnswer","ANS=Inbox"]
["Voicemail","<MANUAL>",null,null,"GetAnswer","ANS=Voicemail"]
["Alarms","<MANUAL>",null,null,"GetAnswer","ANS=Alarms"]
["Data Calls","<MANUAL>",null,null,"GetAnswer","ANS=Data Calls"]
["Fax Calls","<MANUAL>",null,null,"GetAnswer","ANS=Fax Calls"]
["Ringer IDs","On","RDELEM","275C000100430001","SelectCase","00=Off|01=On"]
["Reminders","<MANUAL>",null,null,"GetAnswer","ANS=Reminders"]
["Ringer Volume","<MANUAL>",null,null,"GetAnswer","ANS=Ringer Volume"]
["Key Volume","<MANUAL>",null,null,"GetAnswer","ANS=Key Volume"]
["Header","PERSONALIZE",null,null,"CDMA1XKeys6XXX"]
["Home Screen/Home Keys/Icons","Show","RDELEM","275A000101120001","SelectCase","00=Hide|01=Show|02=2 Clicks"]
[" DEFINE_SOFTKEYS ","PhoneBook=CONTACTS|RecentCall=Recent Calls|Message=Message Center|GetItNow=Get It Now|Browser=Browser|WebAccess=Mobile Web|Mutilmedia=Media Gallery|Settings=Settings|Tools=Tools|PhoneStatus=Phone Info|Shortcuts=Shortcuts|VoiceRecord=Voice Record"]
["Home Screen/Home Keys/Up","Media Center",null,null,"GetAnswer","ANS=Scroll Up"]
["Home Screen/Home Keys/Down","Message Center",null,null,"GetAnswer","ANS=Scroll Down"]
["Home Screen/Home Keys/Left","Brew",null,null,"GetAnswer","ANS=Scroll Left"]
["Home Screen/Home Keys/Right","Browser",null,null,"GetAnswer","ANS=Scroll Right"]
["Home Screen/Home Keys/Left Soft Key","Recent calls",null,null,"GetAnswer","ANS=Left Soft Key"]
["Home Screen/Home Keys/Right Soft Key","Contacts",null,null,"GetAnswer","ANS=Right Soft Key"]
["Home Screen/Layout","Centered","RDELEM","275A000101100001","SelectCase","00=Left Justified|01=Centered"]
["Banner Enabled","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=391|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Home ScreenBanner","Motorola","RDELEM","2773000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Home Screen/Clock","Digital","RDELEM","275A000101110001","SelectCase","00=Digital|01=Analog"]
["Main Menu/View","Icons","RDELEM","275A000100BE0001","SelectCase","00=Icons|01=List"]
["Wallpaper/Picture","<MANUAL>","RDELEM","2947000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Wallpaper","Fit-to-screen","RDELEM","275A000100BA0001","SelectCase","00=Center|01=Tile|02=Fit-to-screen"]
["Screensaver/Picture","<MANUAL>","RDELEM","293D000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Screensaver/Delay","1 minute","RDELEM","275A000100B90001","SelectCase","00=Off|01=1 minute|02=2 minutes|03= 5 minutes|04=10 minutes"]
["Skinning","Moto","RDELEM","29CB000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","IN-CALL-SETUP"]
["Time Format","12 hour","RDELEM","275A000100010001","SelectCase","00=12 hour|01=24 hour"]
["Date Format","12/31/99","RDELEM","275A000100000001","SelectCase","00=12/31/99|01=31/12/99|02=31-DEC-1999"]
["Auto Redial","Off","RDELEM","275A000100030001","SelectCase","00=Off|01=On"]
["Display Timeout","2 minutes","RDELEM","275A0001010E0001","SelectCase","00=Off|01=1 minute|02=2 minutes|03=5 minutes|04=10 minutes"]
["Backlight","5 seconds","RDELEM","275A000100040001","SelectCase","00=Off|01=5 seconds|02=10 seconds|03=20 seconds|04=30 seconds|05=50 seconds"]
["TTY Setup","<MANUAL>","RDELEM","275A000100AF0001","SelectCase","00=Voice|01=TTY|02=VCO|03=HCO"]
["Menu Scroll","Wrap Around","RDELEM","275A000100070001","SelectCase","00=Up/Down|01=Wrap Around"]
["Current Language","Spanish","RDELEM","275E000101440001","Languages"]
["DTMF","Short","RDELEM","275A000100450001","SelectCase","00=Off|01=Short|02=Long"]
["Open to Answer","On","RDELEM","275A000100140001","SelectCase","00=Off|01=On"]
["Multi Key Answer","On","RDELEM","275A000100130001","SelectCase","01=On|00=Off"]
["Auto Answer (Headset and Car Settings)","Off","RDELEM","275A000100520001","SelectCase","00=Off|01=On|02=2 seconds|05=5 seconds|0A=10 seconds"]
["Auto Handsfree","Off","RDELEM","275A000100460001","SelectCase","00=Off|01=On"]
["Auto Display Hyphens","On","RDELEM","275A000101320001","SelectCase","00=Off|01=On|02=Auto"]
["Wake Up Greeting Enable","Enabled","RDELEM","2742000100000000","FeatureId","FeatureId=392|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Carrier Wakeup Banner","<MANUAL>"]
["Carrier Wakeup Greeting","None Entered","RDELEM","284A000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Greeting Editable","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=392|IfSetDisplay=On|IfNotSetDisplay=Off"]
["External Display","Motorola","RDELEM","2771000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2"]
["Browser Splash Screen Picture","<MANUAL>"]
["Browser Splash Screen","<MANUAL>"]
["Time/Date Autoupdate","<MANUAL>","RDELEM","275A0001003C0001","SelectCase","00=Off|01=On"]
["Header","BLUETOOTH SETUP"]
["Power","Off","RDELEM","275A0001004E0001","SelectCase","00=Off|01=On"]
["Voice Dial","On","RDELEM","275A000101340001","SelectCase","00=Off|01=On"]
["Transfer Files","Disabled","RDELEM","2742000100000000","FeatureId","FeatureId=942|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Header","OTHER SETTINGS"]
["Location Setting","On","RDELEM","275A0001015F0001","SelectCase","00=On|01=Off"]
["Location Setting Authorization","<MANUAL>","RDELEM","01C4000100000004","SelectCase","00000000=Location On|03000000=911 Only"]
["Calling Voice Mail when Pressing \"1\"","On","RDELEM","2742000100000000","FeatureId","FeatureId=257|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Digital TTY","On","RDELEM","2742000100000000","FeatureId","FeatureId=529|IfSetDisplay=On|IfNotSetDisplay=Off"]
["EFS File System","Enabled","RDELEM","2742000100000000","FeatureId","FeatureId=728|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Header","MULTIMEDIA SETTINGS"]
["Video Length (Phone & MMC Memory)","Maximum","RDELEM","275A0001011F0001","SelectCase","00=MMS|01=Long|02=Maximum"]
["Camera Resolution","Medium","RDELEM","275A0001011C0001","SelectCase","00=Thumbnail|01=Low|02=Medium|03=High"]
["Header","EVDO Settings"]
["Phone Operation","<MANUAL>"]
["Header","######02_NAM#######################"]
["Header","NAM FIELDS"]
["Header","NAM 1"]
["Option Byte 1","10000000","RDELEM","2798000100080001","Hex2Bin"]
["Mobile Identification Number","0000000000","RDELEM","2798000100040004","CDMA1XMIN","HexIn2=2798000100020002"]
["Mobile Directory Number (Phone Number)","0000000000","RDELEM","27980001001C0005","A20"]
["Station Class Mark (SCM)",234,"RDELEM","2798000100090001","Hex2Dec","BytesPerData=1"]
["Option Byte 3","01000000","RDELEM","2797000100080001","Hex2Bin"]
["Option Byte 4","00100000","RDELEM","27970001000A0001","Hex2Bin"]
["Option Byte 5","00001111","RDELEM","27980001000D0001","Hex2Bin"]
["CDMA Slot Cycle Index",2,"RDELEM","27980001000E0001","Hex2Dec","BytesPerData=1"]
["CDMA & AMPS Home System ID (SID  1)","08832","RDELEM","27A7000100000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["CDMA Network ID (NID 1)",65535,"RDELEM","27A7000100020002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Mobile Country Code (MCC)","370","RDELEM","2798000100100002","CDMA1XMCC"]
["IMSI 12 and IMSI 11","02","RDELEM","27980001000F0001","CDMA1XIMSI12and11"]
["System Mode",1,"RDELEM","27980001001B0001","Hex2Dec","BytesPerData=1"]
["Vocoder Type","EVRC","RDELEM","2798000100240001","SelectCase","00=None|01=13K|02=EVRC"]
["CDMA Primary Ch. System A",283,"RDELEM","2798000100120002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Primary Ch. System B",384,"RDELEM","2798000100140002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System A",691,"RDELEM","2798000100160002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System B",777,"RDELEM","2798000100180002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["Header","NAM 2"]
["Option Byte 1","10000000","RDELEM","2798000200080001","Hex2Bin"]
["Mobile Identification Number","0000000000","RDELEM","2798000200040004","CDMA1XMIN","HexIn2=2798000200020002"]
["Mobile Directory Number (Phone Number)","0000000000","RDELEM","27980002001C0005","A20"]
["Station Class Mark (SCM)",234,"RDELEM","2798000200090001","Hex2Dec","BytesPerData=1"]
["Option Byte 5","00001111","RDELEM","27980002000D0001","Hex2Bin"]
["CDMA Slot Cycle Index",2,"RDELEM","27980002000E0001","Hex2Dec","BytesPerData=1"]
["CDMA & AMPS Home System ID (SID  1)","08832","RDELEM","27A7000200000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["CDMA Network ID (NID 1)",65535,"RDELEM","27A7000200020002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Mobile Country Code (MCC)","370","RDELEM","2798000200100002","CDMA1XMCC"]
["IMSI 12 and IMSI 11","02","RDELEM","27980002000F0001","CDMA1XIMSI12and11"]
["System Mode",1,"RDELEM","27980002001B0001","Hex2Dec","BytesPerData=1"]
["Vocoder Type","EVRC","RDELEM","2798000200240001","SelectCase","00=None|01=13K|02=EVRC"]
["CDMA Primary Ch. System A",283,"RDELEM","2798000200120002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Primary Ch. System B",384,"RDELEM","2798000200140002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System A",691,"RDELEM","2798000200160002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System B",777,"RDELEM","2798000200180002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["Header","OPTION BYTE 3"]
["Number of NAMs",2,"RDELEM","2760000100480001","Hex2Dec","BytesPerData=1"]
["Header","OPTION BYTE 4"]
["Long DTMF Enabled","Y","RDELEM","2742000100000000","FeatureId","FeatureId=538|IfSetDisplay=Y|IfNotSetDisplay=N"]
["Header","OPTION BYTE 5"]
["Header","NAM 1"]
["Mob Term for NID Roamer","<MANUAL>"]
["Mob Term for SID Roamer","<MANUAL>"]
["Mob Term for Home Roamer","<MANUAL>"]
["Voice Privacy","<MANUAL>"]
["Prefferred Mode","<MANUAL>"]
["Force Prefferred Vocoder","<MANUAL>"]
["Header","NAM 2"]
["Mob Term for NID Roamer","<MANUAL>"]
["Mob Term for SID Roamer","<MANUAL>"]
["Mob Term for Home Roamer","<MANUAL>"]
["Voice Privacy","<MANUAL>"]
["Prefferred Mode","<MANUAL>"]
["Force Prefferred Vocoder","<MANUAL>"]
["Header","CARRIER DEFINED PHONE NUMBERS"]
["Emergency Number 1",911,"RDELEM","2744000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Emergency Number 2","None Entered","RDELEM","2791000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Emergency Number 3","None Entered","RDELEM","2792000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Voice Mail Number","*9","RDELEM","2775000100000000","CDMA1XVoiceMailNumber"]
["Voice Portal number (VIVO feature only)","None Entered","RDELEM","29B7000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","SECURITY INFORMATION"]
["A Key  NAM1","<MANUAL>"]
["A Key  NAM2","<MANUAL>"]
["Phone Lock Code",1234,"RDELEM","2784000100000000","CDMA1XPhoneLockCode","ThenFollowsResponse=Initially 1234"]
["Subsidy Lock","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=114|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Number of Retries","<MANUAL>","RDELEM","28D5000100040004","SelectCase","FFFFFFFF=Unlimited|Else=Func:Hex2Dec|ByteSwap=True|BytesPerData=4"]
["Mobile ID Number","<MANUAL>",null,null,"CDMA1XMobileIDNumberType"]
["Header","######03_SMS-MMS#######################"]
["Header","MMS ONLY SETTINGS"]
["MMSC server URL","http://mms.verizon.net.do/servlets/mms","RDELEM","296E000100000000","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["MMSC IP Address","<MANUAL>"]
["MMSC IP port","<MANUAL>"]
["Profile URL","Profile: http://uaprof.vtext.com/mot/v3/v3v1.xml","RDELEM","29BE000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Proxy HTTP URL","None Entered","RDELEM","284D00010048008A","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Proxy HTTP IP","<MANUAL>"]
["Proxy HTTP Port","<MANUAL>"]
["Polling URL","http://mms.verizon.net.do/servlets/mms","RDELEM","296E000100000000","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","SMS ONLY SETTINGS"]
["MO SMS to Email","On","RDELEM","2742000100000000","FeatureId","FeatureId=489|IfSetDisplay=On|IfNotSetDisplay=Off"]
["MO SMS Default Entry Mode","TAP Method","RDELEM","275A0001008E0001","SelectCase","00=iTAP|01=TAP Method|02=Numeric|03=Symbol"]
["SMS to email gateway (NAM 1)",6245,"RDELEM","289D000100000011","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["SMS to email gateway (NAM 2)",6245,"RDELEM","289F000100000011","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Max # of Chars in a MO SMS",160,"RDELEM","2869000100000002","CDMA1XMaxSMSCharacters"]
["Primary Input Method for SMS","TAP (Language)","RDELEM","275A000101040001","SelectCase","00=iTAP English|01=iTAP Español|02=iTAP Português|03=TAP (Language)|04=TAP Extendido"]
["Secondary Input Method for SMS","iTAP Español","RDELEM","275A000101050001","SelectCase","FF=None|00=iTAP English|01=iTAP Español|02=iTAP Português|03=TAP (Language)|04=TAP Extendido"]
["SMS Character Support","7-Bits","RDELEM","275E000101F00004","SelectCase","02000000=7-Bits|08000000=8-Bits"]
["Delivery Report for SMS","Off","RDELEM","2742000100000000","FeatureId","FeatureId=590|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Header","######04_SUBSIDY LOCK#######################"]
["Header","MIN MATCHING TABLE"]
["Line 1","0000","RDELEM","276E000100000002","AsIs"]
["Line 2","0000","RDELEM","276E000100020002","AsIs"]
["Line 3","0000","RDELEM","276E000100040002","AsIs"]
["Line 4","0000","RDELEM","276E000100060002","AsIs"]
["Line 5","0000","RDELEM","276E000100080002","AsIs"]
["Line 6","0000","RDELEM","276E0001000A0002","AsIs"]
["Line 7","0000","RDELEM","276E0001000C0002","AsIs"]
["Line 8","0000","RDELEM","276E0001000E0002","AsIs"]
["Line 9","0000","RDELEM","276E000100100002","AsIs"]
["Line 10","0000","RDELEM","276E000100120002","AsIs"]
["Line 11","0000","RDELEM","276E000100140002","AsIs"]
["Line 12","0000","RDELEM","276E000100160002","AsIs"]
["Line 13","0000","RDELEM","276E000100180002","AsIs"]
["Line 14","0000","RDELEM","276E0001001A0002","AsIs"]
["Line 15","0000","RDELEM","276E0001001C0002","AsIs"]
["Line 16","0000","RDELEM","276E0001001E0002","AsIs"]
["Line 17","0000","RDELEM","276E000100200002","AsIs"]
["Line 18","0000","RDELEM","276E000100220002","AsIs"]
["Line 19","0000","RDELEM","276E000100240002","AsIs"]
["Line 20","0000","RDELEM","276E000100260002","AsIs"]
["Line 21","0000","RDELEM","276E000100280002","AsIs"]
["Line 22","0000","RDELEM","276E0001002A0002","AsIs"]
["Line 23","0000","RDELEM","276E0001002C0002","AsIs"]
["Line 24","0000","RDELEM","276E0001002E0002","AsIs"]
["Line 25","0000","RDELEM","276E000100300002","AsIs"]
["Header","######05_DATA CONNECTIVITY#######################"]
["Header","CDMA BROWSER SETTINGS"]
["Header","PROFILE 1",null,null,"CDMA1XWebSessions"]
["Profile Name","VZW",null,null,"GetAnswer","ANS=(Rec 1) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1","200.88.125.27",null,null,"GetAnswer","ANS=(Rec 1) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2","200.88.125.27",null,null,"GetAnswer","ANS=(Rec 1) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL","http://homepage",null,null,"GetAnswer","ANS=(Rec 1) Homepage"]
["Header","PROFILE 2",null,null,"CDMA1XWebSessions"]
["Profile Name","None Entered",null,null,"GetAnswer","ANS=(Rec 2) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1","000.000.000.000",null,null,"GetAnswer","ANS=(Rec 2) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2","000.000.000.000",null,null,"GetAnswer","ANS=(Rec 2) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL","None Entered",null,null,"GetAnswer","ANS=(Rec 2) Homepage"]
["Header","PROFILE 3",null,null,"CDMA1XWebSessions"]
["Profile Name","None Entered",null,null,"GetAnswer","ANS=(Rec 3) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1","000.000.000.000",null,null,"GetAnswer","ANS=(Rec 3) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2","000.000.000.000",null,null,"GetAnswer","ANS=(Rec 3) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL","None Entered",null,null,"GetAnswer","ANS=(Rec 3) Homepage"]
["Header","PROFILE 4",null,null,"CDMA1XWebSessions"]
["Profile Name","None Entered",null,null,"GetAnswer","ANS=(Rec 4) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1","000.000.000.000",null,null,"GetAnswer","ANS=(Rec 4) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2","000.000.000.000",null,null,"GetAnswer","ANS=(Rec 4) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL","None Entered",null,null,"GetAnswer","ANS=(Rec 4) Homepage"]
["Header","BROWSER OPTIONS"]
["Browser Enable","<MANUAL>"]
["Cache Start Up","<MANUAL>"]
["Confirmation at Start","<MANUAL>"]
["Invisible Net - Instant Messaging URL (Vivo Only)","<MANUAL>"]
["Invisible Net - Chat WAP URL (Vivo Only)","<MANUAL>"]
["Invisible Net - Email WAP URL (Vivo Only)","<MANUAL>"]
["Header","BREW SETTINGS"]
["Primary DNS","196.003.081.005","RDELEM","275E000102880004","CDMA1XBrewDnsIp"]
["Secondary DNS","196.003.081.132","RDELEM","275E0001028C0004","CDMA1XBrewDnsIp"]
["Authentication Policy","SID","RDELEM","275A000100E50001","SelectCase","00=None|01=SID|02=Text|03=Number"]
["Privacy Policy","BREW or Carrier ","RDELEM","275A000100E60001","SelectCase","00=BREW|01=Carrier|02=BREW and Carrier|03=BREW or Carrier"]
["Key Use","B-Key","RDELEM","275A000100E70001","SelectCase","00=B-Key|01=A-Key"]
["Check Prepay Option","Off","RDELEM","275A000100F30001","SelectCase","00=Off|01=On"]
["Prepaid Phone Option","Postpay","RDELEM","275A000100F20001","SelectCase","00=Postpay|01=Prepay"]
["ADS Commercial Server URL","brew.verizon.net.do ","RDELEM","2978000100000000","CDMA1XADS","IfDataIsNullDisplay=None Entered"]
["ADS Test Server URL","None Entered","RDELEM","2976000100000000","CDMA1XADS","IfDataIsNullDisplay=None Entered"]
["Carrier Id",63,"RDELEM","275E000102800004","LittleEndianHex2Dec"]
["Platform Id",8092,"RDELEM","275E000102840004","LittleEndianHex2Dec"]
["Advice of Charge in Brew","<MANUAL>"]
["Header","1X DATA CONNECTION"]
["MDR Mode","SO 33 Preferred","RDELEM","0129000100000001","SelectCase","00=MDR Only|01=MDR|02=No MDR|03=SO 33 Preferred"]
["Service Option","IS-707","RDELEM","00F1000100000001","SelectCase","00=Pre 707|01=QC Proprietary|02=IS-707"]
["Data QNC","Yes","RDELEM","00F0000100000001","SelectCase","00=No|01=Yes"]
["Data SCRM","Yes","RDELEM","01AD000100000001","SelectCase","00=No|01=Yes"]
["Primary DNS","196.3.81.5","RDELEM","01A7000100000080","CDMA1XDataConnectionDNS"]
["Secondary DNS","196.3.81.132","RDELEM","01A8000100000080","CDMA1XDataConnectionDNS"]
["Dial Up Number","<MANUAL>"]
["PAP or CHAP","CHAP","RDELEM","2742000100000000","FeatureId","FeatureId=707|IfSetDisplay=PAP|IfNotSetDisplay=CHAP"]
["Username","%M@vzdr3g.com","RDELEM","29A9000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Password","vzw","RDELEM","29BC000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["PPP Detection","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=707|IfSetDisplay=PAP|IfNotSetDisplay=CHAP"]
["Header","EVDO Data Connection"]
["PAP or CHAP","PAP","RDELEM","2742000100000000","FeatureId","FeatureId=707|IfSetDisplay=CHAP|IfNotSetDisplay=PAP"]
["Username ","%M@vzdr3g.com","RDELEM","29E9000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Password ","vzw","RDELEM","29EA000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","CSD CONNECTION",null,null,"CDMA1XWebSessions"]
["Username","<MANUAL>",null,null,"GetAnswer","ANS=(Rec 1) User Name"]
["Password","<MANUAL>",null,null,"GetAnswer","ANS=(Rec 1) Password"]
["Header","######06_AGPS#######################"]
["Header","AGPS SETTINGS"]
["PTLM Type","TCP/IP","RDELEM","275A0001015E0001","SelectCase","00=TCP/IP|01=Data Burst"]
["PTLM IP","0.0.0.0","RDELEM","275E000103A40004","CDMA1XBrewDnsIp"]
["PTLM Port",0,"RDELEM","275E000103A80004","Hex2Dec","ByteSwap=True|BytesPerData=4"]
["Header","######ENGINEERING (HIDE)#######################"]
["All SMS on Traffic Channel","Enabled","RDELEM","2742000100000000","FeatureId","FeatureId=716|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Allow New System Redial","No","RDELEM","2742000100000000","FeatureId","FeatureId=366|IfSetDisplay=No|IfNotSetDisplay=Yes"]
["BREW Test Enable","Off","RDELEM","275A000100E80001","SelectCase","00=Off|01=On"]
["Background Scan Timer",2700,"RDELEM","275E000101840004","Hex2Dec","ByteSwap=True|BytesPerData=4"]
["Re-scan on Release","Off","RDELEM","2742000100000000","FeatureId","FeatureId=974|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Video Format","H263","RDELEM","275A0001014F0001","SelectCase","00=MP4|01=H263"]
["Audio Format","AMR","RDELEM","275A000101500001","SelectCase","00=QCELP|01=AAC|02=AMR"]
["Send Key Format","Dialed/Received Calls","RDELEM","2742000100000000","FeatureId","FeatureId=781|IfSetDisplay=Dialed/Received Calls|IfNotSetDisplay=Dialed Calls"]
["Service Level","<MANUAL>"]
["WAP Connection Type","<MANUAL>"]
["User Agent Header (MMS)","User-Agent: motov3","RDELEM","29BA000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered\""]
["User Agent Header (Browser)","<MANUAL>"]
["Header","Main Menu Itens Other Settings"]
["Electronic Serial Number (ESN)","<MANUAL>"]
["Bluetooth Address (ULMA)","<MANUAL>"]
["3.1   ERI","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=534|IfSetDisplay=ON|IfNotSetDisplay=OFF"]
["List ID","<MANUAL>","RDELEM","296A000100000002","Hex2Dec","BytesPerData=2|IfThen=0"]
["File System Count","<MANUAL>"]
["Header","Security"]
["Phone Lock","<MANUAL>","RDELEM","275A0001002A0001","SelectCase","01=On|00=Off"]
["Header","Lock Application"]
["Phonebook","<MANUAL>","RDELEM","275A0001002E0001","SelectCase","00=Unlocked|01=Locked|02=View Only"]
["Recent Calls","<MANUAL>","RDELEM","275A0001002C0001","SelectCase","00=Unlocked|01=Locked"]
["Messaging","<MANUAL>","RDELEM","275A000100310001","SelectCase","00=Unlocked|01=Locked"]
[" Messages ","<MANUAL>","RDELEM","275A000100310001","SelectCase","00=Unlocked|01=Locked"]
[" Web Access ","<MANUAL>","RDELEM","275A000100000000","MultipleCases","52=00|90=00|Then=Unlocked|Else=Locked"]
["Get It Now","<MANUAL>","RDELEM","275A000100DF0001","SelectCase","00=Unlocked|01=Locked"]
["Mobile Web","<MANUAL>","RDELEM","275A000100000000","MultipleCases","52=00|90=00|Then=Unlocked|Else=Locked"]
["Web Browser","<MANUAL>","RDELEM","275A000100340001","SelectCase","00=Unlocked|01=Locked"]
[" Web Sessions ","<MANUAL>","RDELEM","275A0001005A0001","SelectCase","00=Unlocked|01=Locked"]
[" Multimedia ","<MANUAL>","RDELEM","275A000101130001","SelectCase","00=Unlocked|01=Locked"]
["Media Gallery","<MANUAL>","RDELEM","275A000101130001","SelectCase","00=Unlocked|01=Locked"]
["Settings","<MANUAL>","RDELEM","275A000100000000","MultipleCases","43=00|177=00|211=00|212=00|213=00|214=00|215=00|216=00|217=00|220=00|221=00|Then=Unlocked|Else=Locked"]
["Ring Styles","<MANUAL>","RDELEM","275A000100B10001","SelectCase","00=Unlocked|01=Locked"]
["Connection","<MANUAL>","RDELEM","275A000100D40001","SelectCase","00=Unlocked|01=Locked"]
["Tools","<MANUAL>","RDELEM","275A000100000000","MultipleCases","15=00|47=00|50=00|171=00|254=00|Then=Unlocked|Else=Locked"]
["Calculator","<MANUAL>","RDELEM","275A000100AB0001","SelectCase","00=Unlocked|01=Locked"]
["Datebook","<MANUAL>","RDELEM","275A0001002F0001","SelectCase","00=Unlocked|01=Locked"]
["Shortcuts","<MANUAL>","RDELEM","275A000100320001","SelectCase","00=Unlocked|01=Locked"]
["Voice Records","<MANUAL>","RDELEM","275A0001000F0001","SelectCase","00=Unlocked|01=Locked"]
["Alarm Clock","<MANUAL>","RDELEM","275A000100FE0001","SelectCase","00=Unlocked|01=Locked"]
["Incoming Calls to Phonebook Available","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=502|IfSetDisplay=Yes|IfNotSetDisplay=No"]
["Restrict Outgoing Calls          Allow","<MANUAL>","RDELEM","275A000100370001","SelectCase","00=None|01=All|02=Phonebook"]
["Restrict Incoming Calls          Allow","<MANUAL>","RDELEM","275A000100380001","SelectCase","00=None|01=All|02=Phonebook"]
["Header","Phonebook Setup"]
["Sort By","<MANUAL>","RDELEM","275A000100730001","SelectCase","00=Name|01=Speed Number|02=Voice Name|03=Email"]
["View","<MANUAL>","RDELEM","275A000100860001","SelectCase","00=All Contacts|01=Primary Contacts"]
["Header","Initial Setup"]
["Speaker Phone","<MANUAL>","RDELEM","275A000100AE0001","SelectCase","00=Always On|01=20 sec timeout"]
["Animation","<MANUAL>","RDELEM","275A000100080001","SelectCase","00=Off|01=On"]
["Header","NAM 1 Field and Contents"]
["AMPS Home System ID (SID)","<MANUAL>","RDELEM","2798000100000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["ACCOLC (New Programming Method)","<MANUAL>","RDELEM","27980001000C0001","Hex2Dec","BytesPerData=1|FormatLength=2"]
["Option Byte 2","<MANUAL>","RDELEM","2797000100070001","Hex2Bin"]
["True IMSI Address Number","<MANUAL>","RDELEM","2798000100250001","DisplayBits","DisplayBits=5"]
["True IMSI Status","<MANUAL>","RDELEM","2798000100250001","DisplayBits","DisplayBits=3"]
["True IMSI Prog/Deprog","<MANUAL>","RDELEM","2798000100250001","DisplayBits","DisplayBits=1"]
["True IMSI","<MANUAL>","RDELEM","2798000100280004","CDMA1XTrueIMSI","HexIn2=27980001002C0002"]
["True IMSI MCC","<MANUAL>","RDELEM","2798000100260002","CDMA1XMCC"]
["True IMSI 11 12","<MANUAL>","RDELEM","27980001002E0001","CDMA1XIMSI12and11"]
["CDMA Home System ID (SID 2)","<MANUAL>","RDELEM","27A7000100040002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["CDMA Network ID (NID 2)","<MANUAL>","RDELEM","27A7000100060002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Header","NAM 2 Field and Contents"]
["(NAM 2) AMPS Home System ID (SID)","<MANUAL>","RDELEM","2798000200000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["(NAM 2) ACCOLC (New Programming Method)","<MANUAL>","RDELEM","27980002000C0001","Hex2Dec","BytesPerData=1|FormatLength=2"]
["(NAM 2) CDMA Home System ID (SID 2)","<MANUAL>","RDELEM","27A7000200040002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["(NAM 2) CDMA Network ID (NID 2)","<MANUAL>","RDELEM","27A7000200060002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Header","Entry Setup"]
["Primary Setup","<MANUAL>","RDELEM","275A000101020001","SelectCase","00=iTAP English|01=iTAP Espanol|02=TAP Method|FF=TAP Method"]
["Secondary Setup","<MANUAL>","RDELEM","275A000101030001","SelectCase","00=iTAP English|01=iTAP Espanol|02=TAP Method|FF=None"]
["Header","Pre-Loaded Quick Notes",null,null,"CDMA1XQuickNotes","OffsetSEEM10000=TRUE|StartIndex=61"]
["Quick Note 1","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 1"]
["Quick Note 2","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 2"]
["Quick Note 3","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 3"]
["Quick Note 4","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 4"]
["Quick Note 5","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 5"]
["Quick Note 6","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 6"]
["Quick Note 7","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 7"]
["Quick Note 8","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 8"]
["Quick Note 9","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 9"]
["Quick Note 10","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 10"]
["Quick Note 11","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 11"]
["Quick Note 12","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 12"]
["Quick Note 13","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 13"]
["Quick Note 14","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 14"]
["Quick Note 15","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 15"]
["Header","MMS Settings"]
["Server Name/IP","<MANUAL>","RDELEM","299A0001003E0000","Hex2ASCII","IfDataIsNullDisplay=None Entered"]
["Server Name/IP 2","<MANUAL>","RDELEM","299A0002003C0000","Hex2ASCII","IfDataIsNullDisplay=None Entered"]
["New MM Retrieval","<MANUAL>","RDELEM","275A0001012D0001","SelectCase","00=Automatic Mode|01=Prompt Mode"]
["Retry Number","<MANUAL>","RDELEM","275E000102BC0004","Hex2Dec","ByteSwap=True|BytesPerData=4"]
["UAPROF URL","<MANUAL>","RDELEM","284D000100480000","CDMA1XUAPROFURL"]
["Album Upload Address","<MANUAL>","RDELEM","29A0000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2"]
["Read ACK","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=788|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Delivery ACK","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=787|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Header","Security Information"]
["Security Code","<MANUAL>","RDELEM","2786000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2"]
["Header","User Activation Information"]
["Allowable Attempts","<MANUAL>","RDELEM","28D5000100200004","SelectCase","FFFFFFFF=Unlimited|Else=Func:Hex2Dec|ByteSwap=True|BytesPerData=4"]
["One Time Sub Lock Status","<MANUAL>","RDELEM","28D3000100060001","CDMA1XOneTimeSubsidyLock","00=Enabled|01=Disabled"]
[" Electronic Serial Number (ESN) ","<MANUAL>","RDELEM","2789000100000008","AsIs"]
[" Factory Flex Switch ","<MANUAL>","RDELEM","2940000100000001","SelectCase","55=Factory(55)|EE=Customer(EE)"]
[" Factory Byte ","<MANUAL>","RDELEM","28D1000100000001","SelectCase","00=Out of Factory(00)|01=In Factory(01)|FF=In Factory(FF)|Else=In Factory(XX)"]
[" Bluetooth Address (ULMA) ","<MANUAL>","RDELEM","01BF000100000006","SelectCase","04=Not Programmed|else=Func:AsIs|ByteSwap=True|BytesPerData=6"]
[" File System Count ","<MANUAL>",null,null,"GetAnswer","ANS=File System Count"]
["Header","BREW Comm Server or BREW IP/URL"]
["BREW Test Enable","<MANUAL>","RDELEM","275A000100E80001","SelectCase","00=Off|01=On"]
["BREW MIN for SID","<MANUAL>","RDELEM","275A000100E90001","SelectCase","00=No|01=Yes"]
["Server Type","<MANUAL>","RDELEM","275A000100EA0001","SelectCase","00=Commercial|01=Test"]
["Header","Network"]
[" Analog Only ","<MANUAL>","RDELEM","275A0001007B0001","SelectCase","00=Off|01=On"]
["Set Mode","<MANUAL>","RDELEM","27980001001A0002","CDMA1XNetworkSetMode"]
["Service Status","<MANUAL>","RDELEM","2760000100C40001","SelectCase","00=Automatic|01=Manual"]
["Header","Engineering Settings"]
["Dynamic Websession","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=116|IfSetDisplay=On|IfNotSetDisplay=Off"]
["MMS Header Line ID","<MANUAL>","RDELEM","29BE000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["SEEM_MMS_MDN_HEADER","<MANUAL>","RDELEM","29BB000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["SEEM_MMS_BLOG_ADDRESS","<MANUAL>","RDELEM","29A0000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Use MIN for SID","<MANUAL>","RDELEM","275A000100E90001","SelectCase"," 01=MDN|01=MMC|02=MCC-MDN|03=MCC-MIN"]
["SID Encode","<MANUAL>","RDELEM","275A000101280001","SelectCase","00=Off|01=On"]
["Disallow Dormancy","<MANUAL>","RDELEM","275A000101290001","SelectCase","00=Off|01=On"]
{"$rows_empty":57}
["Available Commands","Available Functions"]
["FSAC","A20"]
["RDELEM","AsIs"]
["SBSDY_LCK","BrewBarFiles"]
["VERSION","CDMA1XBrewBarFiles"]
[null,"CDMA1XBrewDnsIp"]
[null,"CDMA1XBrowsers"]
[null,"CDMA1XDataConnectionDNS"]
[null,"CDMA1XIMSI12and11"]
[null,"CDMA1XKeys6XXX"]
[null,"CDMA1XKeysV710"]
[null,"CDMA1XMainMenuOrder"]
[null,"CDMA1XMainMenuOrder6XXX"]
[null,"CDMA1XMainMenuOrderT720"]
[null,"CDMA1XMainMenuOrderV710"]
[null,"CDMA1XMaxSMSCharacters"]
[null,"CDMA1XMCC"]
[null,"CDMA1XMessagingMenuOrder"]
[null,"CDMA1XMessagingMenuOrderV710"]
[null,"CDMA1XMIN"]
[null,"CDMA1XMobileIDNumberType"]
[null,"CDMA1XPhoneLockCode"]
[null,"CDMA1XQuickNotes"]
[null,"CDMA1XSubsidyLock"]
[null,"CDMA1XTrueIMSI"]
[null,"CDMA1XVoiceMailNumber"]
[null,"CDMA1XWebSessions"]
[null,"CDMA1XRingStyles"]
[null,"DecAndHex"]
[null,"DisplayBits"]
[null,"FeatureId"]
[null,"GetAnswer"]
[null,"Hex2ASCII"]
[null,"Hex2Bin"]
[null,"Hex2Dec"]
[null,"Languages"]
[null,"LittleEndianHex2Dec"]
[null,"MultipleCases"]
[null,"SelectCase"]