{"text_format":"5","workbook":"xls","n_sheets":5,"sheets":["01_Misc Setup","02_NAM","Template Revision History ","History list","CPV Input"],"props":{"title":"E380 PRI","creator":"Rafael Canabal","last_modified_by":"q15483","manager":"Osvaldo Meneghel","company":"Motorola"},"custom":{"_EmailSubject":"V3m - DSM Model","_AuthorEmail":"Eduardo.Iwai@motorola.com","_AuthorEmailDisplayName":"Iwai Eduardo-Q15483"},"defined_names":["_120E_Ringtones","_60X_Ringtones","_720_MENU_ORDER","_720_RING_TONES","_C33x_Ring","C343_MENU_ORDER","C343_RING_TONES","V60E_P_MENU_ORDER"],"not_rendered":{"external_links":1,"defined_names":12,"comments":24},"notes":{"written":24,"chars":3217},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"01_Misc Setup","index":0,"n_rows":10,"n_cols":10,"rows_kept":10,"merged":[[0,0,0,13],[2,0,3,1],[2,2,2,5],[2,7,2,8],[2,9,2,12],[3,2,3,5],[3,7,3,8],[3,9,3,12],[4,7,4,8],[4,9,4,12],[5,0,5,1],[5,2,5,5],[6,0,6,1],[6,2,6,5],[6,7,6,8],[6,9,6,12],[7,0,7,1],[7,2,7,5],[7,7,7,8],[7,9,7,12],[8,1,8,2],[8,4,8,5],[9,1,9,2],[9,4,9,5]],"headers":{"footer":["Motorola Confidential","","Page"]},"flags":["formulas_cached_only"]}
["DSM Model"]
[]
["T-Option/ \nSpec No:",{"$nulls":6},"PRI Version",null,3.2]
[{"$nulls":7},"PRI Date",null,"2006-11-12"]
[{"$nulls":7},"PRI Expiration Date",null,"2007-11-12"]
["Software Version",null,"NCR_01.18.00R"]
[{"v":"Monster file name","$note":[{"by":"Alexandre Araujo","t":"The file name, cannot be read through UI."}]},null,"V3MLA_01.18.00R_Movilnet_Venezuela_Monster_2006-10-17_JAGla13717.shx",{"$nulls":4},"Carrier",null,"DSM"]
[{"v":"Flex file version ","$note":[{"by":"Alexandre Araujo","t":"To check flex number, go to test mode --> Version View --> Flex Version"}]},null,"XS4MVV01V3MLA16.00R - 0.1.2",{"$nulls":4},"Country",null,"DSM"]
["PRL - NAM1","5002.prl",null,"Version",5002]
["PRL - NAM2","5002.prl",null,"Version",5002]

{"sheet":"02_NAM","index":1,"n_rows":34,"n_cols":20,"rows_kept":34,"merged":[[0,0,1,0],[0,1,0,2],[4,1,4,3],[5,1,5,3],[5,13,5,14],[6,1,6,3],[6,13,6,14],[7,1,7,3],[7,13,7,14],[8,1,8,3],[8,13,8,14],[9,1,9,3],[9,13,9,14],[10,1,10,3],[11,1,11,3],[12,1,12,3],[12,13,12,14],[13,1,13,3],[13,13,13,14],[14,1,14,3],[14,13,14,14],[15,1,15,3],[16,1,16,3],[17,1,17,3],[17,13,17,14],[18,1,18,3],[18,13,18,14],[19,1,19,3],[20,1,20,3],[21,1,21,3],[23,1,23,3],[25,1,25,3]],"headers":{"footer":["Motorola Confidential","","Page"]},"flags":["formulas_cached_only"]}
["Item 2","NAM Settings"]
[]
[]
[null,"NAM Fields",null,null,"NAM1","NAM2","How to Check Manually ?"]
["2.01",{"v":"Option Byte 1","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\nOption Byte 1:\nBit 2 => Dissallow non-Home side foreign SID in PSCAN.  True = 1; False = 0\nBit 7 => Local Use Mark.  This bit must ALWAYS be set to 1"}]},null,null,"10000000","10000000",{"$nulls":3},"Carrier Defined Phone Numbers",{"$nulls":6},"How to Check Manually ?"]
["2.02",{"v":"Mobile Identification Number","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nMIN:\nIf the MIN is not an ESN based number this value must be set to either 1111110111 OR a specific number that is desired.\nIf ESN based it must be 000000****, where **** will be based on the ESN.\n\nNOTE: Make sure you specify if it's ESN based or not in Section 8.0 \"Security Information\" under \"Mobile ID Number\"."}]},null,null,"158000XXXX","158000XXXX",null,null,"2.27","Emergency Number 1",{"$nulls":3},"*171",null,null,"Menu 0setup , 00000  Extended NAM "]
["2.03",{"v":"Mobile Directory Number (Phone Number)","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nMDN:\nMake sure the value of the MDN is the same as the MIN value."}]},null,null,"158000XXXX","158000XXXX",null,null,"2.28","Emergency Number 2",{"$nulls":3},"*1",null,null,"Menu 0setup , 00000  Extended NAM "]
["2.04",{"v":"Station Class Mark (SCM)","$note":[{"by":"batwings","t":"Motorola PC:\nNon-FLEX\n\nSCM: \nThis will have a value between 0-255 decimal. The choices are:\n  106 = CDMA 800/AMPS 800\n  160 = CDMA 1900\n  234 = CDMA Dual Band"}]},null,null,234,234,null,null,"2.29","Emergency Number 3",{"$nulls":6},"Menu 0setup , 00000  Extended NAM "]
["2.05",{"v":"Option Byte 3","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nOption Byte 3:\nbits 7 and  6 => Active NAMS \n   00 = single NAM\n   01 = dual NAM\n\nHence, the 2 options for this field are:\n\"00000000\"=> Single NAM\n\"01000000\"=> Dual NAM"}]},null,null,"01000000",{"$nulls":3},"2.30","Voice Mail Number",{"$nulls":3},"*9",null,null,"Menu, Message Center,   Message settings , voice mail"]
["2.06","Option Byte 4",null,null,"00100000",{"$nulls":3},"2.31","Voice Portal number (VIVO feature only)"]
["2.07",{"v":"Option Byte 5","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nOption Byte 5:\nBit 0=> Mob Term for NID Roamer\n   \"0\"=OFF ; \"1\" =ON;  (must be ON)\nBit 1=> Mob Term for SID Roamer\n   \"0\"=OFF ; \"1\"=ON; (must be ON)\nBit 2=> Mob Term  for Home Roamer\n   \"0\"=OFF ; \"1\"=ON (must be ON)\nBit 3=> Voice Privacy Feature\n   \"0\"= OFF ; \"1\"= ON\nBit 6 and 5=> Preferred mode.\n   If 6 = 0 and 5 = 0, => CDMA Only\n   If 6 = 0 and 5 = 1, => CDMA Preferred\n   If 6 = 1 and 5 = 0. => Analog Only\n   If 6 = 1 and 5 = 1, => CDMA Selected (Voice Privacy)\nBit 7=> Force Preferred VOCODER on Terminations\n   \"0\" = OFF; \"1\" = ON;"}]},null,null,"11101111","11101111"]
["2.08",{"v":"CDMA Slot Cycle Index","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nValid choices for Slot Cycle Index are 0-7."}]},null,null,2,2,{"$nulls":3},"Security Information"]
["2.09",{"v":"CDMA Home System ID (SID  1)","$note":[{"by":"batwings","t":"Motorola PC:\nNon-FLEX\n\nIf SID is only 4 digits, add a 0 before the SID.\n(For eg:  05205)"}]},null,null,"31488","31488","Menu 0setup , 00000  - SID/NID Pair",null,"2.32",{"v":"A Key  NAM1","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe options are:\n  Random\n  Zero"}]},{"$nulls":3},"Zero"]
["2.10","CDMA Network ID (NID 1)",null,null,65535,65535,"Menu 0setup , 00000  - SID/NID Pair",null,"2.33",{"v":"A Key  NAM2","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe options are:\n  Random\n  Zero"}]},{"$nulls":3},"Zero"]
["2.11","Mobile Country Code (MCC)",null,null,"000","000",null,null,"2.34",{"v":"Phone Lock Code","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\n4 digit lock code for locking the phone. Defaulted to \"1234\".\n"}]},{"$nulls":3},1234,null,null,"Menu 0setup , 00000  Extended NAM "]
["2.12","IMSI 12 and IMSI 11",null,null,"00","00",null,null,"2.35",{"v":"Master Subsidy lock","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe choices are:\n  -Random => Type \"Random\"\n  -Fixed => Type in the value of the fixed password that will be used.\n  -Zero (None) => Type \"Zero\"\n"}]},{"$nulls":3},"Zero",{"$note":[{"by":"wed014","t":"If fixed the Password should be field here"}]}]
["2.13",{"v":"System Mode","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nSystem Mode:\n0 - Home Only\n1 - Standard Scan\n2 - ScanA\n3 - ScanB\n4 - Automatic A (Verizon only feature)\n5 - Automatic B (Verizon only feature)"}]},null,null,1,1,null,null,"2.36",{"v":"One-time Subsidy lock","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nThe choices are:\n  -Random => Type \"Random\"\n  -Fixed => Type in the value of the fixed password that will be used.\n  -Zero (None) => NOT SUPPORTED !!!\n"}]},{"$nulls":3},"Zero",{"$note":[{"by":"wed014","t":"If fixed the Password should be field here"}]}]
["2.14",{"v":"Vocoder Type","$note":[{"by":"batwings","t":"Motorola PCS:\nNon-FLEX\n\nThe regular 8K option is not available for 1X phones. Hence the only options for this field are \"Yes\" or \"No\".\n"}]},null,null,"EVRC","EVRC",null,null,"2.37","Number of Retries",{"$nulls":3},10]
["2.15","CDMA Primary Ch. System A",null,null,283,283,"Menu 0setup , 00000  Extended NAM ",null,"2.38",{"v":"Mobile ID Number","$note":[{"by":"batwings","t":"Motorola PCS:\nFACTORY\nESN Based\nNone\n"}]},{"$nulls":3},"ESN BASED"]
["2.16","CDMA Primary Ch. System B",null,null,384,384,"Menu 0setup , 00000  Extended NAM "]
["2.17","CDMA Secondary Ch. System A",null,null,691,691,"Menu 0setup , 00000  Extended NAM ",null,null,"MIN Matching Check",null,"NAM1","NAM2"]
["2.18","CDMA Secondary Ch. System B",null,null,777,777,"Menu 0setup , 00000  Extended NAM ",null,"2.39","NAM"]
[{"$nulls":8},"2.40","MDN"]
[null,"Option Byte 3"]
["2.19","Number of NAMs",null,null,2]
[null,"Option Byte 4"]
["2.20","Menu DTMF Enabled",null,null,"Y"]
[null,"Option Byte 5",null,null,"NAM1","NAM2",{"$nulls":11},"CDMA Preferred","CDMA Only","CDMA Selected (Voice Privacy)"]
["2.21","Mob Term for NID Roamer",null,null,"Y","Y"]
["2.22","Mob Term for SID Roamer",null,null,"Y","Y"]
["2.23","Mob Term for Home Roamer",null,null,"Y","Y"]
["2.24","Voice Privacy",null,null,"Y","Y"]
["2.25","Prefferred Mode",null,null,"CDMA Selected (Voice Privacy)","CDMA Selected (Voice Privacy)"]
["2.26","Force Prefferred Vocoder",null,null,"Y","Y"]

{"sheet":"Template Revision History ","index":2,"n_rows":55,"n_cols":7,"rows_kept":55,"hidden":true,"merged":[[0,0,1,0],[0,1,0,6],[1,1,1,3],[1,4,1,5],[1,7,1,10],[5,5,5,6],[6,5,6,6],[7,5,7,6],[8,5,8,6],[9,5,9,6],[10,5,10,6]],"flags":["formulas_cached_only"]}
["Item 9","History List"]
[]
["Version","Date",{"v":"Owner Name","$note":[{"t":"Administrator:\nWho is executing the change."}]},"Description of Change",{"v":"Item #","$note":[{"t":"Administrator:\nSee number in the PRI Spreadsheet, i.e.:\n4.0.17 (NAM File loc17); 5.0 (Need the field Name);...\n\n"}]},"Field Name"]
["1.0","2005-09-13","Evandro Dalben","Initial Release based on E815 v2.1 CPV"]
["1.1","2005-09-26","Evandro Dalben","CPV Mapping corrected by Eldorado"]
["2.0","2005-10-31","Evandro Dalben","Added new feature","1.43","Browser Splash Screen Picture"]
["2.0","2005-10-31","Evandro Dalben","Moved to Misc_Setup","1.44","Browser Splash Screen"]
["2.0","2005-10-31","Evandro Dalben","Added new feature","1.47","Transfer files"]
["2.0","2005-10-31","Evandro Dalben","Added new feature","3.16","Delivery Report for SMS"]
["2.0","2005-10-31","Evandro Dalben","Added new feature",5.26,"Advice of Charge in Brew"]
["2.1","2005-11-03","Evandro Dalben","Added new feature","2.37","Number of Retries"]
["2.2","2005-12-20","Evandro Dalben","Options and Description","1.42","Wake Up Greeting Editable"," Enabled/Disabled"]
["2.2","2005-12-20","Evandro Dalben","Options and Description","1.47","Location Setting"," On/Off"]
["2.2","2005-12-20","Evandro Dalben","Description","1.46","External Display"," Description"]
["2.2","2005-12-20","Evandro Dalben","Description","1.42","Wake Up Greeting Overwrite"," Description"]
["2.2","2005-12-20","Evandro Dalben","Description","1.54","Phone Operation"]
["2.2","2005-12-20","Evandro Dalben","Options","1.39","Wake Up Greeting Enabled","Enabled;Disabled"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","1.4x","Location Setting Authorization"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","3.01","MMSC server URL"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","2.14","Vocoder Type"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","5.34 / 5.37","PAP or CHAP"]
["2.3","2006-02-23","Rodrigo Pescio","CPV Sheet","5.40 / 5.41","CSD Connection"]
["2.4","2006-03-08","Rodrigo Pescio","Updated description","3.10","MO SMS default entry mode"]
["2.5","2006-03-20","Evandro Dalben","CPV Sheet (Removed option)",null,"Dysplay File System Files"]
["2.6","2006-04-26","Thiago Couto","New options added","1.36","Auto answer (Headset and Car settings)"]
["2.6","2006-04-26","Thiago Couto","\"Invalid Entry\" form correction","5.39","Password"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","7.12","User Agent Header (MMS)"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.01","MMSC server URL"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.05","Proxy HTTP URL"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.08","Polling URL"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.11","SMS to email gateway (NAM 1)"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","3.11","SMS to email gateway (NAM 2)"]
["2.6","2006-04-26","Thiago Couto","CPV Input fuction correction","7.04","Background Scan Timer"]
["2.7","2006-05-11","Thiago Santos","New values added (Random1 and Random2)","5.36 and 5.39","Password"]
["2.8","2006-07-03","Rodrigo Pescio","Hexin values changed","CPV Input"]
["2.9","2006-07-07","Thiago Santos","Voice Dial (Headset) added","1.50","Voice Dial (Headset)"]
["3.0","2006-07-10","Rodrigo Pescio","CPV Input fuctions corrections","CPV Input","Voice Dial (Headset e Bluetooh), Long DTMF Enabled, Subsidy Lock, MIN, MDN, Profile URL, Proxy HTTP URL, Wallpaper, Screensaver"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Current Language"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Wake Up Greeting Enable"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Carrier Wakeup Greeting"]
["3.1","2006-10-19","Thiago Santos","Added","CPV Input","External Display"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Transfer Files"]
["3.1","2006-10-19","Thiago Santos","Definition corrected","2.20","Menu DTMF Enabled"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Profile URL"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Proxy HTTP URL"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","MO SMS Default Entry Mode"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Primary DNS"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Secondary DNS"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Primary DNS"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Secondary DNS"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Username"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Password"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Username"]
["3.1","2006-10-19","Thiago Santos","CPV Input fuction correction","CPV Input","Audio Format"]
["3.2","2006-11-10","Thiago Santos","Sheet creation",7,"MIP Parameters"]

{"sheet":"History list","index":3,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[0,0,0,6],[1,0,1,2],[1,3,1,4],[1,5,1,6],[1,7,1,12]],"flags":["formulas_cached_only"]}
["History List"]
[]
["Date",{"v":"Owner Name","$note":[{"t":"Administrator:\nWho is executing the change."}]},{"v":"Item #","$note":[{"t":"Administrator:\nSee number in the PRI Spreadsheet, i.e.:\n4.0.17 (NAM File loc17); 5.0 (Need the field Name);...\n\n"}]},"Field Name","Old Field Value","New Field Value","Version"]
["2006-11-12","Juan Sosa","All","NA","NA","Initial Creation",{"v":3.2,"d":"3.20"}]

{"sheet":"CPV Input","index":4,"n_rows":522,"n_cols":6,"rows_kept":522,"hidden":true,"flags":["formulas_cached_only"]}
["CUSTOMER ITEM","VALUE","COMMAND","HEXIN","FUNCTION","TOKEN STRING"]
["DEFINE_MA","CDMA1X6500"]
["DEFINE_MODEL","V3CB"]
["Header","######01_MISC SETUP#######################"]
["Header","PHONE STATUS"]
["Software Version","NCR_01.18.00R","VERSION","FFFF","Hex2ASCII","StartByte=5"]
["Flex File","XS4MVV01V3MLA16.00R - 0.1.2","RDELEM","288F00010000001B","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["PRL - NAM1 (Version)",5002,"RDELEM","0101000100010002","Hex2Dec","ByteSwap=True|BytesPerData=2"]
["PRL - NAM2 (Version)",5002,"RDELEM","0101000200010002","Hex2Dec","ByteSwap=True|BytesPerData=2"]
["Header","RINGSTYLES",null,null,"CDMA1XRingStyles"]
["Style",{"$error":"#REF!"},"RDELEM","275A0001000A0001","SelectCase","00=Loud|01=Soft|02=Vibrate|03=Vibe&Ring|04=Silent"]
[" DEFINE_RINGTONES ","00=Continental|01=Classic|03=Acoustica|3B=Alert|14=Jitters|06=Bells|26=Bits & Bytes|2E=Cosmic|28=Ding|27=Door Bell|15=Upbeat|18=Expose|16=Expresso|17=Flare|08=Glacier|09=Guitar Strings|2B=Harmonics|0A=High Impact|0B=High Tide|0C=Higher Plane|2C=Interlude|12=Jubilation|11=Kaleidoscope|0D=Luna|0E=Mania|10=Moonlit Haze|0F=Nightlife|29=One Moment|2A=Provincial|25=Random|1A=Silent|2D=Snaggle|05=Standard|2F=Gyroscope|54=Triads|13=Up and Down|1C=Vibe Dash|1E=Vibe Dot Dash|1D=Vibe Dot Dot|1B=Vibe Dot|1F=Vibe Pulse|58=Wind Chime|30=Sweet|31=Chimes high|32=Chimes low|33=Ding|34=TaDa|35=Notify|36=Drum|37=Claps|38=Fanfare|39=Chord high|3A=Chord low|04=Ambient|3C=Dynamic|3D=Energize|3E=High Impact|3F=Moonlit Haze|48=Hello Moto|41=Passion|42=Power Surge|43=This Is Techno|44=Motion|4C=Velvet"]
["Calls","<MANUAL>",null,null,"GetAnswer","ANS=Calls"]
["Inbox","<MANUAL>",null,null,"GetAnswer","ANS=Inbox"]
["Voicemail","<MANUAL>",null,null,"GetAnswer","ANS=Voicemail"]
["Alarms","<MANUAL>",null,null,"GetAnswer","ANS=Alarms"]
["Data Calls","<MANUAL>",null,null,"GetAnswer","ANS=Data Calls"]
["Fax Calls","<MANUAL>",null,null,"GetAnswer","ANS=Fax Calls"]
["Ringer IDs",{"$error":"#REF!"},"RDELEM",{"$error":"#REF!"},"SelectCase","00=Off|01=On"]
["Reminders","<MANUAL>",null,null,"GetAnswer","ANS=Reminders"]
["Ringer Volume","<MANUAL>",null,null,"GetAnswer","ANS=Ringer Volume"]
["Key Volume","<MANUAL>",null,null,"GetAnswer","ANS=Key Volume"]
["Header","PERSONALIZE",null,null,"CDMA1XKeys6XXX"]
["Home Screen/Home Keys/Icons",{"$error":"#REF!"},"RDELEM","275A000101120001","SelectCase","00=Hide|01=Show|02=2 Clicks"]
[" DEFINE_SOFTKEYS ","PhoneBook=CONTACTS|RecentCall=Recent Calls|Message=Message Center|GetItNow=Get It Now|Browser=Browser|WebAccess=Mobile Web|Mutilmedia=Media Gallery|Settings=Settings|Tools=Tools|PhoneStatus=Phone Info|Shortcuts=Shortcuts|VoiceRecord=Voice Record"]
["Home Screen/Home Keys/Up",{"$error":"#REF!"},null,null,"GetAnswer","ANS=Scroll Up"]
["Home Screen/Home Keys/Down",{"$error":"#REF!"},null,null,"GetAnswer","ANS=Scroll Down"]
["Home Screen/Home Keys/Left",{"$error":"#REF!"},null,null,"GetAnswer","ANS=Scroll Left"]
["Home Screen/Home Keys/Right",{"$error":"#REF!"},null,null,"GetAnswer","ANS=Scroll Right"]
["Home Screen/Home Keys/Left Soft Key",{"$error":"#REF!"},null,null,"GetAnswer","ANS=Left Soft Key"]
["Home Screen/Home Keys/Right Soft Key",{"$error":"#REF!"},null,null,"GetAnswer","ANS=Right Soft Key"]
["Home Screen/Layout",{"$error":"#REF!"},"RDELEM","275A000101100001","SelectCase","00=Left Justified|01=Centered"]
["Banner Enabled","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=391|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Home ScreenBanner",{"$error":"#REF!"},"RDELEM","2773000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Home Screen/Clock",{"$error":"#REF!"},"RDELEM","275A000101110001","SelectCase","00=Digital|01=Analog"]
["Main Menu/View",{"$error":"#REF!"},"RDELEM","275A000100BE0001","SelectCase","00=Icons|01=List"]
["Wallpaper/Picture","<MANUAL>","RDELEM","2947000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Wallpaper",{"$error":"#REF!"},"RDELEM","275A000100BA0001","SelectCase","00=Center|01=Tile|02=Fit-to-screen"]
["Screensaver/Picture","<MANUAL>","RDELEM","293D000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Screensaver/Delay",{"$error":"#REF!"},"RDELEM","275A000100B90001","SelectCase","00=Off|01=1 minute|02=2 minutes|03= 5 minutes|04=10 minutes"]
["Skinning",{"$error":"#REF!"},"RDELEM","29CB000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","IN-CALL-SETUP"]
["Time Format",{"$error":"#REF!"},"RDELEM","275A000100010001","SelectCase","00=12 hour|01=24 hour"]
["Date Format",{"$error":"#REF!"},"RDELEM","275A000100000001","SelectCase","00=12/31/99|01=31/12/99|02=31-DEC-1999"]
["Auto Redial",{"$error":"#REF!"},"RDELEM","275A000100030001","SelectCase","00=Off|01=On"]
["Display Timeout",{"$error":"#REF!"},"RDELEM","275A0001010E0001","SelectCase","00=Off|01=1 minute|02=2 minutes|03=5 minutes|04=10 minutes"]
["Backlight",{"$error":"#REF!"},"RDELEM","275A000100040001","SelectCase","00=Off|01=5 seconds|02=10 seconds|03=20 seconds|04=30 seconds|05=50 seconds"]
["TTY Setup","<MANUAL>","RDELEM","275A000100AF0001","SelectCase","00=Voice|01=TTY|02=VCO|03=HCO"]
["Menu Scroll",{"$error":"#REF!"},"RDELEM","275A000100070001","SelectCase","00=Up/Down|01=Wrap Around"]
["Current Language",{"$error":"#REF!"},"RDELEM","275E000101440001","Languages","0E=Español|01=English|2A=Português"]
["DTMF",{"$error":"#REF!"},"RDELEM","275A000100450001","SelectCase","00=Off|01=Short|02=Long"]
["Open to Answer",{"$error":"#REF!"},"RDELEM","275A000100140001","SelectCase","00=Off|01=On"]
["Multi Key Answer",{"$error":"#REF!"},"RDELEM","275A000100130001","SelectCase","01=On|00=Off"]
["Auto Answer (Headset and Car Settings)",{"$error":"#REF!"},"RDELEM","275A000100520001","SelectCase","00=Off|01=On|02=2 seconds|05=5 seconds|0A=10 seconds"]
["Auto Handsfree",{"$error":"#REF!"},"RDELEM","275A000100460001","SelectCase","00=Off|01=On"]
["Auto Display Hyphens",{"$error":"#REF!"},"RDELEM","275A000101320001","SelectCase","00=Off|01=On|02=Auto"]
["Wake Up Greeting Enable",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=392|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Carrier Wakeup Banner","<MANUAL>"]
["Carrier Wakeup Greeting",{"$error":"#REF!"},"RDELEM","284A000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Greeting Editable","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=392|IfSetDisplay=On|IfNotSetDisplay=Off"]
["External Display","<MANUAL>","RDELEM","2771000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2"]
["Browser Splash Screen Picture","<MANUAL>"]
["Browser Splash Screen","<MANUAL>"]
["Time/Date Autoupdate","<MANUAL>","RDELEM","275A0001003C0001","SelectCase","00=Off|01=On"]
["Header","BLUETOOTH SETUP"]
["Power",{"$error":"#REF!"},"RDELEM","275A0001004E0001","SelectCase","00=Off|01=On"]
["Voice Dial (Bluetooth)",{"$error":"#REF!"},"RDELEM","275A000101340001","SelectCase","00=Off|01=On"]
["Transfer Files",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=942|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Header","OTHER SETTINGS"]
["Location Setting",{"$error":"#REF!"},"RDELEM","275A0001015F0001","SelectCase","00=On|01=Off"]
["Location Setting Authorization","<MANUAL>","RDELEM","01C4000100000004","SelectCase","00000000=Location On|03000000=911 Only"]
["Calling Voice Mail when Pressing \"1\"",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=257|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Voice Dial (Headset)",{"$error":"#REF!"},"RDELEM","275A000100720001","SelectCase","00=Off|01=On"]
["Digital TTY",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=529|IfSetDisplay=On|IfNotSetDisplay=Off"]
["EFS File System",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=728|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Header","MULTIMEDIA SETTINGS"]
["Video Length (Phone & MMC Memory)",{"$error":"#REF!"},"RDELEM","275A0001011F0001","SelectCase","00=MMS|01=Long|02=Maximum"]
["Camera Resolution",{"$error":"#REF!"},"RDELEM","275A0001011C0001","SelectCase","00=Thumbnail|01=Low|02=Medium|03=High"]
["Header","EVDO Settings"]
["Phone Operation","<MANUAL>"]
["Header","######02_NAM#######################"]
["Header","NAM FIELDS"]
["Header","NAM 1"]
["Option Byte 1","10000000","RDELEM","2798000100080001","Hex2Bin"]
["Mobile Identification Number","158000XXXX","RDELEM","2798000100040004","CDMA1XMIN","HexIn2=2798000100020002"]
["Mobile Directory Number (Phone Number)","158000XXXX","RDELEM","27980001001C0005","A20"]
["Station Class Mark (SCM)",234,"RDELEM","2798000100090001","Hex2Dec","BytesPerData=1"]
["Option Byte 3","01000000","RDELEM","2797000100080001","Hex2Bin"]
["Option Byte 4","00100000","RDELEM","27970001000A0001","Hex2Bin"]
["Option Byte 5","11101111","RDELEM","27980001000D0001","Hex2Bin"]
["CDMA Slot Cycle Index",2,"RDELEM","27980001000E0001","Hex2Dec","BytesPerData=1"]
["CDMA & AMPS Home System ID (SID  1)","31488","RDELEM","27A7000100000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["CDMA Network ID (NID 1)",65535,"RDELEM","27A7000100020002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Mobile Country Code (MCC)","000","RDELEM","2798000100100002","CDMA1XMCC"]
["IMSI 12 and IMSI 11","00","RDELEM","27980001000F0001","CDMA1XIMSI12and11"]
["System Mode",1,"RDELEM","27980001001B0001","Hex2Dec","BytesPerData=1"]
["Vocoder Type","EVRC","RDELEM","2798000100240001","SelectCase","00=None|01=13K|02=EVRC"]
["CDMA Primary Ch. System A",283,"RDELEM","2798000100120002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Primary Ch. System B",384,"RDELEM","2798000100140002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System A",691,"RDELEM","2798000100160002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System B",777,"RDELEM","2798000100180002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["Header","NAM 2"]
["Option Byte 1","10000000","RDELEM","2798000200080001","Hex2Bin"]
["Mobile Identification Number","158000XXXX","RDELEM","2798000200040004","CDMA1XMIN","HexIn2=2798000200020002"]
["Mobile Directory Number (Phone Number)","158000XXXX","RDELEM","27980002001C0005","A20"]
["Station Class Mark (SCM)",234,"RDELEM","2798000200090001","Hex2Dec","BytesPerData=1"]
["Option Byte 5","11101111","RDELEM","27980002000D0001","Hex2Bin"]
["CDMA Slot Cycle Index",2,"RDELEM","27980002000E0001","Hex2Dec","BytesPerData=1"]
["CDMA & AMPS Home System ID (SID  1)","31488","RDELEM","27A7000200000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["CDMA Network ID (NID 1)",65535,"RDELEM","27A7000200020002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Mobile Country Code (MCC)","000","RDELEM","2798000200100002","CDMA1XMCC"]
["IMSI 12 and IMSI 11","00","RDELEM","27980002000F0001","CDMA1XIMSI12and11"]
["System Mode",1,"RDELEM","27980002001B0001","Hex2Dec","BytesPerData=1"]
["Vocoder Type","EVRC","RDELEM","2798000200240001","SelectCase","00=None|01=13K|02=EVRC"]
["CDMA Primary Ch. System A",283,"RDELEM","2798000200120002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Primary Ch. System B",384,"RDELEM","2798000200140002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System A",691,"RDELEM","2798000200160002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["CDMA Secondary Ch. System B",777,"RDELEM","2798000200180002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=4"]
["Header","OPTION BYTE 3"]
["Number of NAMs",2,"RDELEM","2760000100480001","Hex2Dec","BytesPerData=1"]
["Header","OPTION BYTE 4"]
["Long DTMF Enabled","Y","RDELEM","2742000100000000","FeatureId","FeatureId=538|IfSetDisplay=Y|IfNotSetDisplay=N"]
["Header","OPTION BYTE 5"]
["Header","NAM 1"]
["Mob Term for NID Roamer","<MANUAL>"]
["Mob Term for SID Roamer","<MANUAL>"]
["Mob Term for Home Roamer","<MANUAL>"]
["Voice Privacy","<MANUAL>"]
["Prefferred Mode","<MANUAL>"]
["Force Prefferred Vocoder","<MANUAL>"]
["Header","NAM 2"]
["Mob Term for NID Roamer","<MANUAL>"]
["Mob Term for SID Roamer","<MANUAL>"]
["Mob Term for Home Roamer","<MANUAL>"]
["Voice Privacy","<MANUAL>"]
["Prefferred Mode","<MANUAL>"]
["Force Prefferred Vocoder","<MANUAL>"]
["Header","CARRIER DEFINED PHONE NUMBERS"]
["Emergency Number 1","*171","RDELEM","2744000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Emergency Number 2","*1","RDELEM","2791000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Emergency Number 3","None Entered","RDELEM","2792000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Voice Mail Number","*9","RDELEM","2775000100000000","CDMA1XVoiceMailNumber"]
["Voice Portal number (VIVO feature only)","None Entered","RDELEM","29B7000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","SECURITY INFORMATION"]
["A Key  NAM1","<MANUAL>"]
["A Key  NAM2","<MANUAL>"]
["Phone Lock Code",1234,"RDELEM","2784000100000000","CDMA1XPhoneLockCode","ThenFollowsResponse=Initially 1234"]
["Subsidy Lock","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=114|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Number of Retries","<MANUAL>","RDELEM","28D5000100040004","SelectCase","FFFFFFFF=Unlimited|Else=Func:Hex2Dec|ByteSwap=True|BytesPerData=4"]
["Mobile ID Number","<MANUAL>",null,null,"CDMA1XMobileIDNumberType"]
["Header","######03_SMS-MMS#######################"]
["Header","MMS ONLY SETTINGS"]
["MMSC server URL",{"$error":"#REF!"},"RDELEM","296E000100000000","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["MMSC IP Address","<MANUAL>"]
["MMSC IP port","<MANUAL>"]
["Profile URL",{"$error":"#REF!"},"RDELEM","29BE000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2|IfDataIsNullDisplay=None Entered"]
["Proxy HTTP URL",{"$error":"#REF!"},"RDELEM","284D00010048008A","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Proxy HTTP IP","<MANUAL>"]
["Proxy HTTP Port","<MANUAL>"]
["Polling URL",{"$error":"#REF!"},"RDELEM","296E000100000000","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","SMS ONLY SETTINGS"]
["MO SMS to Email",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=489|IfSetDisplay=On|IfNotSetDisplay=Off"]
["MO SMS Default Entry Mode",{"$error":"#REF!"},"RDELEM","275A0001008E0001","SelectCase","00=iTAP|01=TAP Method|02=Numeric|03=Symbol"]
["SMS to email gateway (NAM 1)",{"$error":"#REF!"},"RDELEM","289D000100000011","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["SMS to email gateway (NAM 2)",{"$error":"#REF!"},"RDELEM","289F000100000011","Hex2ASCII","BytesPerData=1|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Max # of Chars in a MO SMS",{"$error":"#REF!"},"RDELEM","2869000100000002","CDMA1XMaxSMSCharacters"]
["Primary Input Method for SMS",{"$error":"#REF!"},"RDELEM","275A000101040001","SelectCase","00=iTAP English|01=iTAP Español|02=iTAP Português|03=TAP (Language)|04=TAP Extendido"]
["Secondary Input Method for SMS",{"$error":"#REF!"},"RDELEM","275A000101050001","SelectCase","FF=None|00=iTAP English|01=iTAP Español|02=iTAP Português|03=TAP (Language)|04=TAP Extendido"]
["SMS Character Support",{"$error":"#REF!"},"RDELEM","275E000101F00004","SelectCase","02000000=7-Bits|08000000=8-Bits"]
["Delivery Report for SMS",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=590|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Header","######04_SUBSIDY LOCK#######################"]
["Header","MIN MATCHING TABLE"]
["Line 1",{"$error":"#REF!"},"RDELEM","276E000100000002","AsIs"]
["Line 2",{"$error":"#REF!"},"RDELEM","276E000100020002","AsIs"]
["Line 3",{"$error":"#REF!"},"RDELEM","276E000100040002","AsIs"]
["Line 4",{"$error":"#REF!"},"RDELEM","276E000100060002","AsIs"]
["Line 5",{"$error":"#REF!"},"RDELEM","276E000100080002","AsIs"]
["Line 6",{"$error":"#REF!"},"RDELEM","276E0001000A0002","AsIs"]
["Line 7",{"$error":"#REF!"},"RDELEM","276E0001000C0002","AsIs"]
["Line 8",{"$error":"#REF!"},"RDELEM","276E0001000E0002","AsIs"]
["Line 9",{"$error":"#REF!"},"RDELEM","276E000100100002","AsIs"]
["Line 10",{"$error":"#REF!"},"RDELEM","276E000100120002","AsIs"]
["Line 11",{"$error":"#REF!"},"RDELEM","276E000100140002","AsIs"]
["Line 12",{"$error":"#REF!"},"RDELEM","276E000100160002","AsIs"]
["Line 13",{"$error":"#REF!"},"RDELEM","276E000100180002","AsIs"]
["Line 14",{"$error":"#REF!"},"RDELEM","276E0001001A0002","AsIs"]
["Line 15",{"$error":"#REF!"},"RDELEM","276E0001001C0002","AsIs"]
["Line 16",{"$error":"#REF!"},"RDELEM","276E0001001E0002","AsIs"]
["Line 17",{"$error":"#REF!"},"RDELEM","276E000100200002","AsIs"]
["Line 18",{"$error":"#REF!"},"RDELEM","276E000100220002","AsIs"]
["Line 19",{"$error":"#REF!"},"RDELEM","276E000100240002","AsIs"]
["Line 20",{"$error":"#REF!"},"RDELEM","276E000100260002","AsIs"]
["Line 21",{"$error":"#REF!"},"RDELEM","276E000100280002","AsIs"]
["Line 22",{"$error":"#REF!"},"RDELEM","276E0001002A0002","AsIs"]
["Line 23",{"$error":"#REF!"},"RDELEM","276E0001002C0002","AsIs"]
["Line 24",{"$error":"#REF!"},"RDELEM","276E0001002E0002","AsIs"]
["Line 25",{"$error":"#REF!"},"RDELEM","276E000100300002","AsIs"]
["Header","######05_DATA CONNECTIVITY#######################"]
["Header","CDMA BROWSER SETTINGS"]
["Header","PROFILE 1",null,null,"CDMA1XWebSessions"]
["Profile Name",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 1) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 1) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 1) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 1) Homepage"]
["Header","PROFILE 2",null,null,"CDMA1XWebSessions"]
["Profile Name",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 2) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 2) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 2) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 2) Homepage"]
["Header","PROFILE 3",null,null,"CDMA1XWebSessions"]
["Profile Name",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 3) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 3) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 3) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 3) Homepage"]
["Header","PROFILE 4",null,null,"CDMA1XWebSessions"]
["Profile Name",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 4) Proxy Name"]
["Edit Rights","<MANUAL>"]
["WAP IP 1",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 4) Primary Proxy IP Address"]
["WAP Port 1","<MANUAL>"]
["WAP IP 2",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 4) Secondary Proxy IP Address"]
["WAP Port 2","<MANUAL>"]
["Timeout (Linger Time)","<MANUAL>"]
["Default Home Page URL",{"$error":"#REF!"},null,null,"GetAnswer","ANS=(Rec 4) Homepage"]
["Header","BROWSER OPTIONS"]
["Browser Enable","<MANUAL>"]
["Cache Start Up","<MANUAL>"]
["Confirmation at Start","<MANUAL>"]
["Invisible Net - Instant Messaging URL (Vivo Only)","<MANUAL>"]
["Invisible Net - Chat WAP URL (Vivo Only)","<MANUAL>"]
["Invisible Net - Email WAP URL (Vivo Only)","<MANUAL>"]
["Header","BREW SETTINGS"]
["Primary DNS",{"$error":"#REF!"},"RDELEM","275E000102880004","CDMA1XBrewDnsIp","Format=000.000.000.000|PF_FUNC=IPTemplate"]
["Secondary DNS",{"$error":"#REF!"},"RDELEM","275E0001028C0004","CDMA1XBrewDnsIp","Format=000.000.000.000|PF_FUNC=IPTemplate"]
["Authentication Policy",{"$error":"#REF!"},"RDELEM","275A000100E50001","SelectCase","00=None|01=SID|02=Text|03=Number"]
["Privacy Policy",{"$error":"#REF!"},"RDELEM","275A000100E60001","SelectCase","00=BREW|01=Carrier|02=BREW and Carrier|03=BREW or Carrier"]
["Key Use",{"$error":"#REF!"},"RDELEM","275A000100E70001","SelectCase","00=B-Key|01=A-Key"]
["Check Prepay Option",{"$error":"#REF!"},"RDELEM","275A000100F30001","SelectCase","00=Off|01=On"]
["Prepaid Phone Option",{"$error":"#REF!"},"RDELEM","275A000100F20001","SelectCase","00=Postpay|01=Prepay"]
["ADS Commercial Server URL",{"$error":"#REF!"},"RDELEM","2978000100000000","CDMA1XADS","IfDataIsNullDisplay=None Entered"]
["ADS Test Server URL",{"$error":"#REF!"},"RDELEM","2976000100000000","CDMA1XADS","IfDataIsNullDisplay=None Entered"]
["Carrier Id",{"$error":"#REF!"},"RDELEM","275E000102800004","LittleEndianHex2Dec"]
["Platform Id",{"$error":"#REF!"},"RDELEM","275E000102840004","LittleEndianHex2Dec"]
["Advice of Charge in Brew","<MANUAL>"]
["Header","1X DATA CONNECTION"]
["MDR Mode",{"$error":"#REF!"},"RDELEM","0129000100000001","SelectCase","00=MDR Only|01=MDR|02=No MDR|03=SO 33 Preferred"]
["Service Option",{"$error":"#REF!"},"RDELEM","00F1000100000001","SelectCase","00=Pre 707|01=QC Proprietary|02=IS-707"]
["Data QNC",{"$error":"#REF!"},"RDELEM","00F0000100000001","SelectCase","00=No|01=Yes"]
["Data SCRM",{"$error":"#REF!"},"RDELEM","01AD000100000001","SelectCase","00=No|01=Yes"]
["Primary DNS",{"$error":"#REF!"},"RDELEM","01A7000100000080","CDMA1XDataConnectionDNS","Format=000.000.000.000|PF_FUNC=IPTemplate"]
["Secondary DNS",{"$error":"#REF!"},"RDELEM","01A8000100000080","CDMA1XDataConnectionDNS","Format=000.000.000.000|PF_FUNC=IPTemplate"]
["Dial Up Number","<MANUAL>"]
["PAP or CHAP",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=707|IfSetDisplay=PAP|IfNotSetDisplay=CHAP"]
["Username",{"$error":"#REF!"},"RDELEM","29A9000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Password",{"$error":"#REF!"},"RDELEM","29BC000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["PPP Detection","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=707|IfSetDisplay=PAP|IfNotSetDisplay=CHAP"]
["Header","EVDO Data Connection"]
["PAP or CHAP",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=707|IfSetDisplay=CHAP|IfNotSetDisplay=PAP"]
["Username ",{"$error":"#REF!"},"RDELEM","29E9000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Password ",{"$error":"#REF!"},"RDELEM","29EA000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Header","CSD CONNECTION",null,null,"CDMA1XWebSessions"]
["Username","<MANUAL>",null,null,"GetAnswer","ANS=(Rec 1) User Name"]
["Password","<MANUAL>",null,null,"GetAnswer","ANS=(Rec 1) Password"]
["Header","######06_AGPS#######################"]
["Header","AGPS SETTINGS"]
["PTLM Type",{"$error":"#REF!"},"RDELEM","275A0001015E0001","SelectCase","00=TCP/IP|01=Data Burst"]
["PTLM IP",{"$error":"#REF!"},"RDELEM","275E000103A40004","CDMA1XBrewDnsIp"]
["PTLM Port",{"$error":"#REF!"},"RDELEM","275E000103A80004","Hex2Dec","ByteSwap=True|BytesPerData=4"]
["Header","######07_MIP Parameters#######################"]
["MIP Enabled","<MANUAL>"]
["NAI","<MANUAL>"]
["Tethered NAI","<MANUAL>"]
["IP Mode","<MANUAL>"]
["MN HA SS","<MANUAL>"]
["Set MN HA SPI","<MANUAL>"]
["Algorithm HA Pass","<MANUAL>"]
["MN HA SPI","<MANUAL>"]
["MN AAA SS","<MANUAL>"]
["MN AAA SPI","<MANUAL>"]
["Algorithm AAA Pass","<MANUAL>"]
["MN AAA SPI","<MANUAL>"]
["Reverse Tunnel ","<MANUAL>"]
["Time Delta","<MANUAL>"]
["Home Agent IP","<MANUAL>"]
["Primary HA IP","<MANUAL>"]
["Secondary HA IP","<MANUAL>"]
["Registration Retry Number","<MANUAL>"]
["Retry Interval","<MANUAL>"]
["RFC2002bis MN-HA authenticator calculation","<MANUAL>"]
["Re-registration only if traffic since last RRQ","<MANUAL>"]
["QC optimized dormant handoff","<MANUAL>"]
["Pre-Lifetime-expiry Re-registration Time","<MANUAL>"]
["Initial Registration Retry Interval","<MANUAL>"]
["Header","######ENGINEERING (HIDE)#######################"]
["All SMS on Traffic Channel",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=716|IfSetDisplay=Enabled|IfNotSetDisplay=Disabled"]
["Allow New System Redial",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=366|IfSetDisplay=No|IfNotSetDisplay=Yes"]
["BREW Test Enable",{"$error":"#REF!"},"RDELEM","275A000100E80001","SelectCase","00=Off|01=On"]
["Background Scan Timer",{"$error":"#REF!"},"RDELEM","275E000101840004","Hex2Dec","ByteSwap=True|BytesPerData=4"]
["Re-scan on Release",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=375|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Video Format",{"$error":"#REF!"},"RDELEM","275A0001014F0001","SelectCase","00=MP4|01=H263"]
["Audio Format",{"$error":"#REF!"},"RDELEM","275A000101500001","SelectCase","00=QCELP|01=AMR|02=QCELP|Else=Flex Implementation Error"]
["Send Key Format",{"$error":"#REF!"},"RDELEM","2742000100000000","FeatureId","FeatureId=781|IfSetDisplay=Dialed/Received Calls|IfNotSetDisplay=Dialed Calls"]
["Service Level","<MANUAL>"]
["WAP Connection Type","<MANUAL>"]
["User Agent Header (MMS)",{"$error":"#REF!"},"RDELEM","29BA000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered\""]
["User Agent Header (Browser)","<MANUAL>"]
["Header","Main Menu Itens Other Settings"]
["Electronic Serial Number (ESN)","<MANUAL>"]
["Bluetooth Address (ULMA)","<MANUAL>"]
["3.1   ERI","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=534|IfSetDisplay=ON|IfNotSetDisplay=OFF"]
["List ID","<MANUAL>","RDELEM","296A000100000002","Hex2Dec","BytesPerData=2|IfThen=0"]
["File System Count","<MANUAL>"]
["Header","Security"]
["Phone Lock","<MANUAL>","RDELEM","275A0001002A0001","SelectCase","01=On|00=Off"]
["Header","Lock Application"]
["Phonebook","<MANUAL>","RDELEM","275A0001002E0001","SelectCase","00=Unlocked|01=Locked|02=View Only"]
["Recent Calls","<MANUAL>","RDELEM","275A0001002C0001","SelectCase","00=Unlocked|01=Locked"]
["Messaging","<MANUAL>","RDELEM","275A000100310001","SelectCase","00=Unlocked|01=Locked"]
[" Messages ","<MANUAL>","RDELEM","275A000100310001","SelectCase","00=Unlocked|01=Locked"]
[" Web Access ","<MANUAL>","RDELEM","275A000100000000","MultipleCases","52=00|90=00|Then=Unlocked|Else=Locked"]
["Get It Now","<MANUAL>","RDELEM","275A000100DF0001","SelectCase","00=Unlocked|01=Locked"]
["Mobile Web","<MANUAL>","RDELEM","275A000100000000","MultipleCases","52=00|90=00|Then=Unlocked|Else=Locked"]
["Web Browser","<MANUAL>","RDELEM","275A000100340001","SelectCase","00=Unlocked|01=Locked"]
[" Web Sessions ","<MANUAL>","RDELEM","275A0001005A0001","SelectCase","00=Unlocked|01=Locked"]
[" Multimedia ","<MANUAL>","RDELEM","275A000101130001","SelectCase","00=Unlocked|01=Locked"]
["Media Gallery","<MANUAL>","RDELEM","275A000101130001","SelectCase","00=Unlocked|01=Locked"]
["Settings","<MANUAL>","RDELEM","275A000100000000","MultipleCases","43=00|177=00|211=00|212=00|213=00|214=00|215=00|216=00|217=00|220=00|221=00|Then=Unlocked|Else=Locked"]
["Ring Styles","<MANUAL>","RDELEM","275A000100B10001","SelectCase","00=Unlocked|01=Locked"]
["Connection","<MANUAL>","RDELEM","275A000100D40001","SelectCase","00=Unlocked|01=Locked"]
["Tools","<MANUAL>","RDELEM","275A000100000000","MultipleCases","15=00|47=00|50=00|171=00|254=00|Then=Unlocked|Else=Locked"]
["Calculator","<MANUAL>","RDELEM","275A000100AB0001","SelectCase","00=Unlocked|01=Locked"]
["Datebook","<MANUAL>","RDELEM","275A0001002F0001","SelectCase","00=Unlocked|01=Locked"]
["Shortcuts","<MANUAL>","RDELEM","275A000100320001","SelectCase","00=Unlocked|01=Locked"]
["Voice Records","<MANUAL>","RDELEM","275A0001000F0001","SelectCase","00=Unlocked|01=Locked"]
["Alarm Clock","<MANUAL>","RDELEM","275A000100FE0001","SelectCase","00=Unlocked|01=Locked"]
["Incoming Calls to Phonebook Available","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=502|IfSetDisplay=Yes|IfNotSetDisplay=No"]
["Restrict Outgoing Calls          Allow","<MANUAL>","RDELEM","275A000100370001","SelectCase","00=None|01=All|02=Phonebook"]
["Restrict Incoming Calls          Allow","<MANUAL>","RDELEM","275A000100380001","SelectCase","00=None|01=All|02=Phonebook"]
["Header","Phonebook Setup"]
["Sort By","<MANUAL>","RDELEM","275A000100730001","SelectCase","00=Name|01=Speed Number|02=Voice Name|03=Email"]
["View","<MANUAL>","RDELEM","275A000100860001","SelectCase","00=All Contacts|01=Primary Contacts"]
["Header","Initial Setup"]
["Speaker Phone","<MANUAL>","RDELEM","275A000100AE0001","SelectCase","00=Always On|01=20 sec timeout"]
["Animation","<MANUAL>","RDELEM","275A000100080001","SelectCase","00=Off|01=On"]
["Header","NAM 1 Field and Contents"]
["AMPS Home System ID (SID)","<MANUAL>","RDELEM","2798000100000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["ACCOLC (New Programming Method)","<MANUAL>","RDELEM","27980001000C0001","Hex2Dec","BytesPerData=1|FormatLength=2"]
["Option Byte 2","<MANUAL>","RDELEM","2797000100070001","Hex2Bin"]
["True IMSI Address Number","<MANUAL>","RDELEM","2798000100250001","DisplayBits","DisplayBits=5"]
["True IMSI Status","<MANUAL>","RDELEM","2798000100250001","DisplayBits","DisplayBits=3"]
["True IMSI Prog/Deprog","<MANUAL>","RDELEM","2798000100250001","DisplayBits","DisplayBits=1"]
["True IMSI","<MANUAL>","RDELEM","2798000100280004","CDMA1XTrueIMSI","HexIn2=27980001002C0002"]
["True IMSI MCC","<MANUAL>","RDELEM","2798000100260002","CDMA1XMCC"]
["True IMSI 11 12","<MANUAL>","RDELEM","27980001002E0001","CDMA1XIMSI12and11"]
["CDMA Home System ID (SID 2)","<MANUAL>","RDELEM","27A7000100040002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["CDMA Network ID (NID 2)","<MANUAL>","RDELEM","27A7000100060002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Header","NAM 2 Field and Contents"]
["(NAM 2) AMPS Home System ID (SID)","<MANUAL>","RDELEM","2798000200000002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["(NAM 2) ACCOLC (New Programming Method)","<MANUAL>","RDELEM","27980002000C0001","Hex2Dec","BytesPerData=1|FormatLength=2"]
["(NAM 2) CDMA Home System ID (SID 2)","<MANUAL>","RDELEM","27A7000200040002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["(NAM 2) CDMA Network ID (NID 2)","<MANUAL>","RDELEM","27A7000200060002","Hex2Dec","ByteSwap=True|BytesPerData=2|FormatLength=5"]
["Header","Entry Setup"]
["Primary Setup","<MANUAL>","RDELEM","275A000101020001","SelectCase","00=iTAP English|01=iTAP Espanol|02=TAP Method|FF=TAP Method"]
["Secondary Setup","<MANUAL>","RDELEM","275A000101030001","SelectCase","00=iTAP English|01=iTAP Espanol|02=TAP Method|FF=None"]
["Header","Pre-Loaded Quick Notes",null,null,"CDMA1XQuickNotes","OffsetSEEM10000=TRUE|StartIndex=61"]
["Quick Note 1","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 1"]
["Quick Note 2","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 2"]
["Quick Note 3","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 3"]
["Quick Note 4","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 4"]
["Quick Note 5","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 5"]
["Quick Note 6","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 6"]
["Quick Note 7","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 7"]
["Quick Note 8","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 8"]
["Quick Note 9","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 9"]
["Quick Note 10","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 10"]
["Quick Note 11","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 11"]
["Quick Note 12","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 12"]
["Quick Note 13","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 13"]
["Quick Note 14","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 14"]
["Quick Note 15","<MANUAL>",null,null,"GetAnswer","ANS=Quick Note 15"]
["Header","MMS Settings"]
["Server Name/IP","<MANUAL>","RDELEM","299A0001003E0000","Hex2ASCII","IfDataIsNullDisplay=None Entered"]
["Server Name/IP 2","<MANUAL>","RDELEM","299A0002003C0000","Hex2ASCII","IfDataIsNullDisplay=None Entered"]
["New MM Retrieval","<MANUAL>","RDELEM","275A0001012D0001","SelectCase","00=Automatic Mode|01=Prompt Mode"]
["Retry Number","<MANUAL>","RDELEM","275E000102BC0004","Hex2Dec","ByteSwap=True|BytesPerData=4"]
["UAPROF URL","<MANUAL>","RDELEM","284D000100480000","CDMA1XUAPROFURL"]
["Album Upload Address","<MANUAL>","RDELEM","29A0000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2"]
["Read ACK","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=788|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Delivery ACK","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=787|IfSetDisplay=On|IfNotSetDisplay=Off"]
["Header","Security Information"]
["Security Code","<MANUAL>","RDELEM","2786000100000000","Hex2ASCII","ByteSwap=True|BytesPerData=2"]
["Header","User Activation Information"]
["Allowable Attempts","<MANUAL>","RDELEM","28D5000100200004","SelectCase","FFFFFFFF=Unlimited|Else=Func:Hex2Dec|ByteSwap=True|BytesPerData=4"]
["One Time Sub Lock Status","<MANUAL>","RDELEM","28D3000100060001","CDMA1XOneTimeSubsidyLock","00=Enabled|01=Disabled"]
[" Electronic Serial Number (ESN) ","<MANUAL>","RDELEM","2789000100000008","AsIs"]
[" Factory Flex Switch ","<MANUAL>","RDELEM","2940000100000001","SelectCase","55=Factory(55)|EE=Customer(EE)"]
[" Factory Byte ","<MANUAL>","RDELEM","28D1000100000001","SelectCase","00=Out of Factory(00)|01=In Factory(01)|FF=In Factory(FF)|Else=In Factory(XX)"]
[" Bluetooth Address (ULMA) ","<MANUAL>","RDELEM","01BF000100000006","SelectCase","04=Not Programmed|else=Func:AsIs|ByteSwap=True|BytesPerData=6"]
[" File System Count ","<MANUAL>",null,null,"GetAnswer","ANS=File System Count"]
["Header","BREW Comm Server or BREW IP/URL"]
["BREW Test Enable","<MANUAL>","RDELEM","275A000100E80001","SelectCase","00=Off|01=On"]
["BREW MIN for SID","<MANUAL>","RDELEM","275A000100E90001","SelectCase","00=No|01=Yes"]
["Server Type","<MANUAL>","RDELEM","275A000100EA0001","SelectCase","00=Commercial|01=Test"]
["Header","Network"]
[" Analog Only ","<MANUAL>","RDELEM","275A0001007B0001","SelectCase","00=Off|01=On"]
["Set Mode","<MANUAL>","RDELEM","27980001001A0002","CDMA1XNetworkSetMode"]
["Service Status","<MANUAL>","RDELEM","2760000100C40001","SelectCase","00=Automatic|01=Manual"]
["Header","Engineering Settings"]
["Dynamic Websession","<MANUAL>","RDELEM","2742000100000000","FeatureId","FeatureId=116|IfSetDisplay=On|IfNotSetDisplay=Off"]
["MMS Header Line ID","<MANUAL>","RDELEM","29BE000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["SEEM_MMS_MDN_HEADER","<MANUAL>","RDELEM","29BB000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["SEEM_MMS_BLOG_ADDRESS","<MANUAL>","RDELEM","29A0000100000000","Hex2ASCII","BytesPerData=2|ByteSwap=True|IfDataIsNullDisplay=None Entered"]
["Use MIN for SID","<MANUAL>","RDELEM","275A000100E90001","SelectCase"," 01=MDN|01=MMC|02=MCC-MDN|03=MCC-MIN"]
["SID Encode","<MANUAL>","RDELEM","275A000101280001","SelectCase","00=Off|01=On"]
["Disallow Dormancy","<MANUAL>","RDELEM","275A000101290001","SelectCase","00=Off|01=On"]
{"$rows_empty":57}
["Available Commands","Available Functions"]
["FSAC","A20"]
["RDELEM","AsIs"]
["SBSDY_LCK","BrewBarFiles"]
["VERSION","CDMA1XBrewBarFiles"]
[null,"CDMA1XBrewDnsIp"]
[null,"CDMA1XBrowsers"]
[null,"CDMA1XDataConnectionDNS"]
[null,"CDMA1XIMSI12and11"]
[null,"CDMA1XKeys6XXX"]
[null,"CDMA1XKeysV710"]
[null,"CDMA1XMainMenuOrder"]
[null,"CDMA1XMainMenuOrder6XXX"]
[null,"CDMA1XMainMenuOrderT720"]
[null,"CDMA1XMainMenuOrderV710"]
[null,"CDMA1XMaxSMSCharacters"]
[null,"CDMA1XMCC"]
[null,"CDMA1XMessagingMenuOrder"]
[null,"CDMA1XMessagingMenuOrderV710"]
[null,"CDMA1XMIN"]
[null,"CDMA1XMobileIDNumberType"]
[null,"CDMA1XPhoneLockCode"]
[null,"CDMA1XQuickNotes"]
[null,"CDMA1XSubsidyLock"]
[null,"CDMA1XTrueIMSI"]
[null,"CDMA1XVoiceMailNumber"]
[null,"CDMA1XWebSessions"]
[null,"CDMA1XRingStyles"]
[null,"DecAndHex"]
[null,"DisplayBits"]
[null,"FeatureId"]
[null,"GetAnswer"]
[null,"Hex2ASCII"]
[null,"Hex2Bin"]
[null,"Hex2Dec"]
[null,"Languages"]
[null,"LittleEndianHex2Dec"]
[null,"MultipleCases"]
[null,"SelectCase"]